/dts-v1/;

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "planex,cs-qr10", "ralink,mt7620a-soc";
	model = "YUKAI Engineering BOCCO";

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio1 7 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		s1 {
			gpio-export,name = "rec";
			gpios = <&gpio1 8 GPIO_ACTIVE_HIGH>;
		};
		s2 {
			gpio-export,name = "play";
			gpios = <&gpio1 9 GPIO_ACTIVE_HIGH>;
		};
	};

	sound {
		compatible = "simple-audio-card";
		simple-audio-card,name = "Audio-I2S";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&dailink0_master>;
		simple-audio-card,frame-master = <&dailink0_master>;
		simple-audio-card,widgets =
			"Headphone", "Headphones";
		simple-audio-card,routing =
			"Headphones", "HP_L",
			"Headphones", "HP_R";
		simple-audio-card,mclk-fs = <256>;

		simple-audio-card,cpu {
			sound-dai = <&i2s>;
		};

		dailink0_master: simple-audio-card,codec {
			sound-dai = <&codec>;
		};
	};
};

&gpio0 {
	status = "okay";
};

&gpio1 {
	status = "okay";
};

&gpio2 {
	status = "okay";
};

&gpio3 {
	status = "okay";
};

&i2c {
	status = "okay";

	codec: wm8960@1a {
		#sound-dai-cells = <0>;
		compatible = "wlf,wm8960";
		reg = <0x1a>;

		wlf,shared-lrclk;
	};
};

&i2s {
	#sound-dai-cells = <0>;
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&pcm_i2s_pins>;
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&pcm {
	status = "okay";
};

&gdma {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "spi refclk", "rgmii1";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	pinctrl-names = "default";
	pinctrl-0 = <&ephy_pins>;
	mtd-mac-address = <&factory 0x4>;
	mediatek,portmap = "llllw";
};

&gsw {
	ralink,port4 = "ephy";
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};
