--- a/Documentation/devicetree/bindings/pinctrl/atmel,at91-pio4-pinctrl.txt
+++ b/Documentation/devicetree/bindings/pinctrl/atmel,at91-pio4-pinctrl.txt
@@ -35,7 +35,12 @@ right representation of the pin.
 Optional properties:
 - GENERIC_PINCONFIG: generic pinconfig options to use, bias-disable,
 bias-pull-down, bias-pull-up, drive-open-drain, input-schmitt-enable,
-input-debounce, output-low, output-high.
+input-debounce, output-low, output-high, drive-strength.
+
+Concerning the drive-strength property, the values accepted are
+ATMEL_PIO_DRVSTR_LO, ATMEL_PIO_DRVSTR_ME, ATMEL_PIO_DRVSTR_HI. The current
+depends on VDDIOP. You can find the details in the DC Characteristics table
+from the datasheet.
 
 Example:
 
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -49,6 +49,7 @@ dtb-$(CONFIG_SOC_AT91SAM9) += \
 	wb45n.dtb
 dtb-$(CONFIG_SOC_SAM_V7) += \
 	at91-kizbox2.dtb \
+	at91-sama5d27_som1_ek.dtb \
 	at91-sama5d2_xplained.dtb \
 	at91-sama5d3_xplained.dtb \
 	sama5d31ek.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/at91-sama5d27_som1.dtsi
@@ -0,0 +1,175 @@
+/*
+ * at91-sama5d27_som1.dtsi - Device Tree file for SAMA5D27 SoM1 board
+ *
+ *  Copyright (c) 2017, Microchip Technology Inc.
+ *                2017 Cristian Birsan <cristian.birsan@microchip.com>
+ *                2017 Claudiu Beznea <claudiu.beznea@microchip.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+#include "sama5d2.dtsi"
+#include "sama5d2-pinfunc.h"
+
+/ {
+	model = "Atmel SAMA5D27 SoM1";
+	compatible = "atmel,sama5d27-som1", "atmel,sama5d27", "atmel,sama5d2", "atmel,sama5";
+
+	clocks {
+		slow_xtal {
+			clock-frequency = <32768>;
+		};
+
+		main_xtal {
+			clock-frequency = <24000000>;
+		};
+	};
+
+	ahb {
+		apb {
+			qspi1: spi@f0024000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_qspi1_default>;
+
+				flash@0 {
+					#address-cells = <1>;
+					#size-cells = <1>;
+					compatible = "jedec,spi-nor";
+					reg = <0>;
+					spi-max-frequency = <80000000>;
+					m25p,fast-read;
+
+					at91bootstrap@00000000 {
+						label = "at91bootstrap";
+						reg = <0x00000000 0x00010000>;
+					};
+
+					bootloader@00010000 {
+						label = "bootloader";
+						reg = <0x00010000 0x000a0000>;
+					};
+
+					bootloaderenv@000b0000 {
+						label = "bootloader env";
+						reg = <0x000b0000 0x00010000>;
+					};
+
+					dtb@000c0000 {
+						label = "device tree";
+						reg = <0x000c0000 0x0020000>;
+					};
+
+					kernel@000e0000 {
+						label = "kernel";
+						reg = <0x000e0000 0x0400000>;
+					};
+				};
+			};
+
+			macb0: ethernet@f8008000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_macb0_default>;
+				phy-mode = "rmii";
+
+				ethernet-phy@0 {
+					reg = <0x0>;
+					interrupt-parent = <&pioA>;
+					interrupts = <PIN_PD31 IRQ_TYPE_LEVEL_LOW>;
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_macb0_phy_irq>;
+				};
+			};
+
+			i2c0: i2c@f8028000 {
+				dmas = <0>, <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_i2c0_default>;
+				status = "okay";
+
+				at24@50 {
+					compatible = "24c02";
+					reg = <0x50>;
+					pagesize = <8>;
+				};
+			};
+
+			pinctrl@fc038000 {
+				pinctrl_i2c0_default: i2c0_default {
+					pinmux = <PIN_PD21__TWD0>,
+						 <PIN_PD22__TWCK0>;
+					bias-disable;
+				};
+
+				pinctrl_qspi1_default: qspi1_default {
+					sck_cs {
+						pinmux = <PIN_PB5__QSPI1_SCK>,
+							 <PIN_PB6__QSPI1_CS>;
+						bias-disable;
+					};
+
+					data {
+						pinmux = <PIN_PB7__QSPI1_IO0>,
+							 <PIN_PB8__QSPI1_IO1>,
+							 <PIN_PB9__QSPI1_IO2>,
+							 <PIN_PB10__QSPI1_IO3>;
+						bias-pull-up;
+					};
+				};
+
+				pinctrl_macb0_default: macb0_default {
+					pinmux = <PIN_PD9__GTXCK>,
+						 <PIN_PD10__GTXEN>,
+						 <PIN_PD11__GRXDV>,
+						 <PIN_PD12__GRXER>,
+						 <PIN_PD13__GRX0>,
+						 <PIN_PD14__GRX1>,
+						 <PIN_PD15__GTX0>,
+						 <PIN_PD16__GTX1>,
+						 <PIN_PD17__GMDC>,
+						 <PIN_PD18__GMDIO>;
+					bias-disable;
+				};
+
+				pinctrl_macb0_phy_irq: macb0_phy_irq {
+					pinmux = <PIN_PD31__GPIO>;
+					bias-disable;
+				};
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/at91-sama5d27_som1_ek.dts
@@ -0,0 +1,53 @@
+/*
+ * at91-sama5d27_som1_ek.dts - Device Tree file for SAMA5D27-SOM1-EK board
+ *
+ *  Copyright (c) 2017, Microchip Technology Inc.
+ *                2016 Nicolas Ferre <nicolas.ferre@atmel.com>
+ *                2017 Cristian Birsan <cristian.birsan@microchip.com>
+ *                2017 Claudiu Beznea <claudiu.beznea@microchip.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+/dts-v1/;
+#include "at91-sama5d27_som1_ek_common.dtsi"
+
+/ {
+	model = "Atmel SAMA5D27 SOM1 EK";
+	compatible = "atmel,sama5d27-som1-ek", "atmel,sama5d27-som1", "atmel,sama5d27", "atmel,sama5d2", "atmel,sama5";
+};
--- /dev/null
+++ b/arch/arm/boot/dts/at91-sama5d27_som1_ek_common.dtsi
@@ -0,0 +1,619 @@
+/*
+ * at91-sama5d27_som1_ek_common.dtsi - Device Tree file for SAMA5D27-SOM1-EK board
+ *
+ *  Copyright (c) 2017, Microchip Technology Inc.
+ *                2016 Nicolas Ferre <nicolas.ferre@atmel.com>
+ *                2017 Cristian Birsan <cristian.birsan@microchip.com>
+ *                2017 Claudiu Beznea <claudiu.beznea@microchip.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+#include "at91-sama5d27_som1.dtsi"
+#include <dt-bindings/mfd/atmel-flexcom.h>
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/pinctrl/at91.h>
+
+/ {
+	model = "Atmel SAMA5D27 SOM1 EK";
+	compatible = "atmel,sama5d27-som1-ek", "atmel,sama5d27-som1", "atmel,sama5d27", "atmel,sama5d2", "atmel,sama5";
+
+	aliases {
+		serial0 = &uart1;	/* DBGU */
+		serial1 = &uart4;	/* mikro BUS 1 */
+		serial2 = &uart2;	/* mikro BUS 2 */
+		i2c1	= &i2c1;
+		i2c2	= &i2c2;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	ahb {
+		usb0: gadget@00300000 {
+			atmel,vbus-gpio = <&pioA PIN_PD20 GPIO_ACTIVE_HIGH>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&pinctrl_usba_vbus>;
+			status = "okay";
+		};
+
+		usb1: ohci@00400000 {
+			num-ports = <3>;
+			atmel,vbus-gpio = <0 /* &pioA PIN_PD20 GPIO_ACTIVE_HIGH */
+					   &pioA PIN_PA27 GPIO_ACTIVE_HIGH
+					   0
+					  >;
+			pinctrl-names = "default";
+			pinctrl-0 = <&pinctrl_usb_default>;
+			status = "okay";
+		};
+
+		usb2: ehci@00500000 {
+			status = "okay";
+		};
+
+		sdmmc0: sdio-host@a0000000 {
+			bus-width = <8>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&pinctrl_sdmmc0_default>;
+			status = "okay";
+		};
+
+		sdmmc1: sdio-host@b0000000 {
+			bus-width = <4>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&pinctrl_sdmmc1_default>;
+			status = "okay";
+		};
+
+		apb {
+			hlcdc: hlcdc@f0000000 {
+				status = "disabled";
+
+				hlcdc-display-controller {
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_lcd_base &pinctrl_lcd_rgb>;
+				};
+
+				hlcdc_pwm: hlcdc-pwm {
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_lcd_pwm>;
+				};
+			};
+
+			pmc: pmc@f0014000 {
+				pmc_fast_restart {
+					compatible = "atmel,sama5d2-pmc-fast-startup";
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					atmel,wakeup-rtc-timer;
+
+					wkpin: input@0 {
+						reg = <0>;
+					};
+
+					gmac_wol: input@10 {
+						reg = <10>;
+						atmel,wakeup-active-high;
+					};
+				};
+			};
+
+			isc: isc@f0008000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_isc_base &pinctrl_isc_data_8bit &pinctrl_isc_data_9_10 &pinctrl_isc_data_11_12>;
+				status = "okay";
+			};
+
+			qspi1: spi@f0024000 {
+				status = "okay";
+			};
+
+			spi0: spi@f8000000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_spi0_default>;
+				status = "okay";
+			};
+
+			macb0: ethernet@f8008000 {
+				status = "okay";
+			};
+
+			uart1: serial@f8020000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_uart1_default>;
+				atmel,use-dma-rx;
+				atmel,use-dma-tx;
+				status = "okay";
+			};
+
+			uart2: serial@f8024000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_mikrobus2_uart>;
+				atmel,use-dma-rx;
+				atmel,use-dma-tx;
+				status = "okay";
+			};
+
+			pwm0: pwm@f802c000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_mikrobus1_pwm &pinctrl_mikrobus2_pwm>;
+				status = "disabled"; /* Conflict with leds. */
+			};
+
+			flx1: flexcom@f8038000 {
+				atmel,flexcom-mode = <ATMEL_FLEXCOM_MODE_TWI>;
+				status = "okay";
+
+				i2c2: i2c@600 {
+					compatible = "atmel,sama5d2-i2c";
+					reg = <0x600 0x200>;
+					interrupts = <20 IRQ_TYPE_LEVEL_HIGH 7>;
+					dmas = <0>, <0>;
+					dma-names = "tx", "rx";
+					#address-cells = <1>;
+					#size-cells = <0>;
+					clocks = <&flx1_clk>;
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_mikrobus_i2c>;
+					atmel,fifo-size = <16>;
+					status = "okay";
+				};
+			};
+
+			shdwc@f8048010 {
+				atmel,shdwc-debouncer = <976>;
+				atmel,wakeup-rtc-timer;
+
+				input@0 {
+					reg = <0>;
+					atmel,wakeup-type = "low";
+				};
+			};
+
+			watchdog@f8048040 {
+				status = "okay";
+			};
+
+			uart3: serial@fc008000 {
+				atmel,use-dma-rx;
+				atmel,use-dma-tx;
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_uart3_default>;
+				status = "disabled"; /* Conflict with isc. */
+			};
+
+			uart4: serial@fc00c000 {
+				atmel,use-dma-rx;
+				atmel,use-dma-tx;
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_mikrobus1_uart>;
+				status = "okay";
+			};
+
+			flx3: flexcom@fc014000 {
+				atmel,flexcom-mode = <ATMEL_FLEXCOM_MODE_SPI>;
+				status = "disabled";
+
+				uart7: serial@200 {
+					compatible = "atmel,at91sam9260-usart";
+					reg = <0x200 0x200>;
+					interrupts = <22 IRQ_TYPE_LEVEL_HIGH 7>;
+					clocks = <&flx3_clk>;
+					clock-names = "usart";
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_flx3_default>;
+					atmel,fifo-size = <32>;
+					status = "disabled"; /* Conflict with isc. */
+				};
+
+				spi2: spi@400 {
+					compatible = "atmel,at91rm9200-spi";
+					reg = <0x400 0x200>;
+					interrupts = <22 IRQ_TYPE_LEVEL_HIGH 7>;
+					clocks = <&flx3_clk>;
+					clock-names = "spi_clk";
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_flx3_default>;
+					atmel,fifo-size = <16>;
+					status = "disabled"; /* Conflict with isc. */
+				};
+			};
+
+			flx4: flexcom@fc018000 {
+				atmel,flexcom-mode = <ATMEL_FLEXCOM_MODE_SPI>;
+				status = "okay";
+
+				uart6: serial@200 {
+					compatible = "atmel,at91sam9260-usart";
+					reg = <0x200 0x200>;
+					interrupts = <23 IRQ_TYPE_LEVEL_HIGH 7>;
+					clocks = <&flx4_clk>;
+					clock-names = "usart";
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_flx4_default>;
+					atmel,fifo-size = <32>;
+					status = "disabled"; /* Conflict with spi3 and i2c3. */
+				};
+
+				spi3: spi@400 {
+					compatible = "atmel,at91rm9200-spi";
+					reg = <0x400 0x200>;
+					interrupts = <23 IRQ_TYPE_LEVEL_HIGH 7>;
+					clocks = <&flx4_clk>;
+					clock-names = "spi_clk";
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_mikrobus_spi &pinctrl_mikrobus1_spi_cs &pinctrl_mikrobus2_spi_cs>;
+					atmel,fifo-size = <16>;
+					status = "okay";
+				};
+
+				i2c3: i2c@600 {
+					compatible = "atmel,sama5d2-i2c";
+					reg = <0x600 0x200>;
+					interrupts = <23 IRQ_TYPE_LEVEL_HIGH 7>;
+					dmas = <0>, <0>;
+					dma-names = "tx", "rx";
+					#address-cells = <1>;
+					#size-cells = <0>;
+					clocks = <&flx4_clk>;
+					pinctrl-names = "default";
+					pinctrl-0 = <&pinctrl_flx4_default>;
+					atmel,fifo-size = <16>;
+					status = "disabled"; /* Conflict with uart6 and spi3. */
+				};
+			};
+
+			i2c1: i2c@fc028000 {
+				dmas = <0>, <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_i2c1_default>;
+				status = "okay";
+			};
+
+			pinctrl@fc038000 {
+
+				pinctrl_lcd_base: pinctrl_lcd_base {
+					pinmux = <PIN_PC5__LCDVSYNC>,
+						 <PIN_PC6__LCDHSYNC>,
+						 <PIN_PC8__LCDDEN>,
+						 <PIN_PC7__LCDPCK>;
+					bias-disable;
+					drive-strength = <ATMEL_PIO_DRVSTR_ME>;
+				};
+
+				pinctrl_lcd_rgb: pinctrl_lcd_rgb {
+					pinmux = <PIN_PB11__LCDDAT0>,
+						 <PIN_PB12__LCDDAT1>,
+						 <PIN_PB13__LCDDAT2>,
+						 <PIN_PB14__LCDDAT3>,
+						 <PIN_PB15__LCDDAT4>,
+						 <PIN_PB16__LCDDAT5>,
+						 <PIN_PB17__LCDDAT6>,
+						 <PIN_PB18__LCDDAT7>,
+						 <PIN_PB19__LCDDAT8>,
+						 <PIN_PB20__LCDDAT9>,
+						 <PIN_PB21__LCDDAT10>,
+						 <PIN_PB22__LCDDAT11>,
+						 <PIN_PB23__LCDDAT12>,
+						 <PIN_PB24__LCDDAT13>,
+						 <PIN_PB25__LCDDAT14>,
+						 <PIN_PB26__LCDDAT15>,
+						 <PIN_PB27__LCDDAT16>,
+						 <PIN_PB28__LCDDAT17>,
+						 <PIN_PB29__LCDDAT18>,
+						 <PIN_PB30__LCDDAT19>,
+						 <PIN_PB31__LCDDAT20>,
+						 <PIN_PC0__LCDDAT21>,
+						 <PIN_PC1__LCDDAT22>,
+						 <PIN_PC2__LCDDAT23>;
+					bias-disable;
+				};
+
+				pinctrl_lcd_pwm: pinctrl_lcd_pwm {
+					pinmux = <PIN_PC3__LCDPWM>;
+					bias-disable;
+				};
+
+				pinctrl_can1_default: can1_default {
+					pinmux = <PIN_PC26__CANTX1>,
+						 <PIN_PC27__CANRX1>;
+					bias-disable;
+				};
+
+				pinctrl_flx3_default: flx3_default {
+					pinmux = <PIN_PC20__FLEXCOM3_IO0>,
+						 <PIN_PC19__FLEXCOM3_IO1>,
+						 <PIN_PC18__FLEXCOM3_IO2>,
+						 <PIN_PC21__FLEXCOM3_IO3>,
+						 <PIN_PC22__FLEXCOM3_IO4>;
+					bias-disable;
+				};
+
+				pinctrl_i2c1_default: i2c1_default {
+					pinmux = <PIN_PD4__TWD1>,
+						 <PIN_PD5__TWCK1>;
+					bias-disable;
+				};
+
+				pinctrl_isc_base: isc_base {
+					pinmux = <PIN_PC21__ISC_PCK>,
+						 <PIN_PC22__ISC_VSYNC>,
+						 <PIN_PC23__ISC_HSYNC>,
+						 <PIN_PC24__ISC_MCK>;
+					bias-disable;
+				};
+
+				pinctrl_isc_data_8bit: isc_data_8bit {
+					pinmux = <PIN_PC20__ISC_D11>,
+						 <PIN_PC19__ISC_D10>,
+						 <PIN_PC18__ISC_D9>,
+						 <PIN_PC17__ISC_D8>,
+						 <PIN_PC16__ISC_D7>,
+						 <PIN_PC15__ISC_D6>,
+						 <PIN_PC14__ISC_D5>,
+						 <PIN_PC13__ISC_D4>;
+					bias-disable;
+				};
+
+				pinctrl_isc_data_9_10: isc_data_9_10 {
+					pinmux = <PIN_PC12__ISC_D3>,
+						 <PIN_PC11__ISC_D2>;
+					bias-disable;
+				};
+
+				pinctrl_isc_data_11_12: isc_data_11_12 {
+					pinmux = <PIN_PC10__ISC_D1>,
+						 <PIN_PC9__ISC_D0>;
+					bias-disable;
+				};
+
+				pinctrl_key_gpio_default: key_gpio_default {
+					pinmux = <PIN_PA29__GPIO>;
+					bias-pull-up;
+				};
+
+				pinctrl_led_gpio_default: led_gpio_default {
+					pinmux = <PIN_PA10__GPIO>,
+						 <PIN_PB1__GPIO>,
+						 <PIN_PA31__GPIO>;
+					bias-pull-up;
+				};
+
+				pinctrl_sdmmc0_default: sdmmc0_default {
+					cmd_data {
+						pinmux = <PIN_PA1__SDMMC0_CMD>,
+							 <PIN_PA2__SDMMC0_DAT0>,
+							 <PIN_PA3__SDMMC0_DAT1>,
+							 <PIN_PA4__SDMMC0_DAT2>,
+							 <PIN_PA5__SDMMC0_DAT3>,
+							 <PIN_PA6__SDMMC0_DAT4>,
+							 <PIN_PA7__SDMMC0_DAT5>,
+							 <PIN_PA8__SDMMC0_DAT6>,
+							 <PIN_PA9__SDMMC0_DAT7>;
+						bias-disable;
+					};
+
+					ck_cd_vddsel {
+						pinmux = <PIN_PA0__SDMMC0_CK>,
+							 <PIN_PA11__SDMMC0_VDDSEL>,
+							 <PIN_PA13__SDMMC0_CD>;
+						bias-disable;
+					};
+				};
+
+				pinctrl_sdmmc1_default: sdmmc1_default {
+					cmd_data {
+						pinmux = <PIN_PA28__SDMMC1_CMD>,
+							 <PIN_PA18__SDMMC1_DAT0>,
+							 <PIN_PA19__SDMMC1_DAT1>,
+							 <PIN_PA20__SDMMC1_DAT2>,
+							 <PIN_PA21__SDMMC1_DAT3>;
+						bias-disable;
+					};
+
+					conf-ck_cd {
+						pinmux = <PIN_PA22__SDMMC1_CK>,
+							 <PIN_PA30__SDMMC1_CD>;
+						bias-disable;
+					};
+				};
+
+				pinctrl_spi0_default: spi0_default {
+					pinmux = <PIN_PA14__SPI0_SPCK>,
+						 <PIN_PA15__SPI0_MOSI>,
+						 <PIN_PA16__SPI0_MISO>,
+						 <PIN_PA17__SPI0_NPCS0>;
+					bias-disable;
+				};
+
+				pinctrl_uart1_default: uart1_default {
+					pinmux = <PIN_PD2__URXD1>,
+						 <PIN_PD3__UTXD1>;
+					bias-disable;
+				};
+
+				pinctrl_uart3_default: uart3_default {
+					pinmux = <PIN_PC12__URXD3>,
+						 <PIN_PC13__UTXD3>;
+					bias-disable;
+				};
+
+				pinctrl_usb_default: usb_default {
+					pinmux = <PIN_PA27__GPIO>,
+						 <PIN_PD19__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_usba_vbus: usba_vbus {
+					pinmux = <PIN_PD20__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus1_an: mikrobus1_an {
+					pinmux = <PIN_PD25__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus2_an: mikrobus2_an {
+					pinmux = <PIN_PD26__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus1_rst: mikrobus1_rst {
+					pinmux = <PIN_PB2__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus2_rst: mikrobus2_rst {
+					pinmux = <PIN_PA26__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus1_spi_cs: mikrobus1_spi_cs {
+					pinmux = <PIN_PD0__FLEXCOM4_IO4>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus2_spi_cs: mikrobus2_spi_cs {
+					pinmux = <PIN_PC31__FLEXCOM4_IO3>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus_spi: mikrobus_spi {
+					pinmux = <PIN_PC28__FLEXCOM4_IO0>,
+						 <PIN_PC29__FLEXCOM4_IO1>,
+						 <PIN_PC30__FLEXCOM4_IO2>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus1_pwm: mikrobus1_pwm {
+					pinmux = <PIN_PB1__PWML1>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus2_pwm: mikrobus2_pwm {
+					pinmux = <PIN_PA31__PWML0>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus1_int: mikrobus1_int {
+					pinmux = <PIN_PB0__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus2_int: mikrobus2_int {
+					pinmux = <PIN_PA25__GPIO>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus1_uart: mikrobus1_uart {
+					pinmux = <PIN_PB3__URXD4>,
+						 <PIN_PB4__UTXD4>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus2_uart: mikrobus2_uart {
+					pinmux = <PIN_PD23__URXD2>,
+						 <PIN_PD24__UTXD2>;
+					bias-disable;
+				};
+
+				pinctrl_mikrobus_i2c: mikrobus1_i2c {
+					pinmux = <PIN_PA24__FLEXCOM1_IO0>,
+						 <PIN_PA23__FLEXCOM1_IO1>;
+					bias-disable;
+				};
+
+				pinctrl_flx4_default: flx4_uart_default {
+					pinmux = <PIN_PC28__FLEXCOM4_IO0>,
+						 <PIN_PC29__FLEXCOM4_IO1>,
+						 <PIN_PC30__FLEXCOM4_IO2>,
+						 <PIN_PC31__FLEXCOM4_IO3>,
+						 <PIN_PD0__FLEXCOM4_IO4>;
+					bias-disable;
+				};
+			};
+
+			can1: can@fc050000 {
+				pinctrl-names = "default";
+				pinctrl-0 = <&pinctrl_can1_default>;
+				status = "okay";
+			};
+		};
+	};
+
+	gpio_keys {
+		compatible = "gpio-keys";
+
+		pinctrl-names = "default";
+		pinctrl-0 = <&pinctrl_key_gpio_default>;
+
+		pb4 {
+			label = "USER";
+			gpios = <&pioA PIN_PA29 GPIO_ACTIVE_LOW>;
+			linux,code = <0x104>;
+			wakeup-source;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&pinctrl_led_gpio_default>;
+		status = "okay"; /* Conflict with pwm0. */
+
+		red {
+			label = "red";
+			gpios = <&pioA PIN_PA10 GPIO_ACTIVE_HIGH>;
+		};
+
+		green {
+			label = "green";
+			gpios = <&pioA PIN_PB1 GPIO_ACTIVE_HIGH>;
+		};
+
+		blue {
+			label = "blue";
+			gpios = <&pioA PIN_PA31 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "heartbeat";
+		};
+	};
+};
--- a/include/dt-bindings/pinctrl/at91.h
+++ b/include/dt-bindings/pinctrl/at91.h
@@ -37,4 +37,8 @@
 #define AT91_PERIPH_C		3
 #define AT91_PERIPH_D		4
 
+#define ATMEL_PIO_DRVSTR_LO	1
+#define ATMEL_PIO_DRVSTR_ME	2
+#define ATMEL_PIO_DRVSTR_HI	3
+
 #endif /* __DT_BINDINGS_AT91_PINCTRL_H__ */
