#!/bin/sh
#
# Copyright (C) 2018 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
ubnt,nanostation-ac)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "3"
	;;
esac

board_config_flush

exit 0
