From e8ede0f62b39a3d3b06ae3dc04a74680a1f0a64b Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Fri, 21 Apr 2017 22:19:00 +0200
Subject: [PATCH 30/31] usb: host: fotg2: add Gemini-specific handling

The Cortina Systems Gemini has bolted on a PHY inside the
silicon that can be handled by six bits in a MISC register in
the system controller.

If we are running on Gemini, look up a syscon regmap through
a phandle and enable VBUS and optionally the Mini-B connector.

If the device is flagged as "wakeup-source" using the standard
DT bindings, we also enable this in the global controller for
respective port.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 drivers/usb/host/Kconfig       |  1 +
 drivers/usb/host/fotg210-hcd.c | 76 ++++++++++++++++++++++++++++++++++++++++++
 2 files changed, 77 insertions(+)

--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -375,6 +375,7 @@ config USB_ISP1362_HCD
 config USB_FOTG210_HCD
 	tristate "FOTG210 HCD support"
 	depends on USB && HAS_DMA && HAS_IOMEM
+	select MFD_SYSCON
 	---help---
 	  Faraday FOTG210 is an OTG controller which can be configured as
 	  an USB2.0 host. It is designed to meet USB2.0 EHCI specification
--- a/drivers/usb/host/fotg210-hcd.c
+++ b/drivers/usb/host/fotg210-hcd.c
@@ -46,6 +46,10 @@
 #include <linux/platform_device.h>
 #include <linux/io.h>
 #include <linux/clk.h>
+#include <linux/bitops.h>
+/* For Cortina Gemini */
+#include <linux/mfd/syscon.h>
+#include <linux/regmap.h>
 
 #include <asm/byteorder.h>
 #include <asm/irq.h>
@@ -5583,6 +5587,72 @@ static void fotg210_init(struct fotg210_
 	iowrite32(value, &fotg210->regs->otgcsr);
 }
 
+/*
+ * Gemini-specific initialization function, only executed on the
+ * Gemini SoC using the global misc control register.
+ */
+#define GEMINI_GLOBAL_MISC_CTRL		0x30
+#define GEMINI_MISC_USB0_WAKEUP		BIT(14)
+#define GEMINI_MISC_USB1_WAKEUP		BIT(15)
+#define GEMINI_MISC_USB0_VBUS_ON	BIT(22)
+#define GEMINI_MISC_USB1_VBUS_ON	BIT(23)
+#define GEMINI_MISC_USB0_MINI_B		BIT(29)
+#define GEMINI_MISC_USB1_MINI_B		BIT(30)
+
+static int fotg210_gemini_init(struct device *dev, struct usb_hcd *hcd)
+{
+	struct device_node *np = dev->of_node;
+	struct regmap *map;
+	bool mini_b;
+	bool wakeup;
+	u32 mask, val;
+	int ret;
+
+	map = syscon_regmap_lookup_by_phandle(np, "syscon");
+	if (IS_ERR(map)) {
+		dev_err(dev, "no syscon\n");
+		return PTR_ERR(map);
+	}
+	mini_b = of_property_read_bool(np, "cortina,gemini-mini-b");
+	wakeup = of_property_read_bool(np, "wakeup-source");
+
+	/*
+	 * Figure out if this is USB0 or USB1 by simply checking the
+	 * physical base address.
+	 */
+	mask = 0;
+	if (hcd->rsrc_start == 0x69000000) {
+		val = GEMINI_MISC_USB1_VBUS_ON;
+		if (mini_b)
+			val |= GEMINI_MISC_USB1_MINI_B;
+		else
+			mask |= GEMINI_MISC_USB1_MINI_B;
+		if (wakeup)
+			val |= GEMINI_MISC_USB1_WAKEUP;
+		else
+			mask |= GEMINI_MISC_USB1_WAKEUP;
+	} else {
+		val = GEMINI_MISC_USB0_VBUS_ON;
+		if (mini_b)
+			val |= GEMINI_MISC_USB0_MINI_B;
+		else
+			mask |= GEMINI_MISC_USB0_MINI_B;
+		if (wakeup)
+			val |= GEMINI_MISC_USB0_WAKEUP;
+		else
+			mask |= GEMINI_MISC_USB0_WAKEUP;
+	}
+
+	ret = regmap_update_bits(map, GEMINI_GLOBAL_MISC_CTRL, mask, val);
+	if (ret) {
+		dev_err(dev, "failed to initialize Gemini PHY\n");
+		return ret;
+	}
+
+	dev_info(dev, "initialized Gemini PHY\n");
+	return 0;
+}
+
 /**
  * fotg210_hcd_probe - initialize faraday FOTG210 HCDs
  *
@@ -5662,6 +5732,12 @@ static int fotg210_hcd_probe(struct plat
 
 	fotg210_init(fotg210);
 
+	if (of_device_is_compatible(dev->of_node, "cortina,gemini-usb")) {
+		retval = fotg210_gemini_init(dev, hcd);
+		if (retval)
+			goto failed_dis_clk;
+	}
+
 	retval = usb_add_hcd(hcd, irq, IRQF_SHARED);
 	if (retval) {
 		dev_err(dev, "failed to add hcd with err %d\n", retval);
