From 42611c6d9f12d16ce4247d76b16218e54ef5b949 Mon Sep 17 00:00:00 2001
From: RogerCC Lin <rogercc.lin@mediatek.com>
Date: Thu, 30 Nov 2017 22:10:43 +0800
Subject: [PATCH 165/224] mtd: nand: mtk: update DT bindings

Add MT7622 NAND Flash Controller dt bindings documentation.

Signed-off-by: RogerCC Lin <rogercc.lin@mediatek.com>
Reviewed-by: Matthias Brugger <matthias.bgg@gmail.com>
Signed-off-by: Boris Brezillon <boris.brezillon@free-electrons.com>
---
 Documentation/devicetree/bindings/mtd/mtk-nand.txt | 11 ++++++++---
 1 file changed, 8 insertions(+), 3 deletions(-)

--- a/Documentation/devicetree/bindings/mtd/mtk-nand.txt
+++ b/Documentation/devicetree/bindings/mtd/mtk-nand.txt
@@ -12,8 +12,10 @@ tree nodes.
 
 The first part of NFC is NAND Controller Interface (NFI) HW.
 Required NFI properties:
-- compatible:			Should be one of "mediatek,mt2701-nfc",
-				"mediatek,mt2712-nfc".
+- compatible:			Should be one of
+				"mediatek,mt2701-nfc",
+				"mediatek,mt2712-nfc",
+				"mediatek,mt7622-nfc".
 - reg:				Base physical address and size of NFI.
 - interrupts:			Interrupts of NFI.
 - clocks:			NFI required clocks.
@@ -142,7 +144,10 @@ Example:
 ==============
 
 Required BCH properties:
-- compatible:	Should be one of "mediatek,mt2701-ecc", "mediatek,mt2712-ecc".
+- compatible:	Should be one of
+		"mediatek,mt2701-ecc",
+		"mediatek,mt2712-ecc",
+		"mediatek,mt7622-ecc".
 - reg:		Base physical address and size of ECC.
 - interrupts:	Interrupts of ECC.
 - clocks:	ECC required clocks.
