From 004eb24e939b5b31f828333f37fb5cb2a877d6f2 Mon Sep 17 00:00:00 2001
From: Kristian Evensen <kristian.evensen@gmail.com>
Date: Sun, 17 Jun 2018 14:41:47 +0200
Subject: [PATCH] arm: dts: Add Unielec U7623 DTS

---
 arch/arm/boot/dts/Makefile                         |   1 +
 .../dts/mt7623a-unielec-u7623-02-emmc-512M.dts     |  18 +
 .../boot/dts/mt7623a-unielec-u7623-02-emmc.dtsi    | 366 +++++++++++++++++++++
 3 files changed, 385 insertions(+)
 create mode 100644 arch/arm/boot/dts/mt7623a-unielec-u7623-02-emmc-512M.dts
 create mode 100644 arch/arm/boot/dts/mt7623a-unielec-u7623-02-emmc.dtsi

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -1062,6 +1062,7 @@ dtb-$(CONFIG_ARCH_MEDIATEK) += \
 	mt6589-aquaris5.dtb \
 	mt6592-evb.dtb \
 	mt7623a-rfb-emmc.dtb \
+	mt7623a-unielec-u7623-02-emmc-512M.dtb \
 	mt7623n-rfb-nand.dtb \
 	mt7623n-bananapi-bpi-r2.dtb \
 	mt8127-moose.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/mt7623a-unielec-u7623-02-emmc-512M.dts
@@ -0,0 +1,18 @@
+/*
+ * Copyright 2018 Kristian Evensen <kristian.evensen@gmail.com>
+ *
+ * SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+ */
+
+/dts-v1/;
+#include "mt7623a-unielec-u7623-02-emmc.dtsi"
+
+/ {
+	model = "UniElec U7623-02 eMMC (512M RAM)";
+	compatible = "unielec,u7623-02-emmc-512m", "unielec,u7623-02-emmc", "mediatek,mt7623";
+
+	memory@80000000 {
+		device_type = "memory";
+		reg = <0 0x80000000 0 0x20000000>;
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/mt7623a-unielec-u7623-02-emmc.dtsi
@@ -0,0 +1,366 @@
+/*
+ * Copyright 2018 Kristian Evensen <kristian.evensen@gmail.com>
+ *
+ * SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+ */
+
+#include <dt-bindings/input/input.h>
+#include "mt7623.dtsi"
+#include "mt6323.dtsi"
+
+/ {
+	compatible = "unielec,u7623-02-emmc", "mediatek,mt7623";
+
+	aliases {
+		serial2 = &uart2;
+	};
+
+	chosen {
+		bootargs = "root=/dev/mmcblk0p2 rootfstype=squashfs,f2fs";
+		stdout-path = "serial2:115200n8";
+	};
+
+	cpus {
+		cpu@0 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+
+		cpu@1 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+
+		cpu@2 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+
+		cpu@3 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+	};
+
+	reg_1p8v: regulator-1p8v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-1.8V";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	reg_3p3v: regulator-3p3v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-3.3V";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	reg_5v: regulator-5v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-5V";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&key_pins_a>;
+
+		factory {
+			label = "factory";
+			linux,code = <KEY_RESTART>;
+			gpios = <&pio 256 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&led_pins_unielec>;
+
+		led3 {
+			label = "u7623-01:green:led3";
+			gpios = <&pio 14 GPIO_ACTIVE_LOW>;
+			default-state = "off";
+		};
+
+		led4 {
+			label = "u7623-01:green:led4";
+			gpios = <&pio 15 GPIO_ACTIVE_LOW>;
+			default-state = "off";
+		};
+	};
+
+	mt7530: switch@0 {
+		compatible = "mediatek,mt7530";
+		#address-cells = <1>;
+		#size-cells = <0>;
+	};
+};
+
+&crypto {
+	status = "okay";
+};
+
+&eth {
+	status = "okay";
+
+	gmac0: mac@0 {
+		compatible = "mediatek,eth-mac";
+		reg = <0>;
+		phy-mode = "trgmii";
+
+		fixed-link {
+			speed = <1000>;
+			full-duplex;
+			pause;
+		};
+	};
+
+	mdio: mdio-bus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		phy5: ethernet-phy@5 {
+			reg = <5>;
+			phy-mode = "rgmii-rxid";
+		};
+	};
+};
+
+&mt7530 {
+	compatible = "mediatek,mt7530";
+	#address-cells = <1>;
+	#size-cells = <0>;
+	reg = <0>;
+	pinctrl-names = "default";
+	mediatek,mcm;
+	resets = <&ethsys 2>;
+	reset-names = "mcm";
+	core-supply = <&mt6323_vpa_reg>;
+	io-supply = <&mt6323_vemc3v3_reg>;
+
+	dsa,mii-bus = <&mdio>;
+
+	ports {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0>;
+
+		port@0 {
+			reg = <0>;
+			label = "lan0";
+			cpu = <&cpu_port0>;
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan1";
+			cpu = <&cpu_port0>;
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan2";
+			cpu = <&cpu_port0>;
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan3";
+			cpu = <&cpu_port0>;
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+			cpu = <&cpu_port0>;
+		};
+
+		cpu_port0: port@6 {
+			reg = <6>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+			phy-mode = "trgmii";
+
+			fixed-link {
+				speed = <1000>;
+				full-duplex;
+			};
+		};
+	};
+};
+
+&mmc0 {
+	pinctrl-names = "default", "state_uhs";
+	pinctrl-0 = <&mmc0_pins_default>;
+	pinctrl-1 = <&mmc0_pins_uhs>;
+	status = "okay";
+	bus-width = <8>;
+	max-frequency = <50000000>;
+	cap-mmc-highspeed;
+	vmmc-supply = <&reg_3p3v>;
+	vqmmc-supply = <&reg_1p8v>;
+	non-removable;
+};
+
+&pio {
+	key_pins_a: keys-alt {
+		pins-keys {
+			pinmux = <MT7623_PIN_256_GPIO256_FUNC_GPIO256>,
+				 <MT7623_PIN_257_GPIO257_FUNC_GPIO257>;
+			input-enable;
+		};
+	};
+
+	led_pins_unielec: leds-unielec {
+		pins-leds {
+			pinmux = <MT7623_PIN_14_GPIO14_FUNC_GPIO14>,
+				 <MT7623_PIN_15_GPIO15_FUNC_GPIO15>;
+		};
+	};
+
+	mmc0_pins_default: mmc0default {
+		pins_cmd_dat {
+			pinmux = <MT7623_PIN_111_MSDC0_DAT7_FUNC_MSDC0_DAT7>,
+				 <MT7623_PIN_112_MSDC0_DAT6_FUNC_MSDC0_DAT6>,
+				 <MT7623_PIN_113_MSDC0_DAT5_FUNC_MSDC0_DAT5>,
+				 <MT7623_PIN_114_MSDC0_DAT4_FUNC_MSDC0_DAT4>,
+				 <MT7623_PIN_118_MSDC0_DAT3_FUNC_MSDC0_DAT3>,
+				 <MT7623_PIN_119_MSDC0_DAT2_FUNC_MSDC0_DAT2>,
+				 <MT7623_PIN_120_MSDC0_DAT1_FUNC_MSDC0_DAT1>,
+				 <MT7623_PIN_121_MSDC0_DAT0_FUNC_MSDC0_DAT0>,
+				 <MT7623_PIN_116_MSDC0_CMD_FUNC_MSDC0_CMD>;
+			input-enable;
+			bias-pull-up;
+		};
+
+		pins_clk {
+			pinmux = <MT7623_PIN_117_MSDC0_CLK_FUNC_MSDC0_CLK>;
+			bias-pull-down;
+		};
+
+		pins_rst {
+			pinmux = <MT7623_PIN_115_MSDC0_RSTB_FUNC_MSDC0_RSTB>;
+			bias-pull-up;
+		};
+	};
+
+	mmc0_pins_uhs: mmc0 {
+		pins_cmd_dat {
+			pinmux = <MT7623_PIN_111_MSDC0_DAT7_FUNC_MSDC0_DAT7>,
+				 <MT7623_PIN_112_MSDC0_DAT6_FUNC_MSDC0_DAT6>,
+				 <MT7623_PIN_113_MSDC0_DAT5_FUNC_MSDC0_DAT5>,
+				 <MT7623_PIN_114_MSDC0_DAT4_FUNC_MSDC0_DAT4>,
+				 <MT7623_PIN_118_MSDC0_DAT3_FUNC_MSDC0_DAT3>,
+				 <MT7623_PIN_119_MSDC0_DAT2_FUNC_MSDC0_DAT2>,
+				 <MT7623_PIN_120_MSDC0_DAT1_FUNC_MSDC0_DAT1>,
+				 <MT7623_PIN_121_MSDC0_DAT0_FUNC_MSDC0_DAT0>,
+				 <MT7623_PIN_116_MSDC0_CMD_FUNC_MSDC0_CMD>;
+			input-enable;
+			drive-strength = <MTK_DRIVE_2mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_01>;
+		};
+
+		pins_clk {
+			pinmux = <MT7623_PIN_117_MSDC0_CLK_FUNC_MSDC0_CLK>;
+			drive-strength = <MTK_DRIVE_2mA>;
+			bias-pull-down = <MTK_PUPD_SET_R1R0_01>;
+		};
+
+		pins_rst {
+			pinmux = <MT7623_PIN_115_MSDC0_RSTB_FUNC_MSDC0_RSTB>;
+			bias-pull-up;
+		};
+	};
+
+	pwm_pins_a: pwm@0 {
+		pins_pwm {
+			pinmux = <MT7623_PIN_203_PWM0_FUNC_PWM0>,
+				 <MT7623_PIN_204_PWM1_FUNC_PWM1>,
+				 <MT7623_PIN_205_PWM2_FUNC_PWM2>,
+				 <MT7623_PIN_206_PWM3_FUNC_PWM3>,
+				 <MT7623_PIN_207_PWM4_FUNC_PWM4>;
+		};
+	};
+
+	uart2_pins_b: uart@2 {
+		pins_dat {
+			pinmux = <MT7623_PIN_200_URXD2_FUNC_URXD2>,
+				 <MT7623_PIN_201_UTXD2_FUNC_UTXD2>;
+		};
+	};
+
+	pcie_default: pcie_pin_default {
+		pins_cmd_dat {
+			pinmux = <MT7623_PIN_208_AUD_EXT_CK1_FUNC_PCIE0_PERST_N>,
+				 <MT7623_PIN_209_AUD_EXT_CK2_FUNC_PCIE1_PERST_N>;
+			bias-disable;
+		};
+	};
+};
+
+&pwm {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pwm_pins_a>;
+	status = "okay";
+};
+
+&pwrap {
+	mt6323 {
+		mt6323led: led {
+			compatible = "mediatek,mt6323-led";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@0 {
+				reg = <0>;
+				label = "led0";
+				default-state = "off";
+			};
+		};
+	};
+};
+
+&uart2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart2_pins_b>;
+	status = "okay";
+};
+
+&usb1 {
+	vusb33-supply = <&reg_3p3v>;
+	vbus-supply = <&reg_3p3v>;
+	status = "okay";
+};
+
+&u3phy1 {
+	status = "okay";
+};
+
+&u3phy2 {
+	status = "okay";
+	mediatek,phy-switch = <&hifsys>;
+};
+
+&pcie {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie_default>;
+	status = "okay";
+
+	pcie@1,0 {
+		status = "okay";
+	};
+
+	pcie@2,0 {
+		status = "okay";
+	};
+};
+
+&pcie1_phy {
+	status = "okay";
+};
+
