From 69a99101748bb1bdb2730393ef48bc152c4d244a Mon Sep 17 00:00:00 2001
From: Tim Harvey <tharvey@gateworks.com>
Date: Tue, 12 Dec 2017 12:49:55 -0800
Subject: [PATCH] net: thunderx: add support for rgmii internal delay modes

The XCV_DLL_CTL is being configured with the assumption that
phy-mode is rgmii-txid (PHY_INTERFACE_MODE_RGMII_TXID) which is not always
the case.

This patch parses the phy-mode property and uses it to configure CXV_DLL_CTL
properly.

Signed-off-by: Tim Harvey <tharvey@gateworks.com>
---
 drivers/net/ethernet/cavium/thunder/thunder_bgx.c | 13 +++++++---
 drivers/net/ethernet/cavium/thunder/thunder_bgx.h |  2 +-
 drivers/net/ethernet/cavium/thunder/thunder_xcv.c | 31 ++++++++++++++++++-----
 3 files changed, 35 insertions(+), 11 deletions(-)

--- a/drivers/net/ethernet/cavium/thunder/thunder_bgx.c
+++ b/drivers/net/ethernet/cavium/thunder/thunder_bgx.c
@@ -55,6 +55,7 @@ struct bgx {
 	struct pci_dev		*pdev;
 	bool                    is_dlm;
 	bool                    is_rgx;
+	int			phy_mode;
 };
 
 static struct bgx *bgx_vnic[MAX_BGX_THUNDER];
@@ -841,12 +842,12 @@ static void bgx_poll_for_link(struct wor
 	queue_delayed_work(lmac->check_link, &lmac->dwork, HZ * 2);
 }
 
-static int phy_interface_mode(u8 lmac_type)
+static int phy_interface_mode(struct bgx *bgx, u8 lmac_type)
 {
 	if (lmac_type == BGX_MODE_QSGMII)
 		return PHY_INTERFACE_MODE_QSGMII;
 	if (lmac_type == BGX_MODE_RGMII)
-		return PHY_INTERFACE_MODE_RGMII;
+		return bgx->phy_mode;
 
 	return PHY_INTERFACE_MODE_SGMII;
 }
@@ -912,7 +913,8 @@ static int bgx_lmac_enable(struct bgx *b
 
 		if (phy_connect_direct(&lmac->netdev, lmac->phydev,
 				       bgx_lmac_handler,
-				       phy_interface_mode(lmac->lmac_type)))
+				       phy_interface_mode(bgx,
+							  lmac->lmac_type)))
 			return -ENODEV;
 
 		phy_start_aneg(lmac->phydev);
@@ -1287,6 +1289,8 @@ static int bgx_init_of_phy(struct bgx *b
 		bgx->lmac[lmac].lmacid = lmac;
 
 		phy_np = of_parse_phandle(node, "phy-handle", 0);
+		if (phy_np)
+			bgx->phy_mode = of_get_phy_mode(phy_np);
 		/* If there is no phy or defective firmware presents
 		 * this cortina phy, for which there is no driver
 		 * support, ignore it.
@@ -1390,7 +1394,6 @@ static int bgx_probe(struct pci_dev *pde
 		bgx->max_lmac = 1;
 		bgx->bgx_id = MAX_BGX_PER_CN81XX - 1;
 		bgx_vnic[bgx->bgx_id] = bgx;
-		xcv_init_hw();
 	}
 
 	/* On 81xx all are DLMs and on 83xx there are 3 BGX QLMs and one
@@ -1407,6 +1410,8 @@ static int bgx_probe(struct pci_dev *pde
 	if (err)
 		goto err_enable;
 
+	if (bgx->is_rgx)
+		xcv_init_hw(bgx->phy_mode);
 	bgx_init_hw(bgx);
 
 	/* Enable all LMACs */
--- a/drivers/net/ethernet/cavium/thunder/thunder_bgx.h
+++ b/drivers/net/ethernet/cavium/thunder/thunder_bgx.h
@@ -226,7 +226,7 @@ void bgx_lmac_internal_loopback(int node
 void bgx_lmac_get_pfc(int node, int bgx_idx, int lmacid, void *pause);
 void bgx_lmac_set_pfc(int node, int bgx_idx, int lmacid, void *pause);
 
-void xcv_init_hw(void);
+void xcv_init_hw(int phy_mode);
 void xcv_setup_link(bool link_up, int link_speed);
 
 u64 bgx_get_rx_stats(int node, int bgx_idx, int lmac, int idx);
--- a/drivers/net/ethernet/cavium/thunder/thunder_xcv.c
+++ b/drivers/net/ethernet/cavium/thunder/thunder_xcv.c
@@ -65,7 +65,7 @@ MODULE_LICENSE("GPL v2");
 MODULE_VERSION(DRV_VERSION);
 MODULE_DEVICE_TABLE(pci, xcv_id_table);
 
-void xcv_init_hw(void)
+void xcv_init_hw(int phy_mode)
 {
 	u64  cfg;
 
@@ -81,12 +81,31 @@ void xcv_init_hw(void)
 	/* Wait for DLL to lock */
 	msleep(1);
 
-	/* Configure DLL - enable or bypass
-	 * TX no bypass, RX bypass
-	 */
+	/* enable/bypass DLL providing MAC based internal TX/RX delays */
 	cfg = readq_relaxed(xcv->reg_base + XCV_DLL_CTL);
-	cfg &= ~0xFF03;
-	cfg |= CLKRX_BYP;
+	cfg &= ~0xffff00;
+	switch (phy_mode) {
+	/* RX and TX delays are added by the MAC */
+	case PHY_INTERFACE_MODE_RGMII:
+		break;
+	/* internal RX and TX delays provided by the PHY */
+	case PHY_INTERFACE_MODE_RGMII_ID:
+		cfg |= CLKRX_BYP;
+		cfg |= CLKTX_BYP;
+		break;
+	/* internal RX delay provided by the PHY, the MAC
+	 * should not add an RX delay in this case
+	 */
+	case PHY_INTERFACE_MODE_RGMII_RXID:
+		cfg |= CLKRX_BYP;
+		break;
+	/* internal TX delay provided by the PHY, the MAC
+	 * should not add an TX delay in this case
+	 */
+	case PHY_INTERFACE_MODE_RGMII_TXID:
+		cfg |= CLKRX_BYP;
+		break;
+	}
 	writeq_relaxed(cfg, xcv->reg_base + XCV_DLL_CTL);
 
 	/* Enable compensation controller and force the
