From 2ba4c76bc645b7b4ff04364f294f3022d369108a Mon Sep 17 00:00:00 2001
From: Yangbo Lu <yangbo.lu@nxp.com>
Date: Thu, 5 Jul 2018 16:20:56 +0800
Subject: [PATCH 04/32] dts: support layercape

This is an integrated patch for layerscape dts support.

Signed-off-by: Amrita Kumari <amrita.kumari@nxp.com>
Signed-off-by: Alison Wang <b18965@freescale.com>
Signed-off-by: Li Yang <leoyang.li@nxp.com>
Signed-off-by: Ashish Kumar <Ashish.Kumar@nxp.com>
Signed-off-by: Zhao Qiang <qiang.zhao@nxp.com>
Signed-off-by: Rajesh Bhagat <rajesh.bhagat@freescale.com>
Signed-off-by: Zhang Ying-22455 <ying.zhang22455@nxp.com>
Signed-off-by: Madalin Bucur <madalin.bucur@nxp.com>
Signed-off-by: Minghuan Lian <Minghuan.Lian@nxp.com>
Signed-off-by: Suresh Gupta <suresh.gupta@nxp.com>
Signed-off-by: Chenhui Zhao <chenhui.zhao@nxp.com>
Signed-off-by: Priyanka Jain <priyanka.jain@nxp.com>
Signed-off-by: Hou Zhiqiang <Zhiqiang.Hou@nxp.com>
Signed-off-by: Changming Huang <jerry.huang@nxp.com>
Signed-off-by: Bharat Bhushan <Bharat.Bhushan@nxp.com>
Signed-off-by: Meng Yi <meng.yi@nxp.com>
Signed-off-by: Shaohui Xie <Shaohui.Xie@nxp.com>
Signed-off-by: Marc Zyngier <marc.zyngier@arm.com>
Signed-off-by: Prabhakar Kushwaha <prabhakar.kushwaha@nxp.com>
Signed-off-by: Ran Wang <ran.wang_1@nxp.com>
Signed-off-by: Yangbo Lu <yangbo.lu@nxp.com>
---
 arch/arm/boot/dts/alpine.dtsi                 |   2 +-
 arch/arm/boot/dts/axm55xx.dtsi                |   2 +-
 arch/arm/boot/dts/ecx-2000.dts                |   2 +-
 arch/arm/boot/dts/imx6ul.dtsi                 |   4 +-
 arch/arm/boot/dts/keystone.dtsi               |   4 +-
 arch/arm/boot/dts/ls1021a-qds.dts             |  26 +
 arch/arm/boot/dts/ls1021a-twr.dts             |  25 +
 arch/arm/boot/dts/ls1021a.dtsi                | 284 ++++--
 arch/arm/boot/dts/mt6580.dtsi                 |   2 +-
 arch/arm/boot/dts/mt6589.dtsi                 |   2 +-
 arch/arm/boot/dts/mt8127.dtsi                 |   2 +-
 arch/arm/boot/dts/mt8135.dtsi                 |   2 +-
 arch/arm/boot/dts/rk3288.dtsi                 |   2 +-
 arch/arm/boot/dts/sun6i-a31.dtsi              |   2 +-
 arch/arm/boot/dts/sun7i-a20.dtsi              |   4 +-
 arch/arm/boot/dts/sun8i-a23-a33.dtsi          |   2 +-
 arch/arm/boot/dts/sun9i-a80.dtsi              |   2 +-
 arch/arm64/boot/dts/freescale/Makefile        |  18 +
 .../boot/dts/freescale/fsl-ls1012a-2g5rdb.dts | 123 +++
 .../boot/dts/freescale/fsl-ls1012a-frdm.dts   | 141 +++
 .../boot/dts/freescale/fsl-ls1012a-frwy.dts   | 177 ++++
 .../boot/dts/freescale/fsl-ls1012a-qds.dts    | 166 ++++
 .../boot/dts/freescale/fsl-ls1012a-rdb.dts    | 102 ++
 .../arm64/boot/dts/freescale/fsl-ls1012a.dtsi | 567 +++++++++++
 .../boot/dts/freescale/fsl-ls1043-post.dtsi   |  44 +
 .../dts/freescale/fsl-ls1043a-qds-sdk.dts     |  71 ++
 .../boot/dts/freescale/fsl-ls1043a-qds.dts    | 210 ++++-
 .../dts/freescale/fsl-ls1043a-rdb-sdk.dts     |  71 ++
 .../dts/freescale/fsl-ls1043a-rdb-usdpaa.dts  | 117 +++
 .../boot/dts/freescale/fsl-ls1043a-rdb.dts    | 152 ++-
 .../arm64/boot/dts/freescale/fsl-ls1043a.dtsi | 357 +++++--
 .../boot/dts/freescale/fsl-ls1046-post.dtsi   |  48 +
 .../dts/freescale/fsl-ls1046a-qds-sdk.dts     | 112 +++
 .../boot/dts/freescale/fsl-ls1046a-qds.dts    | 326 +++++++
 .../dts/freescale/fsl-ls1046a-rdb-sdk.dts     |  85 ++
 .../dts/freescale/fsl-ls1046a-rdb-usdpaa.dts  | 110 +++
 .../boot/dts/freescale/fsl-ls1046a-rdb.dts    | 181 ++++
 .../arm64/boot/dts/freescale/fsl-ls1046a.dtsi | 771 +++++++++++++++
 .../boot/dts/freescale/fsl-ls1088a-qds.dts    | 137 +++
 .../boot/dts/freescale/fsl-ls1088a-rdb.dts    | 200 ++++
 .../arm64/boot/dts/freescale/fsl-ls1088a.dtsi | 800 ++++++++++++++++
 .../boot/dts/freescale/fsl-ls2080a-qds.dts    | 229 +----
 .../boot/dts/freescale/fsl-ls2080a-rdb.dts    | 207 ++--
 .../boot/dts/freescale/fsl-ls2080a-simu.dts   |  47 +-
 .../arm64/boot/dts/freescale/fsl-ls2080a.dtsi | 803 ++--------------
 .../boot/dts/freescale/fsl-ls2081a-rdb.dts    | 161 ++++
 .../boot/dts/freescale/fsl-ls2088a-qds.dts    | 126 +++
 .../boot/dts/freescale/fsl-ls2088a-rdb.dts    | 104 ++
 .../arm64/boot/dts/freescale/fsl-ls2088a.dtsi | 159 ++++
 .../boot/dts/freescale/fsl-ls208xa-qds.dtsi   | 162 ++++
 .../boot/dts/freescale/fsl-ls208xa-rdb.dtsi   | 136 +++
 .../arm64/boot/dts/freescale/fsl-ls208xa.dtsi | 885 ++++++++++++++++++
 .../dts/freescale/qoriq-bman-portals-sdk.dtsi |  55 ++
 .../dts/freescale/qoriq-bman-portals.dtsi     |  77 ++
 .../boot/dts/freescale/qoriq-dpaa-eth.dtsi    |  73 ++
 .../dts/freescale/qoriq-fman3-0-10g-0.dtsi    |  43 +
 .../dts/freescale/qoriq-fman3-0-10g-1.dtsi    |  43 +
 .../dts/freescale/qoriq-fman3-0-1g-0.dtsi     |  42 +
 .../dts/freescale/qoriq-fman3-0-1g-1.dtsi     |  42 +
 .../dts/freescale/qoriq-fman3-0-1g-2.dtsi     |  42 +
 .../dts/freescale/qoriq-fman3-0-1g-3.dtsi     |  42 +
 .../dts/freescale/qoriq-fman3-0-1g-4.dtsi     |  42 +
 .../dts/freescale/qoriq-fman3-0-1g-5.dtsi     |  42 +
 .../boot/dts/freescale/qoriq-fman3-0-6oh.dtsi |  47 +
 .../boot/dts/freescale/qoriq-fman3-0.dtsi     | 130 +++
 .../dts/freescale/qoriq-qman-portals-sdk.dtsi |  38 +
 .../dts/freescale/qoriq-qman-portals.dtsi     |  87 ++
 .../boot/dts/fsl/qoriq-bman1-portals.dtsi     |  10 +
 .../boot/dts/fsl/qoriq-fman3-0-10g-0.dtsi     |   4 +-
 .../boot/dts/fsl/qoriq-fman3-0-10g-1.dtsi     |   4 +-
 70 files changed, 8051 insertions(+), 1286 deletions(-)
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1012a-2g5rdb.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1012a-frdm.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1012a-frwy.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1012a-qds.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1012a-rdb.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1043-post.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1043a-qds-sdk.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb-sdk.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb-usdpaa.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1046-post.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1046a-qds-sdk.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1046a-qds.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb-sdk.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb-usdpaa.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1046a.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1088a-qds.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1088a-rdb.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls2081a-rdb.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls2088a-qds.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls2088a-rdb.dts
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls2088a.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls208xa-qds.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls208xa-rdb.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-bman-portals-sdk.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-bman-portals.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-dpaa-eth.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-10g-0.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-10g-1.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-0.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-1.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-2.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-3.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-4.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-5.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0-6oh.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-fman3-0.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-qman-portals-sdk.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-qman-portals.dtsi

--- a/arch/arm/boot/dts/alpine.dtsi
+++ b/arch/arm/boot/dts/alpine.dtsi
@@ -93,7 +93,7 @@
 			interrupt-controller;
 			reg = <0x0 0xfb001000 0x0 0x1000>,
 			      <0x0 0xfb002000 0x0 0x2000>,
-			      <0x0 0xfb004000 0x0 0x1000>,
+			      <0x0 0xfb004000 0x0 0x2000>,
 			      <0x0 0xfb006000 0x0 0x2000>;
 			interrupts =
 				<GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
--- a/arch/arm/boot/dts/axm55xx.dtsi
+++ b/arch/arm/boot/dts/axm55xx.dtsi
@@ -62,7 +62,7 @@
 		#address-cells = <0>;
 		interrupt-controller;
 		reg = <0x20 0x01001000 0 0x1000>,
-		      <0x20 0x01002000 0 0x1000>,
+		      <0x20 0x01002000 0 0x2000>,
 		      <0x20 0x01004000 0 0x2000>,
 		      <0x20 0x01006000 0 0x2000>;
 		interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) |
--- a/arch/arm/boot/dts/ecx-2000.dts
+++ b/arch/arm/boot/dts/ecx-2000.dts
@@ -99,7 +99,7 @@
 			interrupt-controller;
 			interrupts = <1 9 0xf04>;
 			reg = <0xfff11000 0x1000>,
-			      <0xfff12000 0x1000>,
+			      <0xfff12000 0x2000>,
 			      <0xfff14000 0x2000>,
 			      <0xfff16000 0x2000>;
 		};
--- a/arch/arm/boot/dts/imx6ul.dtsi
+++ b/arch/arm/boot/dts/imx6ul.dtsi
@@ -89,11 +89,11 @@
 	};
 
 	intc: interrupt-controller@00a01000 {
-		compatible = "arm,cortex-a7-gic";
+		compatible = "arm,gic-400", "arm,cortex-a7-gic";
 		#interrupt-cells = <3>;
 		interrupt-controller;
 		reg = <0x00a01000 0x1000>,
-		      <0x00a02000 0x1000>,
+		      <0x00a02000 0x2000>,
 		      <0x00a04000 0x2000>,
 		      <0x00a06000 0x2000>;
 	};
--- a/arch/arm/boot/dts/keystone.dtsi
+++ b/arch/arm/boot/dts/keystone.dtsi
@@ -30,12 +30,12 @@
 	};
 
 	gic: interrupt-controller {
-		compatible = "arm,cortex-a15-gic";
+		compatible = "arm,gic-400", "arm,cortex-a15-gic";
 		#interrupt-cells = <3>;
 		interrupt-controller;
 		reg = <0x0 0x02561000 0x0 0x1000>,
 		      <0x0 0x02562000 0x0 0x2000>,
-		      <0x0 0x02564000 0x0 0x1000>,
+		      <0x0 0x02564000 0x0 0x2000>,
 		      <0x0 0x02566000 0x0 0x2000>;
 		interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) |
 				IRQ_TYPE_LEVEL_HIGH)>;
--- a/arch/arm/boot/dts/ls1021a-qds.dts
+++ b/arch/arm/boot/dts/ls1021a-qds.dts
@@ -124,6 +124,19 @@
 	};
 };
 
+&qspi {
+	num-cs = <2>;
+	status = "okay";
+
+	qflash0: s25fl128s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+};
+
 &enet0 {
 	tbi-handle = <&tbi0>;
 	phy-handle = <&sgmii_phy1c>;
@@ -239,6 +252,11 @@
 		device-width = <1>;
 	};
 
+	nand@2,0 {
+		compatible = "fsl,ifc-nand";
+		reg = <0x2 0x0 0x10000>;
+	};
+
 	fpga: board-control@3,0 {
 		#address-cells = <1>;
 		#size-cells = <1>;
@@ -331,3 +349,11 @@
 &uart1 {
 	status = "okay";
 };
+
+&can0 {
+	status = "okay";
+};
+
+&can1 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/ls1021a-twr.dts
+++ b/arch/arm/boot/dts/ls1021a-twr.dts
@@ -142,6 +142,19 @@
 	};
 };
 
+&qspi {
+	num-cs = <2>;
+	status = "okay";
+
+	qflash0: n25q128a13@0 {
+		compatible = "n25q128a13", "jedec,spi-nor";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+};
+
 &enet0 {
 	tbi-handle = <&tbi1>;
 	phy-handle = <&sgmii_phy2>;
@@ -228,6 +241,10 @@
 	};
 };
 
+&esdhc {
+        status = "okay";
+};
+
 &sai1 {
 	status = "okay";
 };
@@ -243,3 +260,11 @@
 &uart1 {
 	status = "okay";
 };
+
+&can0 {
+	status = "okay";
+};
+
+&can1 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/ls1021a.dtsi
+++ b/arch/arm/boot/dts/ls1021a.dtsi
@@ -47,6 +47,7 @@
 
 #include "skeleton64.dtsi"
 #include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/thermal/thermal.h>
 
 / {
 	compatible = "fsl,ls1021a";
@@ -70,21 +71,29 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 
-		cpu@f00 {
+		cpu0: @f00 {
 			compatible = "arm,cortex-a7";
 			device_type = "cpu";
 			reg = <0xf00>;
-			clocks = <&cluster1_clk>;
+			clocks = <&clockgen 1 0>;
+			#cooling-cells = <2>;
 		};
 
-		cpu@f01 {
+		cpu1: @f01 {
 			compatible = "arm,cortex-a7";
 			device_type = "cpu";
 			reg = <0xf01>;
-			clocks = <&cluster1_clk>;
+			clocks = <&clockgen 1 0>;
 		};
 	};
 
+	sysclk: sysclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <100000000>;
+		clock-output-names = "sysclk";
+	};
+
 	timer {
 		compatible = "arm,armv7-timer";
 		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
@@ -108,11 +117,11 @@
 		ranges;
 
 		gic: interrupt-controller@1400000 {
-			compatible = "arm,cortex-a7-gic";
+			compatible = "arm,gic-400", "arm,cortex-a7-gic";
 			#interrupt-cells = <3>;
 			interrupt-controller;
 			reg = <0x0 0x1401000 0x0 0x1000>,
-			      <0x0 0x1402000 0x0 0x1000>,
+			      <0x0 0x1402000 0x0 0x2000>,
 			      <0x0 0x1404000 0x0 0x2000>,
 			      <0x0 0x1406000 0x0 0x2000>;
 			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_HIGH)>;
@@ -120,14 +129,14 @@
 		};
 
 		msi1: msi-controller@1570e00 {
-			compatible = "fsl,1s1021a-msi";
+			compatible = "fsl,ls1021a-msi";
 			reg = <0x0 0x1570e00 0x0 0x8>;
 			msi-controller;
 			interrupts =  <GIC_SPI 179 IRQ_TYPE_LEVEL_HIGH>;
 		};
 
 		msi2: msi-controller@1570e08 {
-			compatible = "fsl,1s1021a-msi";
+			compatible = "fsl,ls1021a-msi";
 			reg = <0x0 0x1570e08 0x0 0x8>;
 			msi-controller;
 			interrupts = <GIC_SPI 180 IRQ_TYPE_LEVEL_HIGH>;
@@ -137,11 +146,12 @@
 			compatible = "fsl,ifc", "simple-bus";
 			reg = <0x0 0x1530000 0x0 0x10000>;
 			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
+			big-endian;
 		};
 
 		dcfg: dcfg@1ee0000 {
 			compatible = "fsl,ls1021a-dcfg", "syscon";
-			reg = <0x0 0x1ee0000 0x0 0x10000>;
+			reg = <0x0 0x1ee0000 0x0 0x1000>;
 			big-endian;
 		};
 
@@ -163,7 +173,7 @@
 			      <0x0 0x20220520 0x0 0x4>;
 			reg-names = "ahci", "sata-ecc";
 			interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			dma-coherent;
 			status = "disabled";
 		};
@@ -214,43 +224,89 @@
 		};
 
 		clockgen: clocking@1ee1000 {
-			#address-cells = <1>;
-			#size-cells = <1>;
-			ranges = <0x0 0x0 0x1ee1000 0x10000>;
+			compatible = "fsl,ls1021a-clockgen";
+			reg = <0x0 0x1ee1000 0x0 0x1000>;
+			#clock-cells = <2>;
+			clocks = <&sysclk>;
+		};
 
-			sysclk: sysclk {
-				compatible = "fixed-clock";
-				#clock-cells = <0>;
-				clock-output-names = "sysclk";
-			};
-
-			cga_pll1: pll@800 {
-				compatible = "fsl,qoriq-core-pll-2.0";
-				#clock-cells = <1>;
-				reg = <0x800 0x10>;
-				clocks = <&sysclk>;
-				clock-output-names = "cga-pll1", "cga-pll1-div2",
-						     "cga-pll1-div4";
-			};
-
-			platform_clk: pll@c00 {
-				compatible = "fsl,qoriq-core-pll-2.0";
-				#clock-cells = <1>;
-				reg = <0xc00 0x10>;
-				clocks = <&sysclk>;
-				clock-output-names = "platform-clk", "platform-clk-div2";
-			};
-
-			cluster1_clk: clk0c0@0 {
-				compatible = "fsl,qoriq-core-mux-2.0";
-				#clock-cells = <0>;
-				reg = <0x0 0x10>;
-				clock-names = "pll1cga", "pll1cga-div2", "pll1cga-div4";
-				clocks = <&cga_pll1 0>, <&cga_pll1 1>, <&cga_pll1 2>;
-				clock-output-names = "cluster1-clk";
+		tmu: tmu@1f00000 {
+			compatible = "fsl,qoriq-tmu";
+			reg = <0x0 0x1f00000 0x0 0x10000>;
+			interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
+			fsl,tmu-range = <0xb0000 0xa0026 0x80048 0x30061>;
+			fsl,tmu-calibration = <0x00000000 0x0000000f
+					       0x00000001 0x00000017
+					       0x00000002 0x0000001e
+					       0x00000003 0x00000026
+					       0x00000004 0x0000002e
+					       0x00000005 0x00000035
+					       0x00000006 0x0000003d
+					       0x00000007 0x00000044
+					       0x00000008 0x0000004c
+					       0x00000009 0x00000053
+					       0x0000000a 0x0000005b
+					       0x0000000b 0x00000064
+
+					       0x00010000 0x00000011
+					       0x00010001 0x0000001c
+					       0x00010002 0x00000024
+					       0x00010003 0x0000002b
+					       0x00010004 0x00000034
+					       0x00010005 0x00000039
+					       0x00010006 0x00000042
+					       0x00010007 0x0000004c
+					       0x00010008 0x00000051
+					       0x00010009 0x0000005a
+					       0x0001000a 0x00000063
+
+					       0x00020000 0x00000013
+					       0x00020001 0x00000019
+					       0x00020002 0x00000024
+					       0x00020003 0x0000002c
+					       0x00020004 0x00000035
+					       0x00020005 0x0000003d
+					       0x00020006 0x00000046
+					       0x00020007 0x00000050
+					       0x00020008 0x00000059
+
+					       0x00030000 0x00000002
+					       0x00030001 0x0000000d
+					       0x00030002 0x00000019
+					       0x00030003 0x00000024>;
+			#thermal-sensor-cells = <1>;
+		};
+
+		thermal-zones {
+			cpu_thermal: cpu-thermal {
+				polling-delay-passive = <1000>;
+				polling-delay = <5000>;
+
+				thermal-sensors = <&tmu 0>;
+
+				trips {
+					cpu_alert: cpu-alert {
+						temperature = <85000>;
+						hysteresis = <2000>;
+						type = "passive";
+					};
+					cpu_crit: cpu-crit {
+						temperature = <95000>;
+						hysteresis = <2000>;
+						type = "critical";
+					};
+				};
+
+				cooling-maps {
+					map0 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu0 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+				};
 			};
 		};
-
 		dspi0: dspi@2100000 {
 			compatible = "fsl,ls1021a-v1.0-dspi";
 			#address-cells = <1>;
@@ -258,7 +314,7 @@
 			reg = <0x0 0x2100000 0x0 0x10000>;
 			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "dspi";
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			spi-num-chipselects = <6>;
 			big-endian;
 			status = "disabled";
@@ -271,31 +327,48 @@
 			reg = <0x0 0x2110000 0x0 0x10000>;
 			interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "dspi";
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			spi-num-chipselects = <6>;
 			big-endian;
 			status = "disabled";
 		};
 
+		qspi: quadspi@1550000 {
+			compatible = "fsl,ls1021a-qspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x1550000 0x0 0x10000>,
+				<0x0 0x40000000 0x0 0x4000000>;
+			reg-names = "QuadSPI", "QuadSPI-memory";
+			interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;
+			clock-names = "qspi_en", "qspi";
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
+			big-endian;
+			amba-base = <0x40000000>;
+			status = "disabled";
+		};
+
 		i2c0: i2c@2180000 {
-			compatible = "fsl,vf610-i2c";
+			compatible = "fsl,vf610-i2c", "fsl,ls1021a-vf610-i2c";
 			#address-cells = <1>;
 			#size-cells = <0>;
 			reg = <0x0 0x2180000 0x0 0x10000>;
 			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "i2c";
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
+			fsl-scl-gpio = <&gpio3 23 0>;
 			status = "disabled";
 		};
 
 		i2c1: i2c@2190000 {
-			compatible = "fsl,vf610-i2c";
+			compatible = "fsl,vf610-i2c", "fsl,ls1021a-vf610-i2c";
 			#address-cells = <1>;
 			#size-cells = <0>;
 			reg = <0x0 0x2190000 0x0 0x10000>;
 			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "i2c";
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
+			fsl-scl-gpio = <&gpio3 23 0>;
 			status = "disabled";
 		};
 
@@ -306,7 +379,7 @@
 			reg = <0x0 0x21a0000 0x0 0x10000>;
 			interrupts = <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "i2c";
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			status = "disabled";
 		};
 
@@ -399,7 +472,7 @@
 			compatible = "fsl,ls1021a-lpuart";
 			reg = <0x0 0x2960000 0x0 0x1000>;
 			interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			clock-names = "ipg";
 			status = "disabled";
 		};
@@ -408,7 +481,7 @@
 			compatible = "fsl,ls1021a-lpuart";
 			reg = <0x0 0x2970000 0x0 0x1000>;
 			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			clock-names = "ipg";
 			status = "disabled";
 		};
@@ -417,7 +490,7 @@
 			compatible = "fsl,ls1021a-lpuart";
 			reg = <0x0 0x2980000 0x0 0x1000>;
 			interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			clock-names = "ipg";
 			status = "disabled";
 		};
@@ -426,7 +499,7 @@
 			compatible = "fsl,ls1021a-lpuart";
 			reg = <0x0 0x2990000 0x0 0x1000>;
 			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			clock-names = "ipg";
 			status = "disabled";
 		};
@@ -435,16 +508,26 @@
 			compatible = "fsl,ls1021a-lpuart";
 			reg = <0x0 0x29a0000 0x0 0x1000>;
 			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			clock-names = "ipg";
 			status = "disabled";
 		};
 
+		ftm0: ftm0@29d0000 {
+			compatible = "fsl,ls1021a-ftm";
+			reg = <0x0 0x29d0000 0x0 0x10000>,
+			      <0x0 0x1ee2140 0x0 0x4>;
+			reg-names = "ftm", "FlexTimer1";
+			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
+			big-endian;
+			status = "okay";
+		};
+
 		wdog0: watchdog@2ad0000 {
 			compatible = "fsl,imx21-wdt";
 			reg = <0x0 0x2ad0000 0x0 0x10000>;
 			interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>;
+			clocks = <&clockgen 4 1>;
 			clock-names = "wdog-en";
 			big-endian;
 		};
@@ -454,8 +537,8 @@
 			compatible = "fsl,vf610-sai";
 			reg = <0x0 0x2b50000 0x0 0x10000>;
 			interrupts = <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>, <&platform_clk 1>,
-				 <&platform_clk 1>, <&platform_clk 1>;
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
+				 <&clockgen 4 1>, <&clockgen 4 1>;
 			clock-names = "bus", "mclk1", "mclk2", "mclk3";
 			dma-names = "tx", "rx";
 			dmas = <&edma0 1 47>,
@@ -468,8 +551,8 @@
 			compatible = "fsl,vf610-sai";
 			reg = <0x0 0x2b60000 0x0 0x10000>;
 			interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 1>, <&platform_clk 1>,
-				 <&platform_clk 1>, <&platform_clk 1>;
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
+				 <&clockgen 4 1>, <&clockgen 4 1>;
 			clock-names = "bus", "mclk1", "mclk2", "mclk3";
 			dma-names = "tx", "rx";
 			dmas = <&edma0 1 45>,
@@ -489,16 +572,31 @@
 			dma-channels = <32>;
 			big-endian;
 			clock-names = "dmamux0", "dmamux1";
-			clocks = <&platform_clk 1>,
-				 <&platform_clk 1>;
+			clocks = <&clockgen 4 1>,
+				 <&clockgen 4 1>;
+		};
+
+		qdma: qdma@8390000 {
+			compatible = "fsl,ls1021a-qdma";
+			reg = <0x0 0x8398000 0x0 0x1000>, /* Controller regs */
+			      <0x0 0x8399000 0x0 0x1000>, /* Status regs */
+			      <0x0 0x839a000 0x0 0x2000>; /* Block regs */
+			interrupts = <GIC_SPI 185 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "qdma-error", "qdma-queue";
+			channels = <8>;
+			queues = <2>;
+			status-sizes = <64>;
+			queue-sizes = <64 64>;
+			big-endian;
 		};
 
 		dcu: dcu@2ce0000 {
 			compatible = "fsl,ls1021a-dcu";
 			reg = <0x0 0x2ce0000 0x0 0x10000>;
 			interrupts = <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&platform_clk 0>,
-				<&platform_clk 0>;
+			clocks = <&clockgen 4 0>,
+				<&clockgen 4 0>;
 			clock-names = "dcu", "pix";
 			big-endian;
 			status = "disabled";
@@ -626,7 +724,11 @@
 			interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
 			dr_mode = "host";
 			snps,quirk-frame-length-adjustment = <0x20>;
+			configure-gfladj;
+			dma-coherent;
 			snps,dis_rxdet_inp3_quirk;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
 		};
 
 		pcie@3400000 {
@@ -634,7 +736,9 @@
 			reg = <0x00 0x03400000 0x0 0x00010000   /* controller registers */
 			       0x40 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>; /* controller interrupt */
+			interrupts = <GIC_SPI 181 IRQ_TYPE_LEVEL_HIGH>,
+					   <GIC_SPI 183 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
+			interrupt-names = "pme", "aer";
 			fsl,pcie-scfg = <&scfg 0>;
 			#address-cells = <3>;
 			#size-cells = <2>;
@@ -643,7 +747,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x40 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x40 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi1>;
+			msi-parent = <&msi1>, <&msi2>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic GIC_SPI 91  IRQ_TYPE_LEVEL_HIGH>,
@@ -657,7 +761,9 @@
 			reg = <0x00 0x03500000 0x0 0x00010000   /* controller registers */
 			       0x48 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
+			interrupts = <GIC_SPI 182 IRQ_TYPE_LEVEL_HIGH>,
+					   <GIC_SPI 184 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
+			interrupt-names = "pme", "aer";
 			fsl,pcie-scfg = <&scfg 1>;
 			#address-cells = <3>;
 			#size-cells = <2>;
@@ -666,7 +772,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x48 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x48 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi2>;
+			msi-parent = <&msi1>, <&msi2>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic GIC_SPI 92  IRQ_TYPE_LEVEL_HIGH>,
@@ -674,5 +780,45 @@
 					<0000 0 0 3 &gic GIC_SPI 191 IRQ_TYPE_LEVEL_HIGH>,
 					<0000 0 0 4 &gic GIC_SPI 193 IRQ_TYPE_LEVEL_HIGH>;
 		};
+
+		can0: can@2a70000 {
+			compatible = "fsl,ls1021ar2-flexcan";
+			reg = <0x0 0x2a70000 0x0 0x1000>;
+			interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
+			clock-names = "ipg", "per";
+			big-endian;
+			status = "disabled";
+		};
+
+		can1: can@2a80000 {
+			compatible = "fsl,ls1021ar2-flexcan";
+			reg = <0x0 0x2a80000 0x0 0x1000>;
+			interrupts = <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
+			clock-names = "ipg", "per";
+			big-endian;
+			status = "disabled";
+		};
+
+		can2: can@2a90000 {
+			compatible = "fsl,ls1021ar2-flexcan";
+			reg = <0x0 0x2a90000 0x0 0x1000>;
+			interrupts = <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
+			clock-names = "ipg", "per";
+			big-endian;
+			status = "disabled";
+		};
+
+		can3: can@2aa0000 {
+			compatible = "fsl,ls1021ar2-flexcan";
+			reg = <0x0 0x2aa0000 0x0 0x1000>;
+			interrupts = <GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
+			clock-names = "ipg", "per";
+			big-endian;
+			status = "disabled";
+		};
 	};
 };
--- a/arch/arm/boot/dts/mt6580.dtsi
+++ b/arch/arm/boot/dts/mt6580.dtsi
@@ -91,7 +91,7 @@
 		#interrupt-cells = <3>;
 		interrupt-parent = <&gic>;
 		reg = <0x10211000 0x1000>,
-		      <0x10212000 0x1000>,
+		      <0x10212000 0x2000>,
 		      <0x10214000 0x2000>,
 		      <0x10216000 0x2000>;
 	};
--- a/arch/arm/boot/dts/mt6589.dtsi
+++ b/arch/arm/boot/dts/mt6589.dtsi
@@ -102,7 +102,7 @@
 			#interrupt-cells = <3>;
 			interrupt-parent = <&gic>;
 			reg = <0x10211000 0x1000>,
-			      <0x10212000 0x1000>,
+			      <0x10212000 0x2000>,
 			      <0x10214000 0x2000>,
 			      <0x10216000 0x2000>;
 		};
--- a/arch/arm/boot/dts/mt8127.dtsi
+++ b/arch/arm/boot/dts/mt8127.dtsi
@@ -129,7 +129,7 @@
 			#interrupt-cells = <3>;
 			interrupt-parent = <&gic>;
 			reg = <0 0x10211000 0 0x1000>,
-			      <0 0x10212000 0 0x1000>,
+			      <0 0x10212000 0 0x2000>,
 			      <0 0x10214000 0 0x2000>,
 			      <0 0x10216000 0 0x2000>;
 		};
--- a/arch/arm/boot/dts/mt8135.dtsi
+++ b/arch/arm/boot/dts/mt8135.dtsi
@@ -221,7 +221,7 @@
 			#interrupt-cells = <3>;
 			interrupt-parent = <&gic>;
 			reg = <0 0x10211000 0 0x1000>,
-			      <0 0x10212000 0 0x1000>,
+			      <0 0x10212000 0 0x2000>,
 			      <0 0x10214000 0 0x2000>,
 			      <0 0x10216000 0 0x2000>;
 		};
--- a/arch/arm/boot/dts/rk3288.dtsi
+++ b/arch/arm/boot/dts/rk3288.dtsi
@@ -1109,7 +1109,7 @@
 		#address-cells = <0>;
 
 		reg = <0xffc01000 0x1000>,
-		      <0xffc02000 0x1000>,
+		      <0xffc02000 0x2000>,
 		      <0xffc04000 0x2000>,
 		      <0xffc06000 0x2000>;
 		interrupts = <GIC_PPI 9 0xf04>;
--- a/arch/arm/boot/dts/sun6i-a31.dtsi
+++ b/arch/arm/boot/dts/sun6i-a31.dtsi
@@ -791,7 +791,7 @@
 		gic: interrupt-controller@01c81000 {
 			compatible = "arm,cortex-a7-gic", "arm,cortex-a15-gic";
 			reg = <0x01c81000 0x1000>,
-			      <0x01c82000 0x1000>,
+			      <0x01c82000 0x2000>,
 			      <0x01c84000 0x2000>,
 			      <0x01c86000 0x2000>;
 			interrupt-controller;
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -1685,9 +1685,9 @@
 		};
 
 		gic: interrupt-controller@01c81000 {
-			compatible = "arm,cortex-a7-gic", "arm,cortex-a15-gic";
+			compatible = "arm,gic-400", "arm,cortex-a7-gic", "arm,cortex-a15-gic";
 			reg = <0x01c81000 0x1000>,
-			      <0x01c82000 0x1000>,
+			      <0x01c82000 0x2000>,
 			      <0x01c84000 0x2000>,
 			      <0x01c86000 0x2000>;
 			interrupt-controller;
--- a/arch/arm/boot/dts/sun8i-a23-a33.dtsi
+++ b/arch/arm/boot/dts/sun8i-a23-a33.dtsi
@@ -488,7 +488,7 @@
 		gic: interrupt-controller@01c81000 {
 			compatible = "arm,cortex-a7-gic", "arm,cortex-a15-gic";
 			reg = <0x01c81000 0x1000>,
-			      <0x01c82000 0x1000>,
+			      <0x01c82000 0x2000>,
 			      <0x01c84000 0x2000>,
 			      <0x01c86000 0x2000>;
 			interrupt-controller;
--- a/arch/arm/boot/dts/sun9i-a80.dtsi
+++ b/arch/arm/boot/dts/sun9i-a80.dtsi
@@ -613,7 +613,7 @@
 		gic: interrupt-controller@01c41000 {
 			compatible = "arm,cortex-a7-gic", "arm,cortex-a15-gic";
 			reg = <0x01c41000 0x1000>,
-			      <0x01c42000 0x1000>,
+			      <0x01c42000 0x2000>,
 			      <0x01c44000 0x2000>,
 			      <0x01c46000 0x2000>;
 			interrupt-controller;
--- a/arch/arm64/boot/dts/freescale/Makefile
+++ b/arch/arm64/boot/dts/freescale/Makefile
@@ -1,8 +1,26 @@
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1012a-frdm.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1012a-frwy.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1012a-qds.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1012a-rdb.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1012a-2g5rdb.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1043a-qds.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1043a-qds-sdk.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1043a-rdb.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1043a-rdb-sdk.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1043a-rdb-usdpaa.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1046a-qds.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1046a-qds-sdk.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1046a-rdb.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1046a-rdb-sdk.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1046a-rdb-usdpaa.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1088a-qds.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1088a-rdb.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2080a-qds.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2080a-rdb.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2081a-rdb.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2080a-simu.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2088a-qds.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2088a-rdb.dtb
  
 always		:= $(dtb-y)
 subdir-y	:= $(dts-dirs)
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a-2g5rdb.dts
@@ -0,0 +1,123 @@
+/*
+ * Device Tree file for NXP LS1012A 2G5RDB Board.
+ *
+ * Copyright 2017 NXP
+ *
+ * Bhaskar Upadhaya <bhaskar.upadhaya@nxp.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+/dts-v1/;
+
+#include "fsl-ls1012a.dtsi"
+
+/ {
+	model = "LS1012A 2G5RDB Board";
+	compatible = "fsl,ls1012a-rdb", "fsl,ls1012a";
+
+	aliases {
+		ethernet0 = &pfe_mac0;
+		ethernet1 = &pfe_mac1;
+	};
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+};
+
+&qspi {
+	num-cs = <2>;
+	bus-num = <0>;
+	status = "okay";
+
+	qflash0: s25fs512s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		m25p,fast-read;
+		reg = <0>;
+	};
+};
+
+&sata {
+	status = "okay";
+};
+
+&pfe {
+	status = "okay";
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	ethernet@0 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x0>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x0>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x1>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "sgmii-2500";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x1>; /* enabled/disabled */
+		};
+	};
+
+	ethernet@1 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x1>;	/* GEM_ID */
+		fsl,gemac-bus-id = < 0x0>;	/* BUS_ID */
+		fsl,gemac-phy-id = < 0x2>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "sgmii-2500";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x0>; /* enabled/disabled */
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a-frdm.dts
@@ -0,0 +1,141 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for Freescale LS1012A Freedom Board.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ */
+/dts-v1/;
+
+#include "fsl-ls1012a.dtsi"
+
+/ {
+	model = "LS1012A Freedom Board";
+	compatible = "fsl,ls1012a-frdm", "fsl,ls1012a";
+
+	aliases {
+		ethernet0 = &pfe_mac0;
+		ethernet1 = &pfe_mac1;
+	};
+
+	sys_mclk: clock-mclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <25000000>;
+	};
+
+	reg_1p8v: regulator-1p8v {
+		compatible = "regulator-fixed";
+		regulator-name = "1P8V";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-always-on;
+	};
+
+	sound {
+		compatible = "simple-audio-card";
+		simple-audio-card,format = "i2s";
+		simple-audio-card,widgets =
+			"Microphone", "Microphone Jack",
+			"Headphone", "Headphone Jack",
+			"Speaker", "Speaker Ext",
+			"Line", "Line In Jack";
+		simple-audio-card,routing =
+			"MIC_IN", "Microphone Jack",
+			"Microphone Jack", "Mic Bias",
+			"LINE_IN", "Line In Jack",
+			"Headphone Jack", "HP_OUT",
+			"Speaker Ext", "LINE_OUT";
+
+		simple-audio-card,cpu {
+			sound-dai = <&sai2>;
+			frame-master;
+			bitclock-master;
+		};
+
+		simple-audio-card,codec {
+			sound-dai = <&codec>;
+			frame-master;
+			bitclock-master;
+			system-clock-frequency = <25000000>;
+		};
+	};
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+
+	codec: sgtl5000@a {
+		#sound-dai-cells = <0>;
+		compatible = "fsl,sgtl5000";
+		reg = <0xa>;
+		VDDA-supply = <&reg_1p8v>;
+		VDDIO-supply = <&reg_1p8v>;
+		clocks = <&sys_mclk>;
+	};
+};
+
+&qspi {
+	num-cs = <1>;
+	bus-num = <0>;
+	status = "okay";
+
+	qflash0: s25fs512s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		m25p,fast-read;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+};
+
+&pfe {
+	status = "okay";
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	ethernet@0 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x0>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x0>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x2>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "sgmii";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x1>; /* enabled/disabled */
+		};
+	};
+
+	ethernet@1 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x1>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x1>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x1>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "sgmii";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x0>; /* enabled/disabled */
+		};
+	};
+};
+
+&sai2 {
+	status = "okay";
+};
+
+&sata {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a-frwy.dts
@@ -0,0 +1,177 @@
+/*
+ * Device Tree file for NXP LS1012A FRWY Board.
+ *
+ * Copyright 2018 NXP
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+/dts-v1/;
+
+#include "fsl-ls1012a.dtsi"
+
+/ {
+	model = "LS1012A FRWY Board";
+	compatible = "fsl,ls1012a-frwy", "fsl,ls1012a";
+
+	aliases {
+		ethernet0 = &pfe_mac0;
+		ethernet1 = &pfe_mac1;
+	};
+
+	sys_mclk: clock-mclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <25000000>;
+	};
+
+	reg_1p8v: regulator-1p8v {
+		compatible = "regulator-fixed";
+		regulator-name = "1P8V";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-always-on;
+	};
+
+	sound {
+		compatible = "simple-audio-card";
+		simple-audio-card,format = "i2s";
+		simple-audio-card,widgets =
+			"Microphone", "Microphone Jack",
+			"Headphone", "Headphone Jack",
+			"Speaker", "Speaker Ext",
+			"Line", "Line In Jack";
+		simple-audio-card,routing =
+			"MIC_IN", "Microphone Jack",
+			"Microphone Jack", "Mic Bias",
+			"LINE_IN", "Line In Jack",
+			"Headphone Jack", "HP_OUT",
+			"Speaker Ext", "LINE_OUT";
+
+		simple-audio-card,cpu {
+			sound-dai = <&sai2>;
+			frame-master;
+			bitclock-master;
+		};
+
+		simple-audio-card,codec {
+			sound-dai = <&codec>;
+			frame-master;
+			bitclock-master;
+			system-clock-frequency = <25000000>;
+		};
+	};
+};
+
+&pcie {
+	status = "okay";
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+
+	codec: sgtl5000@a {
+		compatible = "fsl,sgtl5000";
+		#sound-dai-cells = <0>;
+		reg = <0xa>;
+		VDDA-supply = <&reg_1p8v>;
+		VDDIO-supply = <&reg_1p8v>;
+		clocks = <&sys_mclk>;
+	};
+};
+
+&qspi {
+	num-cs = <1>;
+	bus-num = <0>;
+	status = "okay";
+
+	qflash0: w25q16dw@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		m25p,fast-read;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+};
+
+&pfe {
+	status = "okay";
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	ethernet@0 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x0>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x0>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x2>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "sgmii";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x1>; /* enabled/disabled */
+		};
+	};
+
+	ethernet@1 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x1>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x1>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x1>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "sgmii";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x0>; /* enabled/disabled */
+		};
+	};
+};
+
+&sai2 {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a-qds.dts
@@ -0,0 +1,166 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for Freescale LS1012A QDS Board.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ */
+/dts-v1/;
+
+#include "fsl-ls1012a.dtsi"
+
+/ {
+	model = "LS1012A QDS Board";
+	compatible = "fsl,ls1012a-qds", "fsl,ls1012a";
+
+	aliases {
+		ethernet0 = &pfe_mac0;
+		ethernet1 = &pfe_mac1;
+	};
+
+	sys_mclk: clock-mclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <24576000>;
+	};
+
+	reg_3p3v: regulator-3p3v {
+		compatible = "regulator-fixed";
+		regulator-name = "3P3V";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-always-on;
+	};
+
+	sound {
+		compatible = "simple-audio-card";
+		simple-audio-card,format = "i2s";
+		simple-audio-card,widgets =
+			"Microphone", "Microphone Jack",
+			"Headphone", "Headphone Jack",
+			"Speaker", "Speaker Ext",
+			"Line", "Line In Jack";
+		simple-audio-card,routing =
+			"MIC_IN", "Microphone Jack",
+			"Microphone Jack", "Mic Bias",
+			"LINE_IN", "Line In Jack",
+			"Headphone Jack", "HP_OUT",
+			"Speaker Ext", "LINE_OUT";
+
+		simple-audio-card,cpu {
+			sound-dai = <&sai2>;
+			frame-master;
+			bitclock-master;
+		};
+
+		simple-audio-card,codec {
+			sound-dai = <&codec>;
+			frame-master;
+			bitclock-master;
+			system-clock-frequency = <24576000>;
+		};
+	};
+};
+
+&pcie {
+	status = "okay";
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+
+	pca9547@77 {
+		compatible = "nxp,pca9547";
+		reg = <0x77>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		i2c@4 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x4>;
+
+			codec: sgtl5000@a {
+				#sound-dai-cells = <0>;
+				compatible = "fsl,sgtl5000";
+				reg = <0xa>;
+				VDDA-supply = <&reg_3p3v>;
+				VDDIO-supply = <&reg_3p3v>;
+				clocks = <&sys_mclk>;
+			};
+		};
+	};
+};
+
+&qspi {
+	num-cs = <2>;
+	bus-num = <0>;
+	status = "okay";
+
+	qflash0: s25fs512s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		m25p,fast-read;
+		reg = <0>;
+	};
+};
+
+&pfe {
+	status = "okay";
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	ethernet@0 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x0>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x0>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x1>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x2>;
+		phy-mode = "sgmii-2500";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x1>; /* enabled/disabled */
+		};
+	};
+
+	ethernet@1 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x1>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x1>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x2>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x3>;
+		phy-mode = "sgmii-2500";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x0>; /* enabled/disabled */
+		};
+	};
+};
+
+&sai2 {
+	status = "okay";
+};
+
+&sata {
+	status = "okay";
+};
+
+&esdhc0 {
+	status = "okay";
+};
+
+&esdhc1 {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a-rdb.dts
@@ -0,0 +1,102 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for Freescale LS1012A RDB Board.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ */
+/dts-v1/;
+
+#include "fsl-ls1012a.dtsi"
+
+/ {
+	model = "LS1012A RDB Board";
+	compatible = "fsl,ls1012a-rdb", "fsl,ls1012a";
+
+	aliases {
+		ethernet0 = &pfe_mac0;
+		ethernet1 = &pfe_mac1;
+	};
+};
+
+&pcie {
+	status = "okay";
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+};
+
+&qspi {
+	num-cs = <2>;
+	bus-num = <0>;
+	status = "okay";
+
+	qflash0: s25fs512s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		m25p,fast-read;
+		reg = <0>;
+	};
+};
+
+&sata {
+	status = "okay";
+};
+
+&esdhc0 {
+	sd-uhs-sdr104;
+	sd-uhs-sdr50;
+	sd-uhs-sdr25;
+	sd-uhs-sdr12;
+	status = "okay";
+};
+
+&esdhc1 {
+	mmc-hs200-1_8v;
+	status = "okay";
+};
+
+&pfe {
+	status = "okay";
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	ethernet@0 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x0>;	/* GEM_ID */
+		fsl,gemac-bus-id = <0x0>;	/* BUS_ID */
+		fsl,gemac-phy-id = <0x2>;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "sgmii";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x1>; /* enabled/disabled */
+		};
+	};
+
+	ethernet@1 {
+		compatible = "fsl,pfe-gemac-port";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x1>;	/* GEM_ID */
+		fsl,gemac-bus-id = < 0x1 >;	/* BUS_ID */
+		fsl,gemac-phy-id = < 0x1 >;	/* PHY_ID */
+		fsl,mdio-mux-val = <0x0>;
+		phy-mode = "rgmii-txid";
+		fsl,pfe-phy-if-flags = <0x0>;
+
+		mdio@0 {
+			reg = <0x0>; /* enabled/disabled */
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi
@@ -0,0 +1,567 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Freescale Layerscape-1012A family SoC.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ */
+
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/thermal/thermal.h>
+
+/ {
+	compatible = "fsl,ls1012a";
+	interrupt-parent = <&gic>;
+	#address-cells = <2>;
+	#size-cells = <2>;
+
+	aliases {
+		crypto = &crypto;
+		rtic_a = &rtic_a;
+		rtic_b = &rtic_b;
+		rtic_c = &rtic_c;
+		rtic_d = &rtic_d;
+		sec_mon = &sec_mon;
+	};
+
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x0>;
+			clocks = <&clockgen 1 0>;
+			#cooling-cells = <2>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+	};
+
+	idle-states {
+		/*
+		 * PSCI node is not added default, U-boot will add missing
+		 * parts if it determines to use PSCI.
+		 */
+		entry-method = "arm,psci";
+
+		CPU_PH20: cpu-ph20 {
+			compatible = "arm,idle-state";
+			idle-state-name = "PH20";
+			arm,psci-suspend-param = <0x0>;
+			entry-latency-us = <1000>;
+			exit-latency-us = <1000>;
+			min-residency-us = <3000>;
+		};
+	};
+
+	sysclk: sysclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <125000000>;
+		clock-output-names = "sysclk";
+	};
+
+	coreclk: coreclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <100000000>;
+		clock-output-names = "coreclk";
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <1 13 IRQ_TYPE_LEVEL_LOW>,/* Physical Secure PPI */
+			     <1 14 IRQ_TYPE_LEVEL_LOW>,/* Physical Non-Secure PPI */
+			     <1 11 IRQ_TYPE_LEVEL_LOW>,/* Virtual PPI */
+			     <1 10 IRQ_TYPE_LEVEL_LOW>;/* Hypervisor PPI */
+	};
+
+	pmu {
+		compatible = "arm,armv8-pmuv3";
+		interrupts = <0 106 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	gic: interrupt-controller@1400000 {
+		compatible = "arm,gic-400";
+		#interrupt-cells = <3>;
+		interrupt-controller;
+		reg = <0x0 0x1401000 0 0x1000>, /* GICD */
+		      <0x0 0x1402000 0 0x2000>, /* GICC */
+		      <0x0 0x1404000 0 0x2000>, /* GICH */
+		      <0x0 0x1406000 0 0x2000>; /* GICV */
+		interrupts = <1 9 IRQ_TYPE_LEVEL_LOW>;
+	};
+
+	reboot {
+		compatible = "syscon-reboot";
+		regmap = <&dcfg>;
+		offset = <0xb0>;
+		mask = <0x02>;
+	};
+
+	soc {
+		compatible = "simple-bus";
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		scfg: scfg@1570000 {
+			compatible = "fsl,ls1012a-scfg", "syscon";
+			reg = <0x0 0x1570000 0x0 0x10000>;
+			big-endian;
+		};
+
+		crypto: crypto@1700000 {
+			compatible = "fsl,sec-v5.4", "fsl,sec-v5.0",
+				     "fsl,sec-v4.0";
+			fsl,sec-era = <8>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0x0 0x00 0x1700000 0x100000>;
+			reg = <0x00 0x1700000 0x0 0x100000>;
+			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
+
+			sec_jr0: jr@10000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x10000 0x10000>;
+				interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr1: jr@20000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x20000 0x10000>;
+				interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr2: jr@30000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x30000 0x10000>;
+				interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr3: jr@40000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x40000 0x10000>;
+				interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			caam-dma {
+				compatible = "fsl,sec-v5.4-dma",
+					     "fsl,sec-v5.0-dma",
+					     "fsl,sec-v4.0-dma";
+			};
+
+			rtic@60000 {
+				compatible = "fsl,sec-v5.4-rtic",
+					     "fsl,sec-v5.0-rtic",
+					     "fsl,sec-v4.0-rtic";
+				#address-cells = <1>;
+				#size-cells = <1>;
+				reg = <0x60000 0x100 0x60e00 0x18>;
+				ranges = <0x0 0x60100 0x500>;
+
+				rtic_a: rtic-a@0 {
+					compatible = "fsl,sec-v5.4-rtic-memory",
+						     "fsl,sec-v5.0-rtic-memory",
+						     "fsl,sec-v4.0-rtic-memory";
+					reg = <0x00 0x20 0x100 0x100>;
+				};
+
+				rtic_b: rtic-b@20 {
+					compatible = "fsl,sec-v5.4-rtic-memory",
+						     "fsl,sec-v5.0-rtic-memory",
+						     "fsl,sec-v4.0-rtic-memory";
+					reg = <0x20 0x20 0x200 0x100>;
+				};
+
+				rtic_c: rtic-c@40 {
+					compatible = "fsl,sec-v5.4-rtic-memory",
+						     "fsl,sec-v5.0-rtic-memory",
+						     "fsl,sec-v4.0-rtic-memory";
+					reg = <0x40 0x20 0x300 0x100>;
+				};
+
+				rtic_d: rtic-d@60 {
+					compatible = "fsl,sec-v5.4-rtic-memory",
+						     "fsl,sec-v5.0-rtic-memory",
+						     "fsl,sec-v4.0-rtic-memory";
+					reg = <0x60 0x20 0x400 0x100>;
+				};
+			};
+		};
+
+		sec_mon: sec_mon@1e90000 {
+			compatible = "fsl,sec-v5.4-mon", "fsl,sec-v5.0-mon",
+				     "fsl,sec-v4.0-mon";
+			reg = <0x0 0x1e90000 0x0 0x10000>;
+			interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		dcfg: dcfg@1ee0000 {
+			compatible = "fsl,ls1012a-dcfg",
+				     "syscon";
+			reg = <0x0 0x1ee0000 0x0 0x10000>;
+			big-endian;
+		};
+
+		clockgen: clocking@1ee1000 {
+			compatible = "fsl,ls1012a-clockgen";
+			reg = <0x0 0x1ee1000 0x0 0x1000>;
+			#clock-cells = <2>;
+			clocks = <&sysclk &coreclk>;
+			clock-names = "sysclk", "coreclk";
+		};
+
+		tmu: tmu@1f00000 {
+			compatible = "fsl,qoriq-tmu";
+			reg = <0x0 0x1f00000 0x0 0x10000>;
+			interrupts = <0 33 0x4>;
+			fsl,tmu-range = <0xb0000 0x9002a 0x6004c 0x30062>;
+			fsl,tmu-calibration = <0x00000000 0x00000026
+					       0x00000001 0x0000002d
+					       0x00000002 0x00000032
+					       0x00000003 0x00000039
+					       0x00000004 0x0000003f
+					       0x00000005 0x00000046
+					       0x00000006 0x0000004d
+					       0x00000007 0x00000054
+					       0x00000008 0x0000005a
+					       0x00000009 0x00000061
+					       0x0000000a 0x0000006a
+					       0x0000000b 0x00000071
+
+					       0x00010000 0x00000025
+					       0x00010001 0x0000002c
+					       0x00010002 0x00000035
+					       0x00010003 0x0000003d
+					       0x00010004 0x00000045
+					       0x00010005 0x0000004e
+					       0x00010006 0x00000057
+					       0x00010007 0x00000061
+					       0x00010008 0x0000006b
+					       0x00010009 0x00000076
+
+					       0x00020000 0x00000029
+					       0x00020001 0x00000033
+					       0x00020002 0x0000003d
+					       0x00020003 0x00000049
+					       0x00020004 0x00000056
+					       0x00020005 0x00000061
+					       0x00020006 0x0000006d
+
+					       0x00030000 0x00000021
+					       0x00030001 0x0000002a
+					       0x00030002 0x0000003c
+					       0x00030003 0x0000004e>;
+			big-endian;
+			#thermal-sensor-cells = <1>;
+		};
+
+		thermal-zones {
+			cpu_thermal: cpu-thermal {
+				polling-delay-passive = <1000>;
+				polling-delay = <5000>;
+				thermal-sensors = <&tmu 0>;
+
+				trips {
+					cpu_alert: cpu-alert {
+						temperature = <85000>;
+						hysteresis = <2000>;
+						type = "passive";
+					};
+
+					cpu_crit: cpu-crit {
+						temperature = <95000>;
+						hysteresis = <2000>;
+						type = "critical";
+					};
+				};
+
+				cooling-maps {
+					map0 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu0 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+				};
+			};
+		};
+
+		esdhc0: esdhc@1560000 {
+			compatible = "fsl,ls1012a-esdhc", "fsl,esdhc";
+			reg = <0x0 0x1560000 0x0 0x10000>;
+			interrupts = <0 62 0x4>;
+			clocks = <&clockgen 4 0>;
+			voltage-ranges = <1800 1800 3300 3300>;
+			sdhci,auto-cmd12;
+			big-endian;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		esdhc1: esdhc@1580000 {
+			compatible = "fsl,ls1012a-esdhc", "fsl,esdhc";
+			reg = <0x0 0x1580000 0x0 0x10000>;
+			interrupts = <0 65 0x4>;
+			clocks = <&clockgen 4 0>;
+			voltage-ranges = <1800 1800 3300 3300>;
+			sdhci,auto-cmd12;
+			big-endian;
+			broken-cd;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		rcpm: rcpm@1ee2000 {
+			compatible = "fsl,ls1012a-rcpm", "fsl,qoriq-rcpm-2.1";
+			reg = <0x0 0x1ee2000 0x0 0x1000>;
+			fsl,#rcpm-wakeup-cells = <1>;
+		};
+
+		ftm0: ftm0@29d0000 {
+			compatible = "fsl,ls1012a-ftm";
+			reg = <0x0 0x29d0000 0x0 0x10000>,
+			      <0x0 0x1ee2140 0x0 0x4>;
+			reg-names = "ftm", "FlexTimer1";
+			interrupts = <0 86 0x4>;
+			big-endian;
+		};
+
+		i2c0: i2c@2180000 {
+			compatible = "fsl,vf610-i2c", "fsl,ls1012a-vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2180000 0x0 0x10000>;
+			interrupts = <0 56 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 3>;
+			fsl-scl-gpio = <&gpio0 13 0>;
+			status = "disabled";
+		};
+
+		i2c1: i2c@2190000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2190000 0x0 0x10000>;
+			interrupts = <0 57 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 3>;
+			status = "disabled";
+		};
+
+		duart0: serial@21c0500 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x00 0x21c0500 0x0 0x100>;
+			interrupts = <0 54 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 0>;
+			status = "disabled";
+		};
+
+		duart1: serial@21c0600 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x00 0x21c0600 0x0 0x100>;
+			interrupts = <0 54 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 0>;
+			status = "disabled";
+		};
+
+		gpio0: gpio@2300000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2300000 0x0 0x10000>;
+			interrupts = <0 66 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio1: gpio@2310000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2310000 0x0 0x10000>;
+			interrupts = <0 67 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		qspi: quadspi@1550000 {
+			compatible = "fsl,ls1012a-qspi", "fsl,ls1021a-qspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x1550000 0x0 0x10000>,
+				<0x0 0x40000000 0x0 0x10000000>;
+			reg-names = "QuadSPI", "QuadSPI-memory";
+			interrupts = <0 99 IRQ_TYPE_LEVEL_HIGH>;
+			clock-names = "qspi_en", "qspi";
+			clocks = <&clockgen 4 0>, <&clockgen 4 0>;
+			big-endian;
+			fsl,qspi-has-second-chip;
+			status = "disabled";
+		};
+
+		wdog0: wdog@2ad0000 {
+			compatible = "fsl,ls1012a-wdt",
+				     "fsl,imx21-wdt";
+			reg = <0x0 0x2ad0000 0x0 0x10000>;
+			interrupts = <0 83 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 0>;
+			big-endian;
+		};
+
+		sai1: sai@2b50000 {
+			#sound-dai-cells = <0>;
+			compatible = "fsl,vf610-sai";
+			reg = <0x0 0x2b50000 0x0 0x10000>;
+			interrupts = <0 148 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>,
+				 <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "bus", "mclk1", "mclk2", "mclk3";
+			dma-names = "tx", "rx";
+			dmas = <&edma0 1 47>,
+			       <&edma0 1 46>;
+			status = "disabled";
+		};
+
+		sai2: sai@2b60000 {
+			#sound-dai-cells = <0>;
+			compatible = "fsl,vf610-sai";
+			reg = <0x0 0x2b60000 0x0 0x10000>;
+			interrupts = <0 149 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>,
+				 <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "bus", "mclk1", "mclk2", "mclk3";
+			dma-names = "tx", "rx";
+			dmas = <&edma0 1 45>,
+			       <&edma0 1 44>;
+			status = "disabled";
+		};
+
+		edma0: edma@2c00000 {
+			#dma-cells = <2>;
+			compatible = "fsl,vf610-edma";
+			reg = <0x0 0x2c00000 0x0 0x10000>,
+			      <0x0 0x2c10000 0x0 0x10000>,
+			      <0x0 0x2c20000 0x0 0x10000>;
+			interrupts = <0 103 IRQ_TYPE_LEVEL_HIGH>,
+				     <0 103 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "edma-tx", "edma-err";
+			dma-channels = <32>;
+			big-endian;
+			clock-names = "dmamux0", "dmamux1";
+			clocks = <&clockgen 4 3>,
+				 <&clockgen 4 3>;
+		};
+
+		usb0: usb3@2f00000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x2f00000 0x0 0x10000>;
+			interrupts = <0 60 0x4>;
+			dr_mode = "host";
+			snps,quirk-frame-length-adjustment = <0x20>;
+			snps,dis_rxdet_inp3_quirk;
+		};
+
+		usb1: usb2@8600000 {
+			compatible = "fsl-usb2-dr-v2.5", "fsl-usb2-dr";
+			reg = <0x0 0x8600000 0x0 0x1000>;
+			interrupts = <0 139 0x4>;
+			dr_mode = "host";
+			phy_type = "ulpi";
+		};
+
+		sata: sata@3200000 {
+			compatible = "fsl,ls1012a-ahci", "fsl,ls1043a-ahci";
+			reg = <0x0 0x3200000 0x0 0x10000>,
+				<0x0 0x20140520 0x0 0x4>;
+			reg-names = "ahci", "sata-ecc";
+			interrupts = <0 69 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 0>;
+			dma-coherent;
+			status = "disabled";
+		};
+
+		msi: msi-controller1@1572000 {
+			compatible = "fsl,ls1012a-msi";
+			reg = <0x0 0x1572000 0x0 0x8>;
+			msi-controller;
+			interrupts = <0 126 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pcie: pcie@3400000 {
+			compatible = "fsl,ls1012a-pcie", "snps,dw-pcie";
+			reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
+			       0x40 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <0 118 0x4>, /* AER interrupt */
+				     <0 117 0x4>; /* PME interrupt */
+			interrupt-names = "aer", "pme";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x40 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x40 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&msi>;
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 110 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 2 &gic 0 111 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 3 &gic 0 112 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 4 &gic 0 113 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+		};
+	};
+
+	reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		pfe_reserved: packetbuffer@83400000 {
+			reg = <0 0x83400000 0 0xc00000>;
+		};
+	};
+
+	pfe: pfe@04000000 {
+		compatible = "fsl,pfe";
+		reg =   <0x0 0x04000000 0x0 0xc00000>,	/* AXI 16M */
+			<0x0 0x83400000 0x0 0xc00000>;  /* PFE DDR 12M */
+		reg-names = "pfe", "pfe-ddr";
+		fsl,pfe-num-interfaces = <0x2>;
+		interrupts = <0 172 0x4>,    /* HIF interrupt */
+			     <0 173 0x4>,    /*HIF_NOCPY interrupt */
+			     <0 174 0x4>;    /* WoL interrupt */
+		interrupt-names = "pfe_hif", "pfe_hif_nocpy", "pfe_wol";
+		memory-region = <&pfe_reserved>;
+		fsl,pfe-scfg = <&scfg 0>;
+		fsl,rcpm-wakeup = <&rcpm 0xf0000020>;
+		clocks = <&clockgen 4 0>;
+		clock-names = "pfe";
+
+		status = "okay";
+		pfe_mac0: ethernet@0 {
+		};
+
+		pfe_mac1: ethernet@1 {
+		};
+	};
+
+	firmware {
+		optee {
+			compatible = "linaro,optee-tz";
+			method = "smc";
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043-post.dtsi
@@ -0,0 +1,44 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 device tree nodes for ls1043
+ *
+ * Copyright 2015-2016 Freescale Semiconductor Inc.
+ */
+
+&soc {
+
+/* include used FMan blocks */
+#include "qoriq-fman3-0.dtsi"
+#include "qoriq-fman3-0-1g-0.dtsi"
+#include "qoriq-fman3-0-1g-1.dtsi"
+#include "qoriq-fman3-0-1g-2.dtsi"
+#include "qoriq-fman3-0-1g-3.dtsi"
+#include "qoriq-fman3-0-1g-4.dtsi"
+#include "qoriq-fman3-0-1g-5.dtsi"
+#include "qoriq-fman3-0-10g-0.dtsi"
+
+};
+
+&fman0 {
+	/* these aliases provide the FMan ports mapping */
+	enet0: ethernet@e0000 {
+	};
+
+	enet1: ethernet@e2000 {
+	};
+
+	enet2: ethernet@e4000 {
+	};
+
+	enet3: ethernet@e6000 {
+	};
+
+	enet4: ethernet@e8000 {
+	};
+
+	enet5: ethernet@ea000 {
+	};
+
+	enet6: ethernet@f0000 {
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-qds-sdk.dts
@@ -0,0 +1,71 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1043A family SoC.
+ *
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
+ *
+ * Mingkai Hu <Mingkai.hu@freescale.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "fsl-ls1043a-qds.dts"
+#include "qoriq-qman-portals-sdk.dtsi"
+#include "qoriq-bman-portals-sdk.dtsi"
+
+&bman_fbpr {
+	compatible = "fsl,bman-fbpr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_fqd {
+	compatible = "fsl,qman-fqd";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_pfdr {
+	compatible = "fsl,qman-pfdr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+&soc {
+#include "qoriq-dpaa-eth.dtsi"
+#include "qoriq-fman3-0-6oh.dtsi"
+};
+
+&fman0 {
+	compatible = "fsl,fman", "simple-bus";
+};
--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a-qds.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-qds.dts
@@ -1,51 +1,14 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 /*
  * Device Tree Include file for Freescale Layerscape-1043A family SoC.
  *
- * Copyright 2014-2015, Freescale Semiconductor
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
  *
  * Mingkai Hu <Mingkai.hu@freescale.com>
- *
- * This file is dual-licensed: you can use it either under the terms
- * of the GPLv2 or the X11 license, at your option. Note that this dual
- * licensing only applies to this file, and not this project as a
- * whole.
- *
- *  a) This library is free software; you can redistribute it and/or
- *     modify it under the terms of the GNU General Public License as
- *     published by the Free Software Foundation; either version 2 of the
- *     License, or (at your option) any later version.
- *
- *     This library is distributed in the hope that it will be useful,
- *     but WITHOUT ANY WARRANTY; without even the implied warranty of
- *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- *     GNU General Public License for more details.
- *
- * Or, alternatively,
- *
- *  b) Permission is hereby granted, free of charge, to any person
- *     obtaining a copy of this software and associated documentation
- *     files (the "Software"), to deal in the Software without
- *     restriction, including without limitation the rights to use,
- *     copy, modify, merge, publish, distribute, sublicense, and/or
- *     sell copies of the Software, and to permit persons to whom the
- *     Software is furnished to do so, subject to the following
- *     conditions:
- *
- *     The above copyright notice and this permission notice shall be
- *     included in all copies or substantial portions of the Software.
- *
- *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
- *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
- *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
- *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
- *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
- *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
- *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
- *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
 /dts-v1/;
-/include/ "fsl-ls1043a.dtsi"
+#include "fsl-ls1043a.dtsi"
 
 / {
 	model = "LS1043A QDS Board";
@@ -60,6 +23,22 @@
 		serial1 = &duart1;
 		serial2 = &duart2;
 		serial3 = &duart3;
+		sgmii_riser_s1_p1 = &sgmii_phy_s1_p1;
+		sgmii_riser_s2_p1 = &sgmii_phy_s2_p1;
+		sgmii_riser_s3_p1 = &sgmii_phy_s3_p1;
+		sgmii_riser_s4_p1 = &sgmii_phy_s4_p1;
+		qsgmii_s1_p1 = &qsgmii_phy_s1_p1;
+		qsgmii_s1_p2 = &qsgmii_phy_s1_p2;
+		qsgmii_s1_p3 = &qsgmii_phy_s1_p3;
+		qsgmii_s1_p4 = &qsgmii_phy_s1_p4;
+		qsgmii_s2_p1 = &qsgmii_phy_s2_p1;
+		qsgmii_s2_p2 = &qsgmii_phy_s2_p2;
+		qsgmii_s2_p3 = &qsgmii_phy_s2_p3;
+		qsgmii_s2_p4 = &qsgmii_phy_s2_p4;
+		emi1_slot1 = &ls1043mdio_s1;
+		emi1_slot2 = &ls1043mdio_s2;
+		emi1_slot3 = &ls1043mdio_s3;
+		emi1_slot4 = &ls1043mdio_s4;
 	};
 
 	chosen {
@@ -97,8 +76,11 @@
 	};
 
 	fpga: board-control@2,0 {
-		compatible = "fsl,ls1043aqds-fpga", "fsl,fpga-qixis";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "fsl,ls1043aqds-fpga", "fsl,fpga-qixis", "simple-bus";
 		reg = <0x2 0x0 0x0000100>;
+		ranges = <0 2 0 0x100>;
 	};
 };
 
@@ -181,3 +163,149 @@
 		reg = <0>;
 	};
 };
+
+#include "fsl-ls1043-post.dtsi"
+
+&fman0 {
+	ethernet@e0000 {
+		phy-handle = <&qsgmii_phy_s2_p1>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@e2000 {
+		phy-handle = <&qsgmii_phy_s2_p2>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@e4000 {
+		phy-handle = <&rgmii_phy1>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e6000 {
+		phy-handle = <&rgmii_phy2>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e8000 {
+		phy-handle = <&qsgmii_phy_s2_p3>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@ea000 {
+		phy-handle = <&qsgmii_phy_s2_p4>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@f0000 { /* DTSEC9/10GEC1 */
+		fixed-link = <1 1 10000 0 0>;
+		phy-connection-type = "xgmii";
+	};
+};
+
+&fpga {
+	mdio-mux-emi1 {
+		compatible = "mdio-mux-mmioreg", "mdio-mux";
+		mdio-parent-bus = <&mdio0>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x54 1>;    /* BRDCFG4 */
+		mux-mask = <0xe0>; /* EMI1 */
+
+		/* On-board RGMII1 PHY */
+		ls1043mdio0: mdio@0 {
+			reg = <0>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rgmii_phy1: ethernet-phy@1 { /* MAC3 */
+				reg = <0x1>;
+			};
+		};
+
+		/* On-board RGMII2 PHY */
+		ls1043mdio1: mdio@1 {
+			reg = <0x20>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rgmii_phy2: ethernet-phy@2 { /* MAC4 */
+				reg = <0x2>;
+			};
+		};
+
+		/* Slot 1 */
+		ls1043mdio_s1: mdio@2 {
+			reg = <0x40>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			qsgmii_phy_s1_p1: ethernet-phy@4 {
+				reg = <0x4>;
+			};
+			qsgmii_phy_s1_p2: ethernet-phy@5 {
+				reg = <0x5>;
+			};
+			qsgmii_phy_s1_p3: ethernet-phy@6 {
+				reg = <0x6>;
+			};
+			qsgmii_phy_s1_p4: ethernet-phy@7 {
+				reg = <0x7>;
+			};
+
+			sgmii_phy_s1_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+
+		/* Slot 2 */
+		ls1043mdio_s2: mdio@3 {
+			reg = <0x60>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			qsgmii_phy_s2_p1: ethernet-phy@8 {
+				reg = <0x8>;
+			};
+			qsgmii_phy_s2_p2: ethernet-phy@9 {
+				reg = <0x9>;
+			};
+			qsgmii_phy_s2_p3: ethernet-phy@a {
+				reg = <0xa>;
+			};
+			qsgmii_phy_s2_p4: ethernet-phy@b {
+				reg = <0xb>;
+			};
+
+			sgmii_phy_s2_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+
+		/* Slot 3 */
+		ls1043mdio_s3: mdio@4 {
+			reg = <0x80>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			sgmii_phy_s3_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+
+		/* Slot 4 */
+		ls1043mdio_s4: mdio@5 {
+			reg = <0xa0>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			sgmii_phy_s4_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb-sdk.dts
@@ -0,0 +1,71 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1043A family SoC.
+ *
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
+ *
+ * Mingkai Hu <Mingkai.hu@freescale.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "fsl-ls1043a-rdb.dts"
+#include "qoriq-qman-portals-sdk.dtsi"
+#include "qoriq-bman-portals-sdk.dtsi"
+
+&bman_fbpr {
+	compatible = "fsl,bman-fbpr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_fqd {
+	compatible = "fsl,qman-fqd";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_pfdr {
+	compatible = "fsl,qman-pfdr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+&soc {
+#include "qoriq-dpaa-eth.dtsi"
+#include "qoriq-fman3-0-6oh.dtsi"
+};
+
+&fman0 {
+	compatible = "fsl,fman", "simple-bus";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb-usdpaa.dts
@@ -0,0 +1,117 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1043A family SoC.
+ *
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
+ *
+ * This file is licensed under the terms of the GNU General Public
+ * License version 2.  This program is licensed "as is" without any
+ * warranty of any kind, whether express or implied.
+ */
+
+#include "fsl-ls1043a-rdb-sdk.dts"
+
+&soc {
+	bp7: buffer-pool@7 {
+		compatible = "fsl,p4080-bpool", "fsl,bpool";
+		fsl,bpid = <7>;
+		fsl,bpool-ethernet-cfg = <0 0 0 192 0 0xdeadbeef>;
+		fsl,bpool-thresholds = <0x400 0xc00 0x0 0x0>;
+	};
+
+	bp8: buffer-pool@8 {
+		compatible = "fsl,p4080-bpool", "fsl,bpool";
+		fsl,bpid = <8>;
+		fsl,bpool-ethernet-cfg = <0 0 0 576 0 0xabbaf00d>;
+		fsl,bpool-thresholds = <0x100 0x300 0x0 0x0>;
+	};
+
+	bp9: buffer-pool@9 {
+		compatible = "fsl,p4080-bpool", "fsl,bpool";
+		fsl,bpid = <9>;
+		fsl,bpool-ethernet-cfg = <0 0 0 2048 0 0xfeedabba>;
+		fsl,bpool-thresholds = <0x100 0x300 0x0 0x0>;
+	};
+
+	fsl,dpaa {
+		compatible = "fsl,ls1043a", "fsl,dpaa", "simple-bus";
+
+		ethernet@0 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x50 1 0x51 1>;
+			fsl,qman-frame-queues-tx = <0x70 1 0x71 1>;
+		};
+
+		ethernet@1 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x52 1 0x53 1>;
+			fsl,qman-frame-queues-tx = <0x72 1 0x73 1>;
+		};
+
+		ethernet@2 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x54 1 0x55 1>;
+			fsl,qman-frame-queues-tx = <0x74 1 0x75 1>;
+		};
+
+		ethernet@3 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x56 1 0x57 1>;
+			fsl,qman-frame-queues-tx = <0x76 1 0x77 1>;
+		};
+
+		ethernet@4 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x58 1 0x59 1>;
+			fsl,qman-frame-queues-tx = <0x78 1 0x79 1>;
+		};
+
+		ethernet@5 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x60 1 0x61 1>;
+			fsl,qman-frame-queues-tx = <0x80 1 0x81 1>;
+		};
+
+		ethernet@8 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x5c 1 0x5d 1>;
+			fsl,qman-frame-queues-tx = <0x7c 1 0x7d 1>;
+
+		};
+		dpa-fman0-oh@2 {
+			compatible = "fsl,dpa-oh";
+			/* Define frame queues for the OH port*/
+			/* <OH Rx error, OH Rx default> */
+			fsl,qman-frame-queues-oh = <0x5a 1 0x5b 1>;
+			fsl,fman-oh-port = <&fman0_oh2>;
+		};
+	};
+};
+/ {
+	reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		usdpaa_mem: usdpaa_mem {
+			compatible = "fsl,usdpaa-mem";
+			alloc-ranges = <0 0 0x10000 0>;
+			size = <0 0x10000000>;
+			alignment = <0 0x10000000>;
+		};
+	};
+};
+
+&fman0 {
+	fman0_oh2: port@83000 {
+		cell-index = <1>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x83000 0x1000>;
+	};
+};
--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
@@ -1,51 +1,14 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 /*
  * Device Tree Include file for Freescale Layerscape-1043A family SoC.
  *
- * Copyright 2014-2015, Freescale Semiconductor
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
  *
  * Mingkai Hu <Mingkai.hu@freescale.com>
- *
- * This file is dual-licensed: you can use it either under the terms
- * of the GPLv2 or the X11 license, at your option. Note that this dual
- * licensing only applies to this file, and not this project as a
- * whole.
- *
- *  a) This library is free software; you can redistribute it and/or
- *     modify it under the terms of the GNU General Public License as
- *     published by the Free Software Foundation; either version 2 of the
- *     License, or (at your option) any later version.
- *
- *     This library is distributed in the hope that it will be useful,
- *     but WITHOUT ANY WARRANTY; without even the implied warranty of
- *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- *     GNU General Public License for more details.
- *
- * Or, alternatively,
- *
- *  b) Permission is hereby granted, free of charge, to any person
- *     obtaining a copy of this software and associated documentation
- *     files (the "Software"), to deal in the Software without
- *     restriction, including without limitation the rights to use,
- *     copy, modify, merge, publish, distribute, sublicense, and/or
- *     sell copies of the Software, and to permit persons to whom the
- *     Software is furnished to do so, subject to the following
- *     conditions:
- *
- *     The above copyright notice and this permission notice shall be
- *     included in all copies or substantial portions of the Software.
- *
- *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
- *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
- *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
- *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
- *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
- *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
- *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
- *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
 /dts-v1/;
-/include/ "fsl-ls1043a.dtsi"
+#include "fsl-ls1043a.dtsi"
 
 / {
 	model = "LS1043A RDB Board";
@@ -86,6 +49,10 @@
 		compatible = "pericom,pt7c4338";
 		reg = <0x68>;
 	};
+	rtc@51 {
+		compatible = "nxp,pcf85263";
+		reg = <0x51>;
+	};
 };
 
 &ifc {
@@ -130,6 +97,38 @@
 		reg = <0>;
 		spi-max-frequency = <1000000>; /* input clock */
 	};
+
+	slic@2 {
+		compatible = "maxim,ds26522";
+		reg = <2>;
+		spi-max-frequency = <2000000>;
+		fsl,spi-cs-sck-delay = <100>;
+		fsl,spi-sck-cs-delay = <50>;
+	};
+
+	slic@3 {
+		compatible = "maxim,ds26522";
+		reg = <3>;
+		spi-max-frequency = <2000000>;
+		fsl,spi-cs-sck-delay = <100>;
+		fsl,spi-sck-cs-delay = <50>;
+	};
+};
+
+&uqe {
+	ucc_hdlc: ucc@2000 {
+		compatible = "fsl,ucc-hdlc";
+		rx-clock-name = "clk8";
+		tx-clock-name = "clk9";
+		fsl,rx-sync-clock = "rsync_pin";
+		fsl,tx-sync-clock = "tsync_pin";
+		fsl,tx-timeslot-mask = <0xfffffffe>;
+		fsl,rx-timeslot-mask = <0xfffffffe>;
+		fsl,tdm-framer-type = "e1";
+		fsl,tdm-id = <0>;
+		fsl,siram-entry-id = <0>;
+		fsl,tdm-interface;
+	};
 };
 
 &duart0 {
@@ -139,3 +138,76 @@
 &duart1 {
 	status = "okay";
 };
+
+#include "fsl-ls1043-post.dtsi"
+
+&fman0 {
+	ethernet@e0000 {
+		phy-handle = <&qsgmii_phy1>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@e2000 {
+		phy-handle = <&qsgmii_phy2>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@e4000 {
+		phy-handle = <&rgmii_phy1>;
+		phy-connection-type = "rgmii-txid";
+	};
+
+	ethernet@e6000 {
+		phy-handle = <&rgmii_phy2>;
+		phy-connection-type = "rgmii-txid";
+	};
+
+	ethernet@e8000 {
+		phy-handle = <&qsgmii_phy3>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@ea000 {
+		phy-handle = <&qsgmii_phy4>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@f0000 { /* 10GEC1 */
+		phy-handle = <&aqr105_phy>;
+		phy-connection-type = "xgmii";
+	};
+
+	mdio@fc000 {
+		rgmii_phy1: ethernet-phy@1 {
+			reg = <0x1>;
+		};
+
+		rgmii_phy2: ethernet-phy@2 {
+			reg = <0x2>;
+		};
+
+		qsgmii_phy1: ethernet-phy@4 {
+			reg = <0x4>;
+		};
+
+		qsgmii_phy2: ethernet-phy@5 {
+			reg = <0x5>;
+		};
+
+		qsgmii_phy3: ethernet-phy@6 {
+			reg = <0x6>;
+		};
+
+		qsgmii_phy4: ethernet-phy@7 {
+			reg = <0x7>;
+		};
+	};
+
+	mdio@fd000 {
+		aqr105_phy: ethernet-phy@1 {
+			compatible = "ethernet-phy-ieee802.3-c45";
+			interrupts = <0 132 4>;
+			reg = <0x1>;
+		};
+	};
+};
--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -1,55 +1,32 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 /*
  * Device Tree Include file for Freescale Layerscape-1043A family SoC.
  *
- * Copyright 2014-2015, Freescale Semiconductor
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
  *
  * Mingkai Hu <Mingkai.hu@freescale.com>
- *
- * This file is dual-licensed: you can use it either under the terms
- * of the GPLv2 or the X11 license, at your option. Note that this dual
- * licensing only applies to this file, and not this project as a
- * whole.
- *
- *  a) This library is free software; you can redistribute it and/or
- *     modify it under the terms of the GNU General Public License as
- *     published by the Free Software Foundation; either version 2 of the
- *     License, or (at your option) any later version.
- *
- *     This library is distributed in the hope that it will be useful,
- *     but WITHOUT ANY WARRANTY; without even the implied warranty of
- *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- *     GNU General Public License for more details.
- *
- * Or, alternatively,
- *
- *  b) Permission is hereby granted, free of charge, to any person
- *     obtaining a copy of this software and associated documentation
- *     files (the "Software"), to deal in the Software without
- *     restriction, including without limitation the rights to use,
- *     copy, modify, merge, publish, distribute, sublicense, and/or
- *     sell copies of the Software, and to permit persons to whom the
- *     Software is furnished to do so, subject to the following
- *     conditions:
- *
- *     The above copyright notice and this permission notice shall be
- *     included in all copies or substantial portions of the Software.
- *
- *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
- *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
- *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
- *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
- *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
- *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
- *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
- *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
+#include <dt-bindings/thermal/thermal.h>
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+
 / {
 	compatible = "fsl,ls1043a";
 	interrupt-parent = <&gic>;
 	#address-cells = <2>;
 	#size-cells = <2>;
 
+	aliases {
+		fman0 = &fman0;
+		ethernet0 = &enet0;
+		ethernet1 = &enet1;
+		ethernet2 = &enet2;
+		ethernet3 = &enet3;
+		ethernet4 = &enet4;
+		ethernet5 = &enet5;
+		ethernet6 = &enet6;
+	};
+
 	cpus {
 		#address-cells = <1>;
 		#size-cells = <0>;
@@ -66,6 +43,8 @@
 			reg = <0x0>;
 			clocks = <&clockgen 1 0>;
 			next-level-cache = <&l2>;
+			#cooling-cells = <2>;
+			cpu-idle-states = <&CPU_PH20>;
 		};
 
 		cpu1: cpu@1 {
@@ -74,6 +53,7 @@
 			reg = <0x1>;
 			clocks = <&clockgen 1 0>;
 			next-level-cache = <&l2>;
+			cpu-idle-states = <&CPU_PH20>;
 		};
 
 		cpu2: cpu@2 {
@@ -82,6 +62,7 @@
 			reg = <0x2>;
 			clocks = <&clockgen 1 0>;
 			next-level-cache = <&l2>;
+			cpu-idle-states = <&CPU_PH20>;
 		};
 
 		cpu3: cpu@3 {
@@ -90,6 +71,7 @@
 			reg = <0x3>;
 			clocks = <&clockgen 1 0>;
 			next-level-cache = <&l2>;
+			cpu-idle-states = <&CPU_PH20>;
 		};
 
 		l2: l2-cache {
@@ -97,12 +79,56 @@
 		};
 	};
 
+	idle-states {
+		/*
+		 * PSCI node is not added default, U-boot will add missing
+		 * parts if it determines to use PSCI.
+		 */
+		entry-method = "arm,psci";
+
+		CPU_PH20: cpu-ph20 {
+			compatible = "arm,idle-state";
+			idle-state-name = "PH20";
+			arm,psci-suspend-param = <0x0>;
+			entry-latency-us = <1000>;
+			exit-latency-us = <1000>;
+			min-residency-us = <3000>;
+		};
+	};
+
 	memory@80000000 {
 		device_type = "memory";
 		reg = <0x0 0x80000000 0 0x80000000>;
 		      /* DRAM space 1, size: 2GiB DRAM */
 	};
 
+	reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		bman_fbpr: bman-fbpr {
+			compatible = "shared-dma-pool";
+			size = <0 0x1000000>;
+			alignment = <0 0x1000000>;
+			no-map;
+		};
+
+		qman_fqd: qman-fqd {
+			compatible = "shared-dma-pool";
+			size = <0 0x400000>;
+			alignment = <0 0x400000>;
+			no-map;
+		};
+
+		qman_pfdr: qman-pfdr {
+			compatible = "shared-dma-pool";
+			size = <0 0x2000000>;
+			alignment = <0 0x2000000>;
+			no-map;
+		};
+	};
+
 	sysclk: sysclk {
 		compatible = "fixed-clock";
 		#clock-cells = <0>;
@@ -149,7 +175,7 @@
 		interrupts = <1 9 0xf08>;
 	};
 
-	soc {
+	soc: soc {
 		compatible = "simple-bus";
 		#address-cells = <2>;
 		#size-cells = <2>;
@@ -213,13 +239,14 @@
 
 		dcfg: dcfg@1ee0000 {
 			compatible = "fsl,ls1043a-dcfg", "syscon";
-			reg = <0x0 0x1ee0000 0x0 0x10000>;
+			reg = <0x0 0x1ee0000 0x0 0x1000>;
 			big-endian;
 		};
 
 		ifc: ifc@1530000 {
 			compatible = "fsl,ifc", "simple-bus";
 			reg = <0x0 0x1530000 0x0 0x10000>;
+			big-endian;
 			interrupts = <0 43 0x4>;
 		};
 
@@ -255,6 +282,103 @@
 			big-endian;
 		};
 
+		tmu: tmu@1f00000 {
+			compatible = "fsl,qoriq-tmu";
+			reg = <0x0 0x1f00000 0x0 0x10000>;
+			interrupts = <0 33 0x4>;
+			fsl,tmu-range = <0xb0000 0x9002a 0x6004c 0x30062>;
+			fsl,tmu-calibration = <0x00000000 0x00000026
+					       0x00000001 0x0000002d
+					       0x00000002 0x00000032
+					       0x00000003 0x00000039
+					       0x00000004 0x0000003f
+					       0x00000005 0x00000046
+					       0x00000006 0x0000004d
+					       0x00000007 0x00000054
+					       0x00000008 0x0000005a
+					       0x00000009 0x00000061
+					       0x0000000a 0x0000006a
+					       0x0000000b 0x00000071
+
+					       0x00010000 0x00000025
+					       0x00010001 0x0000002c
+					       0x00010002 0x00000035
+					       0x00010003 0x0000003d
+					       0x00010004 0x00000045
+					       0x00010005 0x0000004e
+					       0x00010006 0x00000057
+					       0x00010007 0x00000061
+					       0x00010008 0x0000006b
+					       0x00010009 0x00000076
+
+					       0x00020000 0x00000029
+					       0x00020001 0x00000033
+					       0x00020002 0x0000003d
+					       0x00020003 0x00000049
+					       0x00020004 0x00000056
+					       0x00020005 0x00000061
+					       0x00020006 0x0000006d
+
+					       0x00030000 0x00000021
+					       0x00030001 0x0000002a
+					       0x00030002 0x0000003c
+					       0x00030003 0x0000004e>;
+			#thermal-sensor-cells = <1>;
+		};
+
+		thermal-zones {
+			cpu_thermal: cpu-thermal {
+				polling-delay-passive = <1000>;
+				polling-delay = <5000>;
+
+				thermal-sensors = <&tmu 3>;
+
+				trips {
+					cpu_alert: cpu-alert {
+						temperature = <85000>;
+						hysteresis = <2000>;
+						type = "passive";
+					};
+					cpu_crit: cpu-crit {
+						temperature = <95000>;
+						hysteresis = <2000>;
+						type = "critical";
+					};
+				};
+
+				cooling-maps {
+					map0 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu0 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+				};
+			};
+		};
+
+		qman: qman@1880000 {
+			compatible = "fsl,qman";
+			reg = <0x00 0x1880000 0x0 0x10000>;
+			interrupts = <0 45 0x4>;
+			memory-region = <&qman_fqd &qman_pfdr>;
+		};
+
+		bman: bman@1890000 {
+			compatible = "fsl,bman";
+			reg = <0x00 0x1890000 0x0 0x10000>;
+			interrupts = <0 45 0x4>;
+			memory-region = <&bman_fbpr>;
+		};
+
+		bportals: bman-portals@508000000 {
+			ranges = <0x0 0x5 0x08000000 0x8000000>;
+		};
+
+		qportals: qman-portals@500000000 {
+			ranges = <0x0 0x5 0x00000000 0x8000000>;
+		};
+
 		dspi0: dspi@2100000 {
 			compatible = "fsl,ls1043a-dspi", "fsl,ls1021a-v1.0-dspi";
 			#address-cells = <1>;
@@ -282,7 +406,7 @@
 		};
 
 		i2c0: i2c@2180000 {
-			compatible = "fsl,vf610-i2c";
+			compatible = "fsl,vf610-i2c", "fsl,ls1043a-vf610-i2c";
 			#address-cells = <1>;
 			#size-cells = <0>;
 			reg = <0x0 0x2180000 0x0 0x10000>;
@@ -292,6 +416,7 @@
 			dmas = <&edma0 1 39>,
 			       <&edma0 1 38>;
 			dma-names = "tx", "rx";
+			fsl-scl-gpio = <&gpio4 12 0>;
 			status = "disabled";
 		};
 
@@ -396,6 +521,72 @@
 			#interrupt-cells = <2>;
 		};
 
+		uqe: uqe@2400000 {
+			#address-cells = <1>;
+			#size-cells = <1>;
+			device_type = "qe";
+			compatible = "fsl,qe", "simple-bus";
+			ranges = <0x0 0x0 0x2400000 0x40000>;
+			reg = <0x0 0x2400000 0x0 0x480>;
+			brg-frequency = <100000000>;
+			bus-frequency = <200000000>;
+
+			fsl,qe-num-riscs = <1>;
+			fsl,qe-num-snums = <28>;
+
+			qeic: qeic@80 {
+				compatible = "fsl,qe-ic";
+				reg = <0x80 0x80>;
+				#address-cells = <0>;
+				interrupt-controller;
+				#interrupt-cells = <1>;
+				interrupts = <0 77 0x04 0 77 0x04>;
+			};
+
+			si1: si@700 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,ls1043-qe-si",
+						"fsl,t1040-qe-si";
+				reg = <0x700 0x80>;
+			};
+
+			siram1: siram@1000 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "fsl,ls1043-qe-siram",
+						"fsl,t1040-qe-siram";
+				reg = <0x1000 0x800>;
+			};
+
+			ucc@2000 {
+				cell-index = <1>;
+				reg = <0x2000 0x200>;
+				interrupts = <32>;
+				interrupt-parent = <&qeic>;
+			};
+
+			ucc@2200 {
+				cell-index = <3>;
+				reg = <0x2200 0x200>;
+				interrupts = <34>;
+				interrupt-parent = <&qeic>;
+			};
+
+			muram@10000 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "fsl,qe-muram", "fsl,cpm-muram";
+				ranges = <0x0 0x10000 0x6000>;
+
+				data-only@0 {
+					compatible = "fsl,qe-muram-data",
+					"fsl,cpm-muram-data";
+					reg = <0x0 0x6000>;
+				};
+			};
+		};
+
 		lpuart0: serial@2950000 {
 			compatible = "fsl,ls1021a-lpuart";
 			reg = <0x0 0x2950000 0x0 0x1000>;
@@ -450,6 +641,16 @@
 			status = "disabled";
 		};
 
+		ftm0: ftm0@29d0000 {
+			compatible = "fsl,ls1043a-ftm";
+			reg = <0x0 0x29d0000 0x0 0x10000>,
+			      <0x0 0x1ee2140 0x0 0x4>;
+			reg-names = "ftm", "FlexTimer1";
+			interrupts = <0 86 0x4>;
+			big-endian;
+			status = "okay";
+		};
+
 		wdog0: wdog@2ad0000 {
 			compatible = "fsl,ls1043a-wdt", "fsl,imx21-wdt";
 			reg = <0x0 0x2ad0000 0x0 0x10000>;
@@ -482,6 +683,10 @@
 			dr_mode = "host";
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
+			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,dma-snooping;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
 		};
 
 		usb1: usb3@3000000 {
@@ -491,6 +696,11 @@
 			dr_mode = "host";
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
+			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,dma-snooping;
+			configure-gfladj;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
 		};
 
 		usb2: usb3@3100000 {
@@ -500,32 +710,54 @@
 			dr_mode = "host";
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
+			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,dma-snooping;
+			configure-gfladj;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
 		};
 
 		sata: sata@3200000 {
 			compatible = "fsl,ls1043a-ahci";
-			reg = <0x0 0x3200000 0x0 0x10000>;
+			reg = <0x0 0x3200000 0x0 0x10000>,
+				<0x0 0x20140520 0x0 0x4>;
+			reg-names = "ahci", "sata-ecc";
 			interrupts = <0 69 0x4>;
 			clocks = <&clockgen 4 0>;
 			dma-coherent;
 		};
 
+		qdma: qdma@8380000 {
+			compatible = "fsl,ls1021a-qdma", "fsl,ls1043a-qdma";
+			reg = <0x0 0x8380000 0x0 0x1000>, /* Controller regs */
+			      <0x0 0x8390000 0x0 0x10000>, /* Status regs */
+			      <0x0 0x83a0000 0x0 0x40000>; /* Block regs */
+			interrupts = <0 152 0x4>,
+				     <0 39 0x4>;
+			interrupt-names = "qdma-error", "qdma-queue";
+			channels = <8>;
+			queues = <2>;
+			status-sizes = <64>;
+			queue-sizes = <64 64>;
+			big-endian;
+		};
+
 		msi1: msi-controller1@1571000 {
-			compatible = "fsl,1s1043a-msi";
+			compatible = "fsl,ls1043a-msi";
 			reg = <0x0 0x1571000 0x0 0x8>;
 			msi-controller;
 			interrupts = <0 116 0x4>;
 		};
 
 		msi2: msi-controller2@1572000 {
-			compatible = "fsl,1s1043a-msi";
+			compatible = "fsl,ls1043a-msi";
 			reg = <0x0 0x1572000 0x0 0x8>;
 			msi-controller;
 			interrupts = <0 126 0x4>;
 		};
 
 		msi3: msi-controller3@1573000 {
-			compatible = "fsl,1s1043a-msi";
+			compatible = "fsl,ls1043a-msi";
 			reg = <0x0 0x1573000 0x0 0x8>;
 			msi-controller;
 			interrupts = <0 160 0x4>;
@@ -536,9 +768,9 @@
 			reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
 			       0x40 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <0 118 0x4>, /* controller interrupt */
-				     <0 117 0x4>; /* PME interrupt */
-			interrupt-names = "intr", "pme";
+			interrupts = <0 117 0x4>, /* PME interrupt */
+				     <0 118 0x4>; /* aer interrupt */
+			interrupt-names = "pme", "aer";
 			#address-cells = <3>;
 			#size-cells = <2>;
 			device_type = "pci";
@@ -547,7 +779,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x40 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x40 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi1>;
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic 0 110 0x4>,
@@ -561,9 +793,9 @@
 			reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
 			       0x48 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <0 128 0x4>,
-				     <0 127 0x4>;
-			interrupt-names = "intr", "pme";
+			interrupts = <0 127 0x4>,
+				     <0 128 0x4>;
+			interrupt-names = "pme", "aer";
 			#address-cells = <3>;
 			#size-cells = <2>;
 			device_type = "pci";
@@ -572,7 +804,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x48 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x48 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi2>;
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic 0 120  0x4>,
@@ -586,9 +818,9 @@
 			reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
 			       0x50 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <0 162 0x4>,
-				     <0 161 0x4>;
-			interrupt-names = "intr", "pme";
+			interrupts = <0 161 0x4>,
+				     <0 162 0x4>;
+			interrupt-names = "pme", "aer";
 			#address-cells = <3>;
 			#size-cells = <2>;
 			device_type = "pci";
@@ -597,7 +829,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x50 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x50 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi3>;
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic 0 154 0x4>,
@@ -607,4 +839,13 @@
 		};
 	};
 
+	firmware {
+		optee {
+			compatible = "linaro,optee-tz";
+			method = "smc";
+		};
+	};
 };
+
+#include "qoriq-qman-portals.dtsi"
+#include "qoriq-bman-portals.dtsi"
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046-post.dtsi
@@ -0,0 +1,48 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 device tree nodes for ls1046
+ *
+ * Copyright 2015-2016 Freescale Semiconductor Inc.
+ *
+ */
+
+&soc {
+
+/* include used FMan blocks */
+#include "qoriq-fman3-0.dtsi"
+#include "qoriq-fman3-0-1g-0.dtsi"
+#include "qoriq-fman3-0-1g-1.dtsi"
+#include "qoriq-fman3-0-1g-2.dtsi"
+#include "qoriq-fman3-0-1g-3.dtsi"
+#include "qoriq-fman3-0-1g-4.dtsi"
+#include "qoriq-fman3-0-1g-5.dtsi"
+#include "qoriq-fman3-0-10g-0.dtsi"
+#include "qoriq-fman3-0-10g-1.dtsi"
+};
+
+&fman0 {
+	/* these aliases provide the FMan ports mapping */
+	enet0: ethernet@e0000 {
+	};
+
+	enet1: ethernet@e2000 {
+	};
+
+	enet2: ethernet@e4000 {
+	};
+
+	enet3: ethernet@e6000 {
+	};
+
+	enet4: ethernet@e8000 {
+	};
+
+	enet5: ethernet@ea000 {
+	};
+
+	enet6: ethernet@f0000 {
+	};
+
+	enet7: ethernet@f2000 {
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a-qds-sdk.dts
@@ -0,0 +1,112 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1046A family SoC.
+ *
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
+ *
+ * Mingkai Hu <Mingkai.hu@freescale.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "fsl-ls1046a-qds.dts"
+#include "qoriq-qman-portals-sdk.dtsi"
+#include "qoriq-bman-portals-sdk.dtsi"
+
+&bman_fbpr {
+	compatible = "fsl,bman-fbpr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_fqd {
+	compatible = "fsl,qman-fqd";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_pfdr {
+	compatible = "fsl,qman-pfdr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+&soc {
+#include "qoriq-dpaa-eth.dtsi"
+#include "qoriq-fman3-0-6oh.dtsi"
+};
+
+&fsldpaa {
+	ethernet@9 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet7>;
+		dma-coherent;
+	};
+};
+
+&fman0 {
+	compatible = "fsl,fman", "simple-bus";
+};
+
+&dspi {
+	bus-num = <0>;
+	status = "okay";
+
+	flash@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "n25q128a11", "jedec,spi-nor";
+		reg = <0>;
+		spi-max-frequency = <10000000>;
+	};
+
+	flash@1 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "sst25wf040b", "jedec,spi-nor";
+		spi-cpol;
+		spi-cpha;
+		reg = <1>;
+		spi-max-frequency = <10000000>;
+	};
+
+	flash@2 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "en25s64", "jedec,spi-nor";
+		spi-cpol;
+		spi-cpha;
+		reg = <2>;
+		spi-max-frequency = <10000000>;
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a-qds.dts
@@ -0,0 +1,326 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Freescale Layerscape-1046A family SoC.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ * Shaohui Xie <Shaohui.Xie@nxp.com>
+ */
+
+/dts-v1/;
+
+#include "fsl-ls1046a.dtsi"
+
+/ {
+	model = "LS1046A QDS Board";
+	compatible = "fsl,ls1046a-qds", "fsl,ls1046a";
+
+	aliases {
+		gpio0 = &gpio0;
+		gpio1 = &gpio1;
+		gpio2 = &gpio2;
+		gpio3 = &gpio3;
+		serial0 = &duart0;
+		serial1 = &duart1;
+		serial2 = &duart2;
+		serial3 = &duart3;
+
+		emi1_slot1 = &ls1046mdio_s1;
+		emi1_slot2 = &ls1046mdio_s2;
+		emi1_slot4 = &ls1046mdio_s4;
+
+		sgmii_s1_p1 = &sgmii_phy_s1_p1;
+		sgmii_s1_p2 = &sgmii_phy_s1_p2;
+		sgmii_s1_p3 = &sgmii_phy_s1_p3;
+		sgmii_s1_p4 = &sgmii_phy_s1_p4;
+		sgmii_s4_p1 = &sgmii_phy_s4_p1;
+		qsgmii_s2_p1 = &qsgmii_phy_s2_p1;
+		qsgmii_s2_p2 = &qsgmii_phy_s2_p2;
+		qsgmii_s2_p3 = &qsgmii_phy_s2_p3;
+		qsgmii_s2_p4 = &qsgmii_phy_s2_p4;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+};
+
+&dspi {
+	bus-num = <0>;
+	status = "okay";
+
+	flash@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "n25q128a11", "jedec,spi-nor";
+		reg = <0>;
+		spi-max-frequency = <10000000>;
+	};
+
+	flash@1 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "sst25wf040b", "jedec,spi-nor";
+		spi-cpol;
+		spi-cpha;
+		reg = <1>;
+		spi-max-frequency = <10000000>;
+	};
+
+	flash@2 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "en25s64", "jedec,spi-nor";
+		spi-cpol;
+		spi-cpha;
+		reg = <2>;
+		spi-max-frequency = <10000000>;
+	};
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&duart1 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+
+	pca9547@77 {
+		compatible = "nxp,pca9547";
+		reg = <0x77>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		i2c@2 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x2>;
+
+			ina220@40 {
+				compatible = "ti,ina220";
+				reg = <0x40>;
+				shunt-resistor = <1000>;
+			};
+
+			ina220@41 {
+				compatible = "ti,ina220";
+				reg = <0x41>;
+				shunt-resistor = <1000>;
+			};
+		};
+
+		i2c@3 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x3>;
+
+			rtc@51 {
+				compatible = "nxp,pcf2129";
+				reg = <0x51>;
+				/* IRQ10_B */
+				interrupts = <0 150 0x4>;
+			};
+
+			eeprom@56 {
+				compatible = "atmel,24c512";
+				reg = <0x56>;
+			};
+
+			eeprom@57 {
+				compatible = "atmel,24c512";
+				reg = <0x57>;
+			};
+
+			temp-sensor@4c {
+				compatible = "adi,adt7461a";
+				reg = <0x4c>;
+			};
+		};
+	};
+};
+
+&ifc {
+	#address-cells = <2>;
+	#size-cells = <1>;
+	/* NOR, NAND Flashes and FPGA on board */
+	ranges = <0x0 0x0 0x0 0x60000000 0x08000000
+		  0x1 0x0 0x0 0x7e800000 0x00010000
+		  0x2 0x0 0x0 0x7fb00000 0x00000100>;
+	status = "okay";
+
+	nor@0,0 {
+		compatible = "cfi-flash";
+		reg = <0x0 0x0 0x8000000>;
+		bank-width = <2>;
+		device-width = <1>;
+	};
+
+	nand@1,0 {
+		compatible = "fsl,ifc-nand";
+		reg = <0x1 0x0 0x10000>;
+	};
+
+	fpga: board-control@2,0 {
+		compatible = "fsl,ls1046aqds-fpga", "fsl,fpga-qixis", "simple-bus";
+		reg = <0x2 0x0 0x0000100>;
+		ranges = <0 2 0 0x100>;
+	};
+};
+
+&lpuart0 {
+	status = "okay";
+};
+
+&qspi {
+	num-cs = <2>;
+	bus-num = <0>;
+	status = "okay";
+
+	qflash0: s25fl128s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+};
+
+#include "fsl-ls1046-post.dtsi"
+
+&fman0 {
+	ethernet@e0000 {
+		phy-handle = <&qsgmii_phy_s2_p1>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@e2000 {
+		phy-handle = <&sgmii_phy_s4_p1>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@e4000 {
+		phy-handle = <&rgmii_phy1>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e6000 {
+		phy-handle = <&rgmii_phy2>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e8000 {
+		phy-handle = <&sgmii_phy_s1_p3>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@ea000 {
+		phy-handle = <&sgmii_phy_s1_p4>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@f0000 { /* DTSEC9/10GEC1 */
+		phy-handle = <&sgmii_phy_s1_p1>;
+		phy-connection-type = "xgmii";
+	};
+
+	ethernet@f2000 { /* DTSEC10/10GEC2 */
+		phy-handle = <&sgmii_phy_s1_p2>;
+		phy-connection-type = "xgmii";
+	};
+};
+
+&fpga {
+	#address-cells = <1>;
+	#size-cells = <1>;
+	mdio-mux-emi1 {
+		compatible = "mdio-mux-mmioreg", "mdio-mux";
+		mdio-parent-bus = <&mdio0>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x54 1>;    /* BRDCFG4 */
+		mux-mask = <0xe0>; /* EMI1 */
+
+		/* On-board RGMII1 PHY */
+		ls1046mdio0: mdio@0 {
+			reg = <0>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rgmii_phy1: ethernet-phy@1 { /* MAC3 */
+				reg = <0x1>;
+			};
+		};
+
+		/* On-board RGMII2 PHY */
+		ls1046mdio1: mdio@1 {
+			reg = <0x20>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rgmii_phy2: ethernet-phy@2 { /* MAC4 */
+				reg = <0x2>;
+			};
+		};
+
+		/* Slot 1 */
+		ls1046mdio_s1: mdio@2 {
+			reg = <0x40>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			sgmii_phy_s1_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+
+			sgmii_phy_s1_p2: ethernet-phy@1d {
+				reg = <0x1d>;
+			};
+
+			sgmii_phy_s1_p3: ethernet-phy@1e {
+				reg = <0x1e>;
+			};
+
+			sgmii_phy_s1_p4: ethernet-phy@1f {
+				reg = <0x1f>;
+			};
+		};
+
+		/* Slot 2 */
+		ls1046mdio_s2: mdio@3 {
+			reg = <0x60>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			qsgmii_phy_s2_p1: ethernet-phy@8 {
+				reg = <0x8>;
+			};
+			qsgmii_phy_s2_p2: ethernet-phy@9 {
+				reg = <0x9>;
+			};
+			qsgmii_phy_s2_p3: ethernet-phy@a {
+				reg = <0xa>;
+			};
+			qsgmii_phy_s2_p4: ethernet-phy@b {
+				reg = <0xb>;
+			};
+		};
+
+		/* Slot 4 */
+		ls1046mdio_s4: mdio@5 {
+			reg = <0x80>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			sgmii_phy_s4_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb-sdk.dts
@@ -0,0 +1,85 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1046A family SoC.
+ *
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
+ *
+ * Mingkai Hu <Mingkai.hu@freescale.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "fsl-ls1046a-rdb.dts"
+#include "qoriq-qman-portals-sdk.dtsi"
+#include "qoriq-bman-portals-sdk.dtsi"
+
+&bman_fbpr {
+	compatible = "fsl,bman-fbpr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_fqd {
+	compatible = "fsl,qman-fqd";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+&qman_pfdr {
+	compatible = "fsl,qman-pfdr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+&soc {
+#include "qoriq-dpaa-eth.dtsi"
+#include "qoriq-fman3-0-6oh.dtsi"
+};
+
+&fsldpaa {
+	ethernet@0 {
+		status = "disabled";
+	};
+	ethernet@1 {
+		status = "disabled";
+	};
+	ethernet@9 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet7>;
+		dma-coherent;
+	};
+};
+
+&fman0 {
+	compatible = "fsl,fman", "simple-bus";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb-usdpaa.dts
@@ -0,0 +1,110 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1046A family SoC.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ * This file is licensed under the terms of the GNU General Public
+ * License version 2.  This program is licensed "as is" without any
+ * warranty of any kind, whether express or implied.
+ */
+
+#include "fsl-ls1046a-rdb-sdk.dts"
+
+&soc {
+	bp7: buffer-pool@7 {
+		compatible = "fsl,ls1046a-bpool", "fsl,bpool";
+		fsl,bpid = <7>;
+		fsl,bpool-ethernet-cfg = <0 0 0 192 0 0xdeadbeef>;
+		fsl,bpool-thresholds = <0x400 0xc00 0x0 0x0>;
+	};
+
+	bp8: buffer-pool@8 {
+		compatible = "fsl,ls1046a-bpool", "fsl,bpool";
+		fsl,bpid = <8>;
+		fsl,bpool-ethernet-cfg = <0 0 0 576 0 0xabbaf00d>;
+		fsl,bpool-thresholds = <0x100 0x300 0x0 0x0>;
+	};
+
+	bp9: buffer-pool@9 {
+		compatible = "fsl,ls1046a-bpool", "fsl,bpool";
+		fsl,bpid = <9>;
+		fsl,bpool-ethernet-cfg = <0 0 0 2048 0 0xfeedabba>;
+		fsl,bpool-thresholds = <0x100 0x300 0x0 0x0>;
+	};
+
+	fsl,dpaa {
+		compatible = "fsl,ls1046a", "fsl,dpaa", "simple-bus";
+
+		ethernet@2 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x54 1 0x55 1>;
+			fsl,qman-frame-queues-tx = <0x74 1 0x75 1>;
+		};
+
+		ethernet@3 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x56 1 0x57 1>;
+			fsl,qman-frame-queues-tx = <0x76 1 0x77 1>;
+		};
+
+		ethernet@4 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x58 1 0x59 1>;
+			fsl,qman-frame-queues-tx = <0x78 1 0x79 1>;
+		};
+
+		ethernet@5 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x5a 1 0x5b 1>;
+			fsl,qman-frame-queues-tx = <0x7a 1 0x7b 1>;
+		};
+
+		ethernet@8 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x5c 1 0x5d 1>;
+			fsl,qman-frame-queues-tx = <0x7c 1 0x7d 1>;
+		};
+
+		ethernet@9 {
+			compatible = "fsl,dpa-ethernet-init";
+			fsl,bman-buffer-pools = <&bp7 &bp8 &bp9>;
+			fsl,qman-frame-queues-rx = <0x5e 1 0x5f 1>;
+			fsl,qman-frame-queues-tx = <0x7e 1 0x7f 1>;
+		};
+
+		dpa-fman0-oh@2 {
+			compatible = "fsl,dpa-oh";
+			/* Define frame queues for the OH port*/
+			/* <OH Rx error, OH Rx default> */
+			fsl,qman-frame-queues-oh = <0x60 1 0x61 1>;
+			fsl,fman-oh-port = <&fman0_oh2>;
+		};
+	};
+};
+/ {
+	reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		usdpaa_mem: usdpaa_mem {
+			compatible = "fsl,usdpaa-mem";
+			alloc-ranges = <0 0 0x10000 0>;
+			size = <0 0x10000000>;
+			alignment = <0 0x10000000>;
+		};
+	};
+};
+
+&fman0 {
+	fman0_oh2: port@83000 {
+		cell-index = <1>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x83000 0x1000>;
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a-rdb.dts
@@ -0,0 +1,181 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Freescale Layerscape-1046A family SoC.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ * Mingkai Hu <mingkai.hu@nxp.com>
+ */
+
+/dts-v1/;
+
+#include "fsl-ls1046a.dtsi"
+
+/ {
+	model = "LS1046A RDB Board";
+	compatible = "fsl,ls1046a-rdb", "fsl,ls1046a";
+
+	aliases {
+		serial0 = &duart0;
+		serial1 = &duart1;
+		serial2 = &duart2;
+		serial3 = &duart3;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+};
+
+&esdhc {
+	mmc-hs200-1_8v;
+	sd-uhs-sdr104;
+	sd-uhs-sdr50;
+	sd-uhs-sdr25;
+	sd-uhs-sdr12;
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&duart1 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+
+	ina220@40 {
+		compatible = "ti,ina220";
+		reg = <0x40>;
+		shunt-resistor = <1000>;
+	};
+
+	temp-sensor@4c {
+		compatible = "adi,adt7461";
+		reg = <0x4c>;
+	};
+
+	eeprom@56 {
+		compatible = "atmel,24c512";
+		reg = <0x52>;
+	};
+
+	eeprom@57 {
+		compatible = "atmel,24c512";
+		reg = <0x53>;
+	};
+};
+
+&i2c3 {
+	status = "okay";
+
+	rtc@51 {
+		compatible = "nxp,pcf2129";
+		reg = <0x51>;
+	};
+};
+
+&ifc {
+	#address-cells = <2>;
+	#size-cells = <1>;
+	/* NAND Flashe and CPLD on board */
+	ranges = <0x0 0x0 0x0 0x7e800000 0x00010000
+		  0x2 0x0 0x0 0x7fb00000 0x00000100>;
+	status = "okay";
+
+	nand@0,0 {
+		compatible = "fsl,ifc-nand";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		reg = <0x0 0x0 0x10000>;
+	};
+
+	cpld: board-control@2,0 {
+		compatible = "fsl,ls1046ardb-cpld";
+		reg = <0x2 0x0 0x0000100>;
+	};
+};
+
+&qspi {
+	num-cs = <2>;
+	bus-num = <0>;
+	status = "okay";
+
+	qflash0: s25fs512s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+
+	qflash1: s25fs512s@1 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		reg = <1>;
+	};
+};
+
+#include "fsl-ls1046-post.dtsi"
+
+&fman0 {
+	ethernet@e4000 {
+		phy-handle = <&rgmii_phy1>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e6000 {
+		phy-handle = <&rgmii_phy2>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e8000 {
+		phy-handle = <&sgmii_phy1>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@ea000 {
+		phy-handle = <&sgmii_phy2>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@f0000 { /* 10GEC1 */
+		phy-handle = <&aqr106_phy>;
+		phy-connection-type = "xgmii";
+	};
+
+	ethernet@f2000 { /* 10GEC2 */
+		fixed-link = <0 1 1000 0 0>;
+		phy-connection-type = "xgmii";
+	};
+
+	mdio@fc000 {
+		rgmii_phy1: ethernet-phy@1 {
+			reg = <0x1>;
+		};
+
+		rgmii_phy2: ethernet-phy@2 {
+			reg = <0x2>;
+		};
+
+		sgmii_phy1: ethernet-phy@3 {
+			reg = <0x3>;
+		};
+
+		sgmii_phy2: ethernet-phy@4 {
+			reg = <0x4>;
+		};
+	};
+
+	mdio@fd000 {
+		aqr106_phy: ethernet-phy@0 {
+			compatible = "ethernet-phy-ieee802.3-c45";
+			interrupts = <0 131 4>;
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a.dtsi
@@ -0,0 +1,771 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Freescale Layerscape-1046A family SoC.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ *
+ * Mingkai Hu <mingkai.hu@nxp.com>
+ */
+
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/thermal/thermal.h>
+
+/ {
+	compatible = "fsl,ls1046a";
+	interrupt-parent = <&gic>;
+	#address-cells = <2>;
+	#size-cells = <2>;
+
+	aliases {
+		crypto = &crypto;
+		fman0 = &fman0;
+		ethernet0 = &enet0;
+		ethernet1 = &enet1;
+		ethernet2 = &enet2;
+		ethernet3 = &enet3;
+		ethernet4 = &enet4;
+		ethernet5 = &enet5;
+		ethernet6 = &enet6;
+		ethernet7 = &enet7;
+	};
+
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <0x0>;
+			clocks = <&clockgen 1 0>;
+			next-level-cache = <&l2>;
+			cpu-idle-states = <&CPU_PH20>;
+			#cooling-cells = <2>;
+		};
+
+		cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <0x1>;
+			clocks = <&clockgen 1 0>;
+			next-level-cache = <&l2>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <0x2>;
+			clocks = <&clockgen 1 0>;
+			next-level-cache = <&l2>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <0x3>;
+			clocks = <&clockgen 1 0>;
+			next-level-cache = <&l2>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		l2: l2-cache {
+			compatible = "cache";
+		};
+	};
+
+	idle-states {
+		/*
+		 * PSCI node is not added default, U-boot will add missing
+		 * parts if it determines to use PSCI.
+		 */
+		entry-method = "arm,psci";
+
+		CPU_PH20: cpu-ph20 {
+			compatible = "arm,idle-state";
+			idle-state-name = "PH20";
+			arm,psci-suspend-param = <0x0>;
+			entry-latency-us = <1000>;
+			exit-latency-us = <1000>;
+			min-residency-us = <3000>;
+		};
+	};
+
+	memory@80000000 {
+		device_type = "memory";
+	};
+
+	sysclk: sysclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <100000000>;
+		clock-output-names = "sysclk";
+	};
+
+	reboot {
+		compatible ="syscon-reboot";
+		regmap = <&dcfg>;
+		offset = <0xb0>;
+		mask = <0x02>;
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_RAW(0xf) |
+					  IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 14 (GIC_CPU_MASK_RAW(0xf) |
+					  IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 11 (GIC_CPU_MASK_RAW(0xf) |
+					  IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 10 (GIC_CPU_MASK_RAW(0xf) |
+					  IRQ_TYPE_LEVEL_LOW)>;
+	};
+
+	pmu {
+		compatible = "arm,cortex-a72-pmu";
+		interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>,
+			     <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>,
+			     <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>,
+			     <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-affinity = <&cpu0>,
+				     <&cpu1>,
+				     <&cpu2>,
+				     <&cpu3>;
+	};
+
+	gic: interrupt-controller@1400000 {
+		compatible = "arm,gic-400";
+		#interrupt-cells = <3>;
+		interrupt-controller;
+		reg = <0x0 0x1410000 0 0x10000>, /* GICD */
+		      <0x0 0x1420000 0 0x20000>, /* GICC */
+		      <0x0 0x1440000 0 0x20000>, /* GICH */
+		      <0x0 0x1460000 0 0x20000>; /* GICV */
+		interrupts = <GIC_PPI 9 (GIC_CPU_MASK_RAW(0xf) |
+					 IRQ_TYPE_LEVEL_LOW)>;
+	};
+
+	soc: soc {
+		compatible = "simple-bus";
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		ddr: memory-controller@1080000 {
+			compatible = "fsl,qoriq-memory-controller";
+			reg = <0x0 0x1080000 0x0 0x1000>;
+			interrupts = <GIC_SPI 144 IRQ_TYPE_LEVEL_HIGH>;
+			big-endian;
+		};
+
+		ifc: ifc@1530000 {
+			compatible = "fsl,ifc", "simple-bus";
+			reg = <0x0 0x1530000 0x0 0x10000>;
+			big-endian;
+			interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		qspi: quadspi@1550000 {
+			compatible = "fsl,ls1021a-qspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x1550000 0x0 0x10000>,
+				<0x0 0x40000000 0x0 0x10000000>;
+			reg-names = "QuadSPI", "QuadSPI-memory";
+			interrupts = <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>;
+			clock-names = "qspi_en", "qspi";
+			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
+			big-endian;
+			fsl,qspi-has-second-chip;
+			status = "disabled";
+		};
+
+		esdhc: esdhc@1560000 {
+			compatible = "fsl,ls1046a-esdhc", "fsl,esdhc";
+			reg = <0x0 0x1560000 0x0 0x10000>;
+			interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 2 1>;
+			voltage-ranges = <1800 1800 3300 3300>;
+			sdhci,auto-cmd12;
+			big-endian;
+			bus-width = <4>;
+		};
+
+		scfg: scfg@1570000 {
+			compatible = "fsl,ls1046a-scfg", "syscon";
+			reg = <0x0 0x1570000 0x0 0x10000>;
+			big-endian;
+		};
+
+		crypto: crypto@1700000 {
+			compatible = "fsl,sec-v5.4", "fsl,sec-v5.0",
+				     "fsl,sec-v4.0";
+			fsl,sec-era = <8>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0x0 0x00 0x1700000 0x100000>;
+			reg = <0x00 0x1700000 0x0 0x100000>;
+			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
+
+			sec_jr0: jr@10000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x10000 0x10000>;
+				interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr1: jr@20000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x20000 0x10000>;
+				interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr2: jr@30000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x30000 0x10000>;
+				interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr3: jr@40000 {
+				compatible = "fsl,sec-v5.4-job-ring",
+					     "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x40000 0x10000>;
+				interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+
+		qman: qman@1880000 {
+			compatible = "fsl,qman";
+			reg = <0x00 0x1880000 0x0 0x10000>;
+			interrupts = <0 45 0x4>;
+			memory-region = <&qman_fqd &qman_pfdr>;
+
+		};
+
+		bman: bman@1890000 {
+			compatible = "fsl,bman";
+			reg = <0x00 0x1890000 0x0 0x10000>;
+			interrupts = <0 45 0x4>;
+			memory-region = <&bman_fbpr>;
+
+		};
+
+		qportals: qman-portals@500000000 {
+			ranges = <0x0 0x5 0x00000000 0x8000000>;
+		};
+
+		bportals: bman-portals@508000000 {
+			ranges = <0x0 0x5 0x08000000 0x8000000>;
+		};
+
+		dcfg: dcfg@1ee0000 {
+			compatible = "fsl,ls1046a-dcfg", "syscon";
+			reg = <0x0 0x1ee0000 0x0 0x1000>;
+			big-endian;
+		};
+
+		clockgen: clocking@1ee1000 {
+			compatible = "fsl,ls1046a-clockgen";
+			reg = <0x0 0x1ee1000 0x0 0x1000>;
+			#clock-cells = <2>;
+			clocks = <&sysclk>;
+		};
+
+		tmu: tmu@1f00000 {
+			compatible = "fsl,qoriq-tmu";
+			reg = <0x0 0x1f00000 0x0 0x10000>;
+			interrupts = <0 33 0x4>;
+			fsl,tmu-range = <0xb0000 0x9002a 0x6004c 0x30062>;
+			fsl,tmu-calibration =
+				/* Calibration data group 1 */
+				<0x00000000 0x00000026
+				0x00000001 0x0000002d
+				0x00000002 0x00000032
+				0x00000003 0x00000039
+				0x00000004 0x0000003f
+				0x00000005 0x00000046
+				0x00000006 0x0000004d
+				0x00000007 0x00000054
+				0x00000008 0x0000005a
+				0x00000009 0x00000061
+				0x0000000a 0x0000006a
+				0x0000000b 0x00000071
+				/* Calibration data group 2 */
+				0x00010000 0x00000025
+				0x00010001 0x0000002c
+				0x00010002 0x00000035
+				0x00010003 0x0000003d
+				0x00010004 0x00000045
+				0x00010005 0x0000004e
+				0x00010006 0x00000057
+				0x00010007 0x00000061
+				0x00010008 0x0000006b
+				0x00010009 0x00000076
+				/* Calibration data group 3 */
+				0x00020000 0x00000029
+				0x00020001 0x00000033
+				0x00020002 0x0000003d
+				0x00020003 0x00000049
+				0x00020004 0x00000056
+				0x00020005 0x00000061
+				0x00020006 0x0000006d
+				/* Calibration data group 4 */
+				0x00030000 0x00000021
+				0x00030001 0x0000002a
+				0x00030002 0x0000003c
+				0x00030003 0x0000004e>;
+			big-endian;
+			#thermal-sensor-cells = <1>;
+		};
+
+		thermal-zones {
+			cpu_thermal: cpu-thermal {
+				polling-delay-passive = <1000>;
+				polling-delay = <5000>;
+				thermal-sensors = <&tmu 3>;
+
+				trips {
+					cpu_alert: cpu-alert {
+						temperature = <85000>;
+						hysteresis = <2000>;
+						type = "passive";
+					};
+
+					cpu_crit: cpu-crit {
+						temperature = <95000>;
+						hysteresis = <2000>;
+						type = "critical";
+					};
+				};
+
+				cooling-maps {
+					map0 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu0 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+				};
+			};
+		};
+
+		dspi: dspi@2100000 {
+			compatible = "fsl,ls1021a-v1.0-dspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2100000 0x0 0x10000>;
+			interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
+			clock-names = "dspi";
+			clocks = <&clockgen 4 1>;
+			spi-num-chipselects = <5>;
+			big-endian;
+			status = "disabled";
+		};
+
+		i2c0: i2c@2180000 {
+			compatible = "fsl,vf610-i2c", "fsl,ls1046a-vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2180000 0x0 0x10000>;
+			interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			dmas = <&edma0 1 39>,
+			       <&edma0 1 38>;
+			dma-names = "tx", "rx";
+			fsl-scl-gpio = <&gpio3 12 0>;
+			status = "disabled";
+		};
+
+		i2c1: i2c@2190000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2190000 0x0 0x10000>;
+			interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			status = "disabled";
+		};
+
+		i2c2: i2c@21a0000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x21a0000 0x0 0x10000>;
+			interrupts = <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			status = "disabled";
+		};
+
+		i2c3: i2c@21b0000 {
+			compatible = "fsl,vf610-i2c", "fsl,ls1046a-vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x21b0000 0x0 0x10000>;
+			interrupts = <GIC_SPI 59 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			fsl-scl-gpio = <&gpio3 12 0>;
+			status = "disabled";
+		};
+
+		duart0: serial@21c0500 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x00 0x21c0500 0x0 0x100>;
+			interrupts = <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+		};
+
+		duart1: serial@21c0600 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x00 0x21c0600 0x0 0x100>;
+			interrupts = <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+		};
+
+		duart2: serial@21d0500 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21d0500 0x0 0x100>;
+			interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+		};
+
+		duart3: serial@21d0600 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21d0600 0x0 0x100>;
+			interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+		};
+
+		gpio0: gpio@2300000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2300000 0x0 0x10000>;
+			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio1: gpio@2310000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2310000 0x0 0x10000>;
+			interrupts = <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio2: gpio@2320000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2320000 0x0 0x10000>;
+			interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio3: gpio@2330000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2330000 0x0 0x10000>;
+			interrupts = <GIC_SPI 134 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		lpuart0: serial@2950000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2950000 0x0 0x1000>;
+			interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 0>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart1: serial@2960000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2960000 0x0 0x1000>;
+			interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart2: serial@2970000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2970000 0x0 0x1000>;
+			interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart3: serial@2980000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2980000 0x0 0x1000>;
+			interrupts = <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart4: serial@2990000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2990000 0x0 0x1000>;
+			interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart5: serial@29a0000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x29a0000 0x0 0x1000>;
+			interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		ftm0: ftm0@29d0000 {
+			compatible = "fsl,ls1046a-ftm";
+			reg = <0x0 0x29d0000 0x0 0x10000>,
+			      <0x0 0x1ee2140 0x0 0x4>;
+			reg-names = "ftm", "FlexTimer1";
+			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
+			big-endian;
+		};
+
+		wdog0: watchdog@2ad0000 {
+			compatible = "fsl,imx21-wdt";
+			reg = <0x0 0x2ad0000 0x0 0x10000>;
+			interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			big-endian;
+		};
+
+		edma0: edma@2c00000 {
+			#dma-cells = <2>;
+			compatible = "fsl,vf610-edma";
+			reg = <0x0 0x2c00000 0x0 0x10000>,
+			      <0x0 0x2c10000 0x0 0x10000>,
+			      <0x0 0x2c20000 0x0 0x10000>;
+			interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "edma-tx", "edma-err";
+			dma-channels = <32>;
+			big-endian;
+			clock-names = "dmamux0", "dmamux1";
+			clocks = <&clockgen 4 1>,
+				 <&clockgen 4 1>;
+		};
+
+		usb0: usb@2f00000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x2f00000 0x0 0x10000>;
+			interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
+			dr_mode = "host";
+			snps,quirk-frame-length-adjustment = <0x20>;
+			snps,dis_rxdet_inp3_quirk;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
+		};
+
+		usb1: usb@3000000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3000000 0x0 0x10000>;
+			interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
+			dr_mode = "host";
+			snps,quirk-frame-length-adjustment = <0x20>;
+			snps,dis_rxdet_inp3_quirk;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
+		};
+
+		usb2: usb@3100000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3100000 0x0 0x10000>;
+			interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
+			dr_mode = "host";
+			snps,quirk-frame-length-adjustment = <0x20>;
+			snps,dis_rxdet_inp3_quirk;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
+		};
+
+		sata: sata@3200000 {
+			compatible = "fsl,ls1046a-ahci";
+			reg = <0x0 0x3200000 0x0 0x10000>,
+				<0x0 0x20140520 0x0 0x4>;
+			reg-names = "ahci", "sata-ecc";
+			interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 1>;
+			dma-coherent;
+		};
+
+		qdma: qdma@8380000 {
+			compatible = "fsl,ls1046a-qdma", "fsl,ls1021a-qdma";
+			reg = <0x0 0x8380000 0x0 0x1000>, /* Controller regs */
+			      <0x0 0x8390000 0x0 0x10000>, /* Status regs */
+			      <0x0 0x83a0000 0x0 0x40000>; /* Block regs */
+			interrupts = <0 153 0x4>,
+				     <0 39 0x4>;
+			interrupt-names = "qdma-error", "qdma-queue";
+			channels = <8>;
+			queues = <2>;
+			status-sizes = <64>;
+			queue-sizes = <64 64>;
+			big-endian;
+		};
+
+		msi1: msi-controller@1580000 {
+			compatible = "fsl,ls1046a-msi";
+			msi-controller;
+			reg = <0x0 0x1580000 0x0 0x10000>;
+			interrupts = <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		msi2: msi-controller@1590000 {
+			compatible = "fsl,ls1046a-msi";
+			msi-controller;
+			reg = <0x0 0x1590000 0x0 0x10000>;
+			interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 122 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		msi3: msi-controller@15a0000 {
+			compatible = "fsl,ls1046a-msi";
+			msi-controller;
+			reg = <0x0 0x15a0000 0x0 0x10000>;
+			interrupts = <GIC_SPI 160 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pcie@3400000 {
+			compatible = "fsl,ls1046a-pcie", "snps,dw-pcie";
+			reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
+			       0x40 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>, /* PME interrupt */
+				     <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
+			interrupt-names = "pme", "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x40 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x40 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 2 &gic GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 3 &gic GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 4 &gic GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pcie@3500000 {
+			compatible = "fsl,ls1046a-pcie", "snps,dw-pcie";
+			reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
+			       0x48 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "pme", "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <2>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x48 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x48 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 2 &gic GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 3 &gic GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 4 &gic GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pcie@3600000 {
+			compatible = "fsl,ls1046a-pcie", "snps,dw-pcie";
+			reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
+			       0x50 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <GIC_SPI 161 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 162 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "pme", "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <2>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x50 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x50 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 2 &gic GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 3 &gic GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 4 &gic GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+	};
+
+	reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		bman_fbpr: bman-fbpr {
+			compatible = "shared-dma-pool";
+			size = <0 0x1000000>;
+			alignment = <0 0x1000000>;
+			no-map;
+		};
+		qman_fqd: qman-fqd {
+			compatible = "shared-dma-pool";
+			size = <0 0x800000>;
+			alignment = <0 0x800000>;
+			no-map;
+		};
+		qman_pfdr: qman-pfdr {
+			compatible = "shared-dma-pool";
+			size = <0 0x2000000>;
+			alignment = <0 0x2000000>;
+			no-map;
+		};
+	};
+
+	firmware {
+		optee {
+			compatible = "linaro,optee-tz";
+			method = "smc";
+		};
+	};
+};
+
+#include "qoriq-qman-portals.dtsi"
+#include "qoriq-bman-portals.dtsi"
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1088a-qds.dts
@@ -0,0 +1,137 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for NXP LS1088A QDS Board.
+ *
+ * Copyright 2017 NXP
+ *
+ * Harninder Rai <harninder.rai@nxp.com>
+ *
+ */
+
+/dts-v1/;
+
+#include "fsl-ls1088a.dtsi"
+
+/ {
+	model = "LS1088A QDS Board";
+	compatible = "fsl,ls1088a-qds", "fsl,ls1088a";
+};
+
+&i2c0 {
+	status = "okay";
+
+	i2c-switch@77 {
+		compatible = "nxp,pca9547";
+		reg = <0x77>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		i2c@2 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x2>;
+
+			ina220@40 {
+				compatible = "ti,ina220";
+				reg = <0x40>;
+				shunt-resistor = <1000>;
+			};
+
+			ina220@41 {
+				compatible = "ti,ina220";
+				reg = <0x41>;
+				shunt-resistor = <1000>;
+			};
+		};
+
+		i2c@3 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x3>;
+
+			temp-sensor@4c {
+				compatible = "adi,adt7461a";
+				reg = <0x4c>;
+			};
+
+			rtc@51 {
+				compatible = "nxp,pcf2129";
+				reg = <0x51>;
+				/* IRQ10_B */
+				interrupts = <0 150 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			eeprom@56 {
+				compatible = "atmel,24c512";
+				reg = <0x56>;
+			};
+
+			eeprom@57 {
+				compatible = "atmel,24c512";
+				reg = <0x57>;
+			};
+		};
+	};
+};
+
+&qspi {
+	status = "okay";
+	qflash0: s25fs512s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		m25p,fast-read;
+		reg = <0>;
+	};
+
+	qflash1: s25fs512s@1 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		spi-max-frequency = <20000000>;
+		m25p,fast-read;
+		reg = <1>;
+	};
+};
+
+&ifc {
+	status = "okay";
+
+	ranges = <0 0 0x5 0x80000000 0x08000000
+		  2 0 0x5 0x30000000 0x00010000
+		  3 0 0x5 0x20000000 0x00010000>;
+
+	nor@0,0 {
+		compatible = "cfi-flash";
+		reg = <0x0 0x0 0x8000000>;
+		bank-width = <2>;
+		device-width = <1>;
+	};
+
+	nand@2,0 {
+		compatible = "fsl,ifc-nand";
+		reg = <0x2 0x0 0x10000>;
+	};
+
+	fpga: board-control@3,0 {
+		compatible = "fsl,ls1088aqds-fpga", "fsl,fpga-qixis";
+		reg = <0x3 0x0 0x0000100>;
+	};
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&duart1 {
+	status = "okay";
+};
+
+&esdhc {
+	status = "okay";
+};
+
+&sata {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1088a-rdb.dts
@@ -0,0 +1,200 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for NXP LS1088A RDB Board.
+ *
+ * Copyright 2017 NXP
+ *
+ * Harninder Rai <harninder.rai@nxp.com>
+ *
+ */
+
+/dts-v1/;
+
+#include "fsl-ls1088a.dtsi"
+
+/ {
+	model = "L1088A RDB Board";
+	compatible = "fsl,ls1088a-rdb", "fsl,ls1088a";
+};
+
+&i2c0 {
+	status = "okay";
+
+	i2c-switch@77 {
+		compatible = "nxp,pca9547";
+		reg = <0x77>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		i2c@2 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x2>;
+
+			ina220@40 {
+				compatible = "ti,ina220";
+				reg = <0x40>;
+				shunt-resistor = <1000>;
+			};
+		};
+
+		i2c@3 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x3>;
+
+			temp-sensor@4c {
+				compatible = "adi,adt7461a";
+				reg = <0x4c>;
+			};
+
+			rtc@51 {
+				compatible = "nxp,pcf2129";
+				reg = <0x51>;
+				/* IRQ10_B */
+				interrupts = <0 150 IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+	};
+};
+
+&qspi {
+	status = "okay";
+	qflash0: s25fs512s@0 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		m25p,fast-read;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+
+	qflash1: s25fs512s@1 {
+		compatible = "spansion,m25p80";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		m25p,fast-read;
+		spi-max-frequency = <20000000>;
+		reg = <1>;
+	};
+};
+
+&ifc {
+	status = "okay";
+
+	ranges = <0 0 0x5 0x30000000 0x00010000
+		  2 0 0x5 0x20000000 0x00010000>;
+
+	nand@0,0 {
+		compatible = "fsl,ifc-nand";
+		reg = <0x0 0x0 0x10000>;
+	};
+
+	fpga: board-control@2,0 {
+		compatible = "fsl,ls1088ardb-fpga", "fsl,fpga-qixis";
+		reg = <0x2 0x0 0x0000100>;
+	};
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&duart1 {
+	status = "okay";
+};
+
+&usb0 {
+	status = "okay";
+};
+
+&usb1 {
+	status = "okay";
+};
+
+&esdhc {
+	status = "okay";
+};
+
+&sata {
+	status = "okay";
+};
+
+&emdio1 {
+	/* Freescale F104 PHY1 */
+	mdio1_phy1: emdio1_phy@1 {
+		reg = <0x1c>;
+		phy-connection-type = "qsgmii";
+	};
+	mdio1_phy2: emdio1_phy@2 {
+		reg = <0x1d>;
+		phy-connection-type = "qsgmii";
+	};
+	mdio1_phy3: emdio1_phy@3 {
+		reg = <0x1e>;
+		phy-connection-type = "qsgmii";
+	};
+	mdio1_phy4: emdio1_phy@4 {
+		reg = <0x1f>;
+		phy-connection-type = "qsgmii";
+	};
+	/* F104 PHY2 */
+	mdio1_phy5: emdio1_phy@5 {
+		reg = <0x0c>;
+		phy-connection-type = "qsgmii";
+	};
+	mdio1_phy6: emdio1_phy@6 {
+		reg = <0x0d>;
+		phy-connection-type = "qsgmii";
+	};
+	mdio1_phy7: emdio1_phy@7 {
+		reg = <0x0e>;
+		phy-connection-type = "qsgmii";
+	};
+	mdio1_phy8: emdio1_phy@8 {
+		reg = <0x0f>;
+		phy-connection-type = "qsgmii";
+	};
+};
+
+&emdio2 {
+	/* Aquantia AQR105 10G PHY */
+	mdio2_phy1: emdio2_phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 2 0x4>;
+		reg = <0x0>;
+		phy-connection-type = "xfi";
+	};
+};
+
+/* DPMAC connections to external PHYs
+ * based on LS1088A RM RevC - $24.1.2 SerDes Options
+ */
+/* DPMAC1 is 10G SFP+, fixed link */
+&dpmac2 {
+	phy-handle = <&mdio2_phy1>;
+};
+&dpmac3 {
+	phy-handle = <&mdio1_phy5>;
+};
+&dpmac4 {
+	phy-handle = <&mdio1_phy6>;
+};
+&dpmac5 {
+	phy-handle = <&mdio1_phy7>;
+};
+&dpmac6 {
+	phy-handle = <&mdio1_phy8>;
+};
+&dpmac7 {
+	phy-handle = <&mdio1_phy1>;
+};
+&dpmac8 {
+	phy-handle = <&mdio1_phy2>;
+};
+&dpmac9 {
+	phy-handle = <&mdio1_phy3>;
+};
+&dpmac10 {
+	phy-handle = <&mdio1_phy4>;
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
@@ -0,0 +1,800 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for NXP Layerscape-1088A family SoC.
+ *
+ * Copyright 2017 NXP
+ *
+ * Harninder Rai <harninder.rai@nxp.com>
+ *
+ */
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/thermal/thermal.h>
+
+/ {
+	compatible = "fsl,ls1088a";
+	interrupt-parent = <&gic>;
+	#address-cells = <2>;
+	#size-cells = <2>;
+
+	aliases {
+		crypto = &crypto;
+	};
+
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		/* We have 2 clusters having 4 Cortex-A53 cores each */
+		cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x0>;
+			clocks = <&clockgen 1 0>;
+			#cooling-cells = <2>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x1>;
+			clocks = <&clockgen 1 0>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x2>;
+			clocks = <&clockgen 1 0>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x3>;
+			clocks = <&clockgen 1 0>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu4: cpu@100 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x100>;
+			clocks = <&clockgen 1 1>;
+			#cooling-cells = <2>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu5: cpu@101 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x101>;
+			clocks = <&clockgen 1 1>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu6: cpu@102 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x102>;
+			clocks = <&clockgen 1 1>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+
+		cpu7: cpu@103 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x103>;
+			clocks = <&clockgen 1 1>;
+			cpu-idle-states = <&CPU_PH20>;
+		};
+	};
+
+	idle-states {
+		/*
+		 * PSCI node is not added default, U-boot will add missing
+		 * parts if it determines to use PSCI.
+		 */
+		entry-method = "arm,psci";
+
+		CPU_PH20: cpu-ph20 {
+			compatible = "arm,idle-state";
+			idle-state-name = "PH20";
+			arm,psci-suspend-param = <0x0>;
+			entry-latency-us = <1000>;
+			exit-latency-us = <1000>;
+			min-residency-us = <3000>;
+		};
+	};
+
+	gic: interrupt-controller@6000000 {
+		compatible = "arm,gic-v3";
+		#interrupt-cells = <3>;
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		interrupt-controller;
+		reg = <0x0 0x06000000 0 0x10000>, /* GIC Dist */
+		      <0x0 0x06100000 0 0x100000>, /* GICR(RD_base+SGI_base)*/
+		      <0x0 0x0c0c0000 0 0x2000>, /* GICC */
+		      <0x0 0x0c0d0000 0 0x1000>, /* GICH */
+		      <0x0 0x0c0e0000 0 0x20000>; /* GICV */
+		interrupts = <1 9 IRQ_TYPE_LEVEL_HIGH>;
+
+		its: gic-its@6020000 {
+			compatible = "arm,gic-v3-its";
+			msi-controller;
+			reg = <0x0 0x6020000 0 0x20000>;
+		};
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <1 13 IRQ_TYPE_LEVEL_LOW>,/* Physical Secure PPI */
+			     <1 14 IRQ_TYPE_LEVEL_LOW>,/* Physical Non-Secure PPI */
+			     <1 11 IRQ_TYPE_LEVEL_LOW>,/* Virtual PPI */
+			     <1 10 IRQ_TYPE_LEVEL_LOW>;/* Hypervisor PPI */
+	};
+
+	sysclk: sysclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <100000000>;
+		clock-output-names = "sysclk";
+	};
+
+	dcfg: dcfg@1e00000 {
+		compatible = "fsl,ls1088a-dcfg", "syscon";
+		reg = <0x0 0x1e00000 0x0 0x10000>;
+		little-endian;
+	};
+
+	rstcr: syscon@1e60000 {
+		compatible = "fsl,ls1088a-rstcr", "syscon";
+		reg = <0x0 0x1e60000 0x0 0x4>;
+	};
+
+	reboot {
+		compatible = "syscon-reboot";
+		regmap = <&rstcr>;
+		offset = <0x0>;
+		mask = <0x02>;
+	};
+
+
+	soc {
+		compatible = "simple-bus";
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		dma-ranges = <0x0 0x0 0x0 0x0 0x10000 0x00000000>;
+
+		clockgen: clocking@1300000 {
+			compatible = "fsl,ls1088a-clockgen";
+			reg = <0 0x1300000 0 0xa0000>;
+			#clock-cells = <2>;
+			clocks = <&sysclk>;
+		};
+
+		tmu: tmu@1f80000 {
+			compatible = "fsl,qoriq-tmu";
+			reg = <0x0 0x1f80000 0x0 0x10000>;
+			interrupts = <0 23 0x4>;
+			fsl,tmu-range = <0xb0000 0x9002a 0x6004c 0x30062>;
+			fsl,tmu-calibration =
+				/* Calibration data group 1 */
+				<0x00000000 0x00000026
+				0x00000001 0x0000002d
+				0x00000002 0x00000032
+				0x00000003 0x00000039
+				0x00000004 0x0000003f
+				0x00000005 0x00000046
+				0x00000006 0x0000004d
+				0x00000007 0x00000054
+				0x00000008 0x0000005a
+				0x00000009 0x00000061
+				0x0000000a 0x0000006a
+				0x0000000b 0x00000071
+				/* Calibration data group 2 */
+				0x00010000 0x00000025
+				0x00010001 0x0000002c
+				0x00010002 0x00000035
+				0x00010003 0x0000003d
+				0x00010004 0x00000045
+				0x00010005 0x0000004e
+				0x00010006 0x00000057
+				0x00010007 0x00000061
+				0x00010008 0x0000006b
+				0x00010009 0x00000076
+				/* Calibration data group 3 */
+				0x00020000 0x00000029
+				0x00020001 0x00000033
+				0x00020002 0x0000003d
+				0x00020003 0x00000049
+				0x00020004 0x00000056
+				0x00020005 0x00000061
+				0x00020006 0x0000006d
+				/* Calibration data group 4 */
+				0x00030000 0x00000021
+				0x00030001 0x0000002a
+				0x00030002 0x0000003c
+				0x00030003 0x0000004e>;
+			little-endian;
+			#thermal-sensor-cells = <1>;
+		};
+
+		thermal-zones {
+			cpu_thermal: cpu-thermal {
+				polling-delay-passive = <1000>;
+				polling-delay = <5000>;
+				thermal-sensors = <&tmu 0>;
+
+				trips {
+					cpu_alert: cpu-alert {
+						temperature = <85000>;
+						hysteresis = <2000>;
+						type = "passive";
+					};
+
+					cpu_crit: cpu-crit {
+						temperature = <95000>;
+						hysteresis = <2000>;
+						type = "critical";
+					};
+				};
+
+				cooling-maps {
+					map0 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu0 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+					map1 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu4 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+				};
+			};
+		};
+
+		duart0: serial@21c0500 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21c0500 0x0 0x100>;
+			clocks = <&clockgen 4 3>;
+			interrupts = <0 32 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+		};
+
+		duart1: serial@21c0600 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21c0600 0x0 0x100>;
+			clocks = <&clockgen 4 3>;
+			interrupts = <0 32 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+		};
+
+		cluster1_core0_watchdog: wdt@c000000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc000000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster1_core1_watchdog: wdt@c010000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc010000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster1_core2_watchdog: wdt@c020000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc020000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster1_core3_watchdog: wdt@c030000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc030000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster2_core0_watchdog: wdt@c100000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc100000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster2_core1_watchdog: wdt@c110000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc110000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster2_core2_watchdog: wdt@c120000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc120000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster2_core3_watchdog: wdt@c130000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc130000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		gpio0: gpio@2300000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2300000 0x0 0x10000>;
+			interrupts = <0 36 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio1: gpio@2310000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2310000 0x0 0x10000>;
+			interrupts = <0 36 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio2: gpio@2320000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2320000 0x0 0x10000>;
+			interrupts = <0 37 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio3: gpio@2330000 {
+			compatible = "fsl,qoriq-gpio";
+			reg = <0x0 0x2330000 0x0 0x10000>;
+			interrupts = <0 37 IRQ_TYPE_LEVEL_HIGH>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		/* TODO: WRIOP (CCSR?) */
+		emdio1: mdio@0x8B96000 { /* WRIOP0: 0x8B8_0000,
+					  * E-MDIO1: 0x1_6000
+					  */
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8B96000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;	/* force the driver in LE mode */
+
+			/* Not necessary on the QDS, but needed on the RDB */
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		emdio2: mdio@0x8B97000 { /* WRIOP0: 0x8B8_0000,
+					  * E-MDIO2: 0x1_7000
+					  */
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8B97000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;	/* force the driver in LE mode */
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		ifc: ifc@2240000 {
+			compatible = "fsl,ifc", "simple-bus";
+			reg = <0x0 0x2240000 0x0 0x20000>;
+			interrupts = <0 21 IRQ_TYPE_LEVEL_HIGH>;
+			little-endian;
+			#address-cells = <2>;
+			#size-cells = <1>;
+
+		};
+
+		ftm0: ftm0@2800000 {
+			compatible = "fsl,ls1088a-ftm";
+			reg = <0x0 0x2800000 0x0 0x10000>,
+			      <0x0 0x1e34050 0x0 0x4>;
+			interrupts = <0 44 4>;
+			reg-names = "ftm", "FlexTimer1";
+		};
+
+		i2c0: i2c@2000000 {
+			compatible = "fsl,vf610-i2c", "fsl,ls1088a-vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2000000 0x0 0x10000>;
+			interrupts = <0 34 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 7>;
+			fsl-scl-gpio = <&gpio3 30 0>;
+			status = "disabled";
+		};
+
+		i2c1: i2c@2010000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2010000 0x0 0x10000>;
+			interrupts = <0 34 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 7>;
+			status = "disabled";
+		};
+
+		i2c2: i2c@2020000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2020000 0x0 0x10000>;
+			interrupts = <0 35 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 7>;
+			status = "disabled";
+		};
+
+		i2c3: i2c@2030000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2030000 0x0 0x10000>;
+			interrupts = <0 35 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 7>;
+			status = "disabled";
+		};
+
+		qspi: quadspi@20c0000 {
+			compatible = "fsl,ls2080a-qspi", "fsl,ls1088a-qspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x20c0000 0x0 0x10000>,
+				<0x0 0x20000000 0x0 0x10000000>;
+			reg-names = "QuadSPI", "QuadSPI-memory";
+			interrupts = <0 25 0x4>; /* Level high type */
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "qspi_en", "qspi";
+			fsl,qspi-has-second-chip;
+		};
+
+		esdhc: esdhc@2140000 {
+			compatible = "fsl,ls1088a-esdhc", "fsl,esdhc";
+			reg = <0x0 0x2140000 0x0 0x10000>;
+			interrupts = <0 28 0x4>; /* Level high type */
+			clock-frequency = <0>;
+			voltage-ranges = <1800 1800 3300 3300>;
+			sdhci,auto-cmd12;
+			little-endian;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		usb0: usb3@3100000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3100000 0x0 0x10000>;
+			interrupts = <0 80 0x4>; /* Level high type */
+			dr_mode = "host";
+			configure-gfladj;
+			snps,dis_rxdet_inp3_quirk;
+		};
+
+		usb1: usb3@3110000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3110000 0x0 0x10000>;
+			interrupts = <0 81 0x4>; /* Level high type */
+			dr_mode = "host";
+			configure-gfladj;
+			snps,dis_rxdet_inp3_quirk;
+		};
+
+		sata: sata@3200000 {
+			compatible = "fsl,ls1088a-ahci";
+			reg = <0x0 0x3200000 0x0 0x10000>,
+				<0x7 0x100520 0x0 0x4>;
+			reg-names = "ahci", "sata-ecc";
+			interrupts = <0 133 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clockgen 4 3>;
+			dma-coherent;
+			status = "disabled";
+		};
+
+		pcie@3400000 {
+			compatible = "fsl,ls2088a-pcie", "fsl,ls1088a-pcie",
+				     "snps,dw-pcie";
+			reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
+			       0x20 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <0 108 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
+			interrupt-names = "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x20 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x20 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 1>;	/* This is fixed-up by u-boot */
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 0 0 109 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 2 &gic 0 0 0 110 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 3 &gic 0 0 0 111 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 4 &gic 0 0 0 112 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pcie@3500000 {
+			compatible = "fsl,ls2088a-pcie", "fsl,ls1088a-pcie",
+				     "snps,dw-pcie";
+			reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
+			       0x28 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <0 113 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
+			interrupt-names = "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x28 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x28 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 1>;	/* This is fixed-up by u-boot */
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 0 0 114 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 2 &gic 0 0 0 115 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 3 &gic 0 0 0 116 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 4 &gic 0 0 0 117 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pcie@3600000 {
+			compatible = "fsl,ls2088a-pcie", "fsl,ls1088a-pcie",
+				     "snps,dw-pcie";
+			reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
+			       0x30 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <0 118 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
+			interrupt-names = "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <8>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x30 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x30 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 1>;	/* This is fixed-up by u-boot */
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 0 0 119 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 2 &gic 0 0 0 120 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 3 &gic 0 0 0 121 IRQ_TYPE_LEVEL_HIGH>,
+					<0000 0 0 4 &gic 0 0 0 122 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		fsl_mc: fsl-mc@80c000000 {
+			compatible = "fsl,qoriq-mc";
+			reg = <0x00000008 0x0c000000 0 0x40>,	 /* MC portal base */
+			      <0x00000000 0x08340000 0 0x40000>; /* MC control reg */
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 0>;	/* This is fixed-up by u-boot */
+			dma-coherent;
+			#address-cells = <3>;
+			#size-cells = <1>;
+
+			/*
+			 * Region type 0x0 - MC portals
+			 * Region type 0x1 - QBMAN portals
+			 */
+			ranges = <0x0 0x0 0x0 0x8 0x0c000000 0x4000000
+				  0x1 0x0 0x0 0x8 0x18000000 0x8000000>;
+
+			dpmacs {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				dpmac1: dpmac@1 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <1>;
+				};
+
+				dpmac2: dpmac@2 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <2>;
+				};
+
+				dpmac3: dpmac@3 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <3>;
+				};
+
+				dpmac4: dpmac@4 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <4>;
+				};
+
+				dpmac5: dpmac@5 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <5>;
+				};
+
+				dpmac6: dpmac@6 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <6>;
+				};
+
+				dpmac7: dpmac@7 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <7>;
+				};
+
+				dpmac8: dpmac@8 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <8>;
+				};
+
+				dpmac9: dpmac@9 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <9>;
+				};
+
+				dpmac10: dpmac@a {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0xa>;
+				};
+			};
+		};
+
+		smmu: iommu@5000000 {
+			compatible = "arm,mmu-500";
+			reg = <0 0x5000000 0 0x800000>;
+			#global-interrupts = <12>;
+			#iommu-cells = <1>;
+			stream-match-mask = <0x7C00>;
+			interrupts = <0 13 4>, /* global secure fault */
+				     <0 14 4>, /* combined secure interrupt */
+				     <0 15 4>, /* global non-secure fault */
+				     <0 16 4>, /* combined non-secure interrupt */
+				/* performance counter interrupts 0-7 */
+				     <0 211 4>,
+				     <0 212 4>,
+				     <0 213 4>,
+				     <0 214 4>,
+				     <0 215 4>,
+				     <0 216 4>,
+				     <0 217 4>,
+				     <0 218 4>,
+				/* per context interrupt, 64 interrupts */
+				     <0 146 4>,
+				     <0 147 4>,
+				     <0 148 4>,
+				     <0 149 4>,
+				     <0 150 4>,
+				     <0 151 4>,
+				     <0 152 4>,
+				     <0 153 4>,
+				     <0 154 4>,
+				     <0 155 4>,
+				     <0 156 4>,
+				     <0 157 4>,
+				     <0 158 4>,
+				     <0 159 4>,
+				     <0 160 4>,
+				     <0 161 4>,
+				     <0 162 4>,
+				     <0 163 4>,
+				     <0 164 4>,
+				     <0 165 4>,
+				     <0 166 4>,
+				     <0 167 4>,
+				     <0 168 4>,
+				     <0 169 4>,
+				     <0 170 4>,
+				     <0 171 4>,
+				     <0 172 4>,
+				     <0 173 4>,
+				     <0 174 4>,
+				     <0 175 4>,
+				     <0 176 4>,
+				     <0 177 4>,
+				     <0 178 4>,
+				     <0 179 4>,
+				     <0 180 4>,
+				     <0 181 4>,
+				     <0 182 4>,
+				     <0 183 4>,
+				     <0 184 4>,
+				     <0 185 4>,
+				     <0 186 4>,
+				     <0 187 4>,
+				     <0 188 4>,
+				     <0 189 4>,
+				     <0 190 4>,
+				     <0 191 4>,
+				     <0 192 4>,
+				     <0 193 4>,
+				     <0 194 4>,
+				     <0 195 4>,
+				     <0 196 4>,
+				     <0 197 4>,
+				     <0 198 4>,
+				     <0 199 4>,
+				     <0 200 4>,
+				     <0 201 4>,
+				     <0 202 4>,
+				     <0 203 4>,
+				     <0 204 4>,
+				     <0 205 4>,
+				     <0 206 4>,
+				     <0 207 4>,
+				     <0 208 4>,
+				     <0 209 4>;
+		};
+
+		crypto: crypto@8000000 {
+			compatible = "fsl,sec-v5.0", "fsl,sec-v4.0";
+			fsl,sec-era = <8>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0x0 0x00 0x8000000 0x100000>;
+			reg = <0x00 0x8000000 0x0 0x100000>;
+			interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
+			dma-coherent;
+
+			sec_jr0: jr@10000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x10000 0x10000>;
+				interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr1: jr@20000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x20000 0x10000>;
+				interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr2: jr@30000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x30000 0x10000>;
+				interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr3: jr@40000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x40000 0x10000>;
+				interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+	};
+
+	firmware {
+		optee {
+			compatible = "linaro,optee-tz";
+			method = "smc";
+		};
+	};
+
+};
--- a/arch/arm64/boot/dts/freescale/fsl-ls2080a-qds.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2080a-qds.dts
@@ -1,214 +1,87 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 /*
  * Device Tree file for Freescale LS2080a QDS Board.
  *
- * Copyright (C) 2015, Freescale Semiconductor
+ * Copyright 2015-2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
  *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
  * Bhupesh Sharma <bhupesh.sharma@freescale.com>
  *
- * This file is dual-licensed: you can use it either under the terms
- * of the GPLv2 or the X11 license, at your option. Note that this dual
- * licensing only applies to this file, and not this project as a
- * whole.
- *
- *  a) This library is free software; you can redistribute it and/or
- *     modify it under the terms of the GNU General Public License as
- *     published by the Free Software Foundation; either version 2 of the
- *     License, or (at your option) any later version.
- *
- *     This library is distributed in the hope that it will be useful,
- *     but WITHOUT ANY WARRANTY; without even the implied warranty of
- *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- *     GNU General Public License for more details.
- *
- * Or, alternatively,
- *
- *  b) Permission is hereby granted, free of charge, to any person
- *     obtaining a copy of this software and associated documentation
- *     files (the "Software"), to deal in the Software without
- *     restriction, including without limitation the rights to use,
- *     copy, modify, merge, publish, distribute, sublicense, and/or
- *     sell copies of the Software, and to permit persons to whom the
- *     Software is furnished to do so, subject to the following
- *     conditions:
- *
- *     The above copyright notice and this permission notice shall be
- *     included in all copies or substantial portions of the Software.
- *
- *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
- *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
- *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
- *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
- *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
- *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
- *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
- *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
 /dts-v1/;
 
-/include/ "fsl-ls2080a.dtsi"
+#include "fsl-ls2080a.dtsi"
+#include "fsl-ls208xa-qds.dtsi"
 
 / {
 	model = "Freescale Layerscape 2080a QDS Board";
 	compatible = "fsl,ls2080a-qds", "fsl,ls2080a";
 
-	aliases {
-		serial0 = &serial0;
-		serial1 = &serial1;
-	};
-
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
 };
 
-&esdhc {
-	status = "okay";
-};
-
 &ifc {
-	status = "okay";
-	#address-cells = <2>;
-	#size-cells = <1>;
-	ranges = <0x0 0x0 0x5 0x80000000 0x08000000
-		  0x2 0x0 0x5 0x30000000 0x00010000
-		  0x3 0x0 0x5 0x20000000 0x00010000>;
-
-	nor@0,0 {
+	boardctrl: board-control@3,0 {
 		#address-cells = <1>;
 		#size-cells = <1>;
-		compatible = "cfi-flash";
-		reg = <0x0 0x0 0x8000000>;
-		bank-width = <2>;
-		device-width = <1>;
-	};
-
-	nand@2,0 {
-	     compatible = "fsl,ifc-nand";
-	     reg = <0x2 0x0 0x10000>;
-	};
+		compatible = "fsl,tetra-fpga", "fsl,fpga-qixis", "simple-bus";
+		reg = <3 0 0x300>;		/* TODO check address */
+		ranges = <0 3 0 0x300>;
 
-	cpld@3,0 {
-	     reg = <0x3 0x0 0x10000>;
-	     compatible = "fsl,ls2080aqds-fpga", "fsl,fpga-qixis";
-	};
-};
-
-&i2c0 {
-	status = "okay";
-	pca9547@77 {
-		compatible = "nxp,pca9547";
-		reg = <0x77>;
-		#address-cells = <1>;
-		#size-cells = <0>;
-		i2c@0 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x00>;
-			rtc@68 {
-				compatible = "dallas,ds3232";
-				reg = <0x68>;
-			};
-		};
-
-		i2c@2 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x02>;
-
-			ina220@40 {
-				compatible = "ti,ina220";
-				reg = <0x40>;
-				shunt-resistor = <500>;
-			};
-
-			ina220@41 {
-				compatible = "ti,ina220";
-				reg = <0x41>;
-				shunt-resistor = <1000>;
-			};
-		};
+		mdio_mux_emi1 {
+			compatible = "mdio-mux-mmioreg", "mdio-mux";
+			mdio-parent-bus = <&emdio1>;
+			reg = <0x54 1>;		/* BRDCFG4 */
+			mux-mask = <0xe0>;	/* EMI1_MDIO */
 
-		i2c@3 {
-			#address-cells = <1>;
+			#address-cells=<1>;
 			#size-cells = <0>;
-			reg = <0x3>;
 
-			adt7481@4c {
-				compatible = "adi,adt7461";
-				reg = <0x4c>;
+			/* Child MDIO buses, one for each riser card:
+			 * reg = 0x0, 0x20, 0x40, 0x60, 0x80, 0xa0.
+			 * VSC8234 PHYs on the riser cards.
+			 */
+
+			mdio_mux3: mdio@60 {
+				reg = <0x60>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				mdio0_phy12: mdio_phy0@1c {
+					reg = <0x1c>;
+					phy-connection-type = "sgmii";
+				};
+				mdio0_phy13: mdio_phy1@1d {
+					reg = <0x1d>;
+					phy-connection-type = "sgmii";
+				};
+				mdio0_phy14: mdio_phy2@1e {
+					reg = <0x1e>;
+					phy-connection-type = "sgmii";
+				};
+				mdio0_phy15: mdio_phy3@1f {
+					reg = <0x1f>;
+					phy-connection-type = "sgmii";
+				};
 			};
 		};
 	};
 };
 
-&i2c1 {
-	status = "disabled";
+/* Update DPMAC connections to external PHYs, under SerDes 0x2a_0x49. */
+&dpmac9 {
+	phy-handle = <&mdio0_phy12>;
 };
-
-&i2c2 {
-	status = "disabled";
-};
-
-&i2c3 {
-	status = "disabled";
-};
-
-&dspi {
-	status = "okay";
-	dflash0: n25q128a {
-		#address-cells = <1>;
-		#size-cells = <1>;
-		compatible = "st,m25p80";
-		spi-max-frequency = <3000000>;
-		reg = <0>;
-	};
-	dflash1: sst25wf040b {
-		#address-cells = <1>;
-		#size-cells = <1>;
-		compatible = "st,m25p80";
-		spi-max-frequency = <3000000>;
-		reg = <1>;
-	};
-	dflash2: en25s64 {
-		#address-cells = <1>;
-		#size-cells = <1>;
-		compatible = "st,m25p80";
-		spi-max-frequency = <3000000>;
-		reg = <2>;
-	};
+&dpmac10 {
+	phy-handle = <&mdio0_phy13>;
 };
-
-&qspi {
-	status = "okay";
-	flash0: s25fl256s1@0 {
-		#address-cells = <1>;
-		#size-cells = <1>;
-		compatible = "st,m25p80";
-		spi-max-frequency = <20000000>;
-		reg = <0>;
-	};
-	flash2: s25fl256s1@2 {
-		#address-cells = <1>;
-		#size-cells = <1>;
-		compatible = "st,m25p80";
-		spi-max-frequency = <20000000>;
-		reg = <0>;
-	};
+&dpmac11 {
+	phy-handle = <&mdio0_phy14>;
 };
-
-&sata0 {
-	status = "okay";
-};
-
-&sata1 {
-	status = "okay";
-};
-
-&usb0 {
-	status = "okay";
-};
-
-&usb1 {
-	status = "okay";
+&dpmac12 {
+	phy-handle = <&mdio0_phy15>;
 };
--- a/arch/arm64/boot/dts/freescale/fsl-ls2080a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2080a-rdb.dts
@@ -1,170 +1,105 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 /*
  * Device Tree file for Freescale LS2080a RDB Board.
  *
- * Copyright (C) 2015, Freescale Semiconductor
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
  *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
  * Bhupesh Sharma <bhupesh.sharma@freescale.com>
  *
- * This file is dual-licensed: you can use it either under the terms
- * of the GPLv2 or the X11 license, at your option. Note that this dual
- * licensing only applies to this file, and not this project as a
- * whole.
- *
- *  a) This library is free software; you can redistribute it and/or
- *     modify it under the terms of the GNU General Public License as
- *     published by the Free Software Foundation; either version 2 of the
- *     License, or (at your option) any later version.
- *
- *     This library is distributed in the hope that it will be useful,
- *     but WITHOUT ANY WARRANTY; without even the implied warranty of
- *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- *     GNU General Public License for more details.
- *
- * Or, alternatively,
- *
- *  b) Permission is hereby granted, free of charge, to any person
- *     obtaining a copy of this software and associated documentation
- *     files (the "Software"), to deal in the Software without
- *     restriction, including without limitation the rights to use,
- *     copy, modify, merge, publish, distribute, sublicense, and/or
- *     sell copies of the Software, and to permit persons to whom the
- *     Software is furnished to do so, subject to the following
- *     conditions:
- *
- *     The above copyright notice and this permission notice shall be
- *     included in all copies or substantial portions of the Software.
- *
- *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
- *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
- *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
- *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
- *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
- *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
- *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
- *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
 /dts-v1/;
 
-/include/ "fsl-ls2080a.dtsi"
+#include "fsl-ls2080a.dtsi"
+#include "fsl-ls208xa-rdb.dtsi"
 
 / {
 	model = "Freescale Layerscape 2080a RDB Board";
 	compatible = "fsl,ls2080a-rdb", "fsl,ls2080a";
 
-	aliases {
-		serial0 = &serial0;
-		serial1 = &serial1;
-	};
-
 	chosen {
 		stdout-path = "serial1:115200n8";
 	};
 };
 
-&esdhc {
-	status = "okay";
-};
-
-&ifc {
-	status = "okay";
-	#address-cells = <2>;
-	#size-cells = <1>;
-	ranges = <0x0 0x0 0x5 0x80000000 0x08000000
-		  0x2 0x0 0x5 0x30000000 0x00010000
-		  0x3 0x0 0x5 0x20000000 0x00010000>;
-
-	nor@0,0 {
-		#address-cells = <1>;
-		#size-cells = <1>;
-		compatible = "cfi-flash";
-		reg = <0x0 0x0 0x8000000>;
-		bank-width = <2>;
-		device-width = <1>;
-	};
-
-	nand@2,0 {
-	     compatible = "fsl,ifc-nand";
-	     reg = <0x2 0x0 0x10000>;
-	};
-
-	cpld@3,0 {
-	     reg = <0x3 0x0 0x10000>;
-	     compatible = "fsl,ls2080aqds-fpga", "fsl,fpga-qixis";
-	};
-
-};
-
-&i2c0 {
-	status = "okay";
-	pca9547@75 {
-		compatible = "nxp,pca9547";
-		reg = <0x75>;
-		#address-cells = <1>;
-		#size-cells = <0>;
-		status = "disabled";
-		i2c@1 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x01>;
-			rtc@68 {
-				compatible = "dallas,ds3232";
-				reg = <0x68>;
-			};
-		};
-
-		i2c@3 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x3>;
-
-			adt7481@4c {
-				compatible = "adi,adt7461";
-				reg = <0x4c>;
-			};
-		};
-	};
-};
-
-&i2c1 {
-	status = "disabled";
-};
-
-&i2c2 {
-	status = "disabled";
-};
-
-&i2c3 {
+&emdio1 {
 	status = "disabled";
+	/* CS4340 PHYs */
+	mdio1_phy1: emdio1_phy@1 {
+		reg = <0x10>;
+		phy-connection-type = "xfi";
+	};
+	mdio1_phy2: emdio1_phy@2 {
+		reg = <0x11>;
+		phy-connection-type = "xfi";
+	};
+	mdio1_phy3: emdio1_phy@3 {
+		reg = <0x12>;
+		phy-connection-type = "xfi";
+	};
+	mdio1_phy4: emdio1_phy@4 {
+		reg = <0x13>;
+		phy-connection-type = "xfi";
+	};
 };
 
-&dspi {
-	status = "okay";
-	dflash0: n25q512a {
-		#address-cells = <1>;
-		#size-cells = <1>;
-		compatible = "st,m25p80";
-		spi-max-frequency = <3000000>;
-		reg = <0>;
+&emdio2 {
+	/* AQR405 PHYs */
+	mdio2_phy1: emdio2_phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 1 0x4>; /* Level high type */
+		reg = <0x0>;
+		phy-connection-type = "xfi";
+	};
+	mdio2_phy2: emdio2_phy@2 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 2 0x4>; /* Level high type */
+		reg = <0x1>;
+		phy-connection-type = "xfi";
+	};
+	mdio2_phy3: emdio2_phy@3 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 4 0x4>; /* Level high type */
+		reg = <0x2>;
+		phy-connection-type = "xfi";
+	};
+	mdio2_phy4: emdio2_phy@4 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 5 0x4>; /* Level high type */
+		reg = <0x3>;
+		phy-connection-type = "xfi";
 	};
 };
 
-&qspi {
-	status = "disabled";
-};
+/* Update DPMAC connections to external PHYs, under the assumption of
+ * SerDes 0x2a_0x41. This is currently the only SerDes supported on the board.
+ */
+/* Leave Cortina nodes commented out until driver is integrated
+ *&dpmac1 {
+ *	phy-handle = <&mdio1_phy1>;
+ *};
+ *&dpmac2 {
+ *	phy-handle = <&mdio1_phy2>;
+ *};
+ *&dpmac3 {
+ *	phy-handle = <&mdio1_phy3>;
+ *};
+ *&dpmac4 {
+ *	phy-handle = <&mdio1_phy4>;
+ *};
+ */
 
-&sata0 {
-	status = "okay";
+&dpmac5 {
+	phy-handle = <&mdio2_phy1>;
 };
-
-&sata1 {
-	status = "okay";
+&dpmac6 {
+	phy-handle = <&mdio2_phy2>;
 };
-
-&usb0 {
-	status = "okay";
+&dpmac7 {
+	phy-handle = <&mdio2_phy3>;
 };
-
-&usb1 {
-	status = "okay";
+&dpmac8 {
+	phy-handle = <&mdio2_phy4>;
 };
--- a/arch/arm64/boot/dts/freescale/fsl-ls2080a-simu.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2080a-simu.dts
@@ -1,62 +1,21 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 /*
  * Device Tree file for Freescale LS2080a software Simulator model
  *
- * Copyright (C) 2014-2015, Freescale Semiconductor
+ * Copyright 2014-2015 Freescale Semiconductor, Inc.
  *
  * Bhupesh Sharma <bhupesh.sharma@freescale.com>
  *
- * This file is dual-licensed: you can use it either under the terms
- * of the GPL or the X11 license, at your option. Note that this dual
- * licensing only applies to this file, and not this project as a
- * whole.
- *
- *  a) This library is free software; you can redistribute it and/or
- *     modify it under the terms of the GNU General Public License as
- *     published by the Free Software Foundation; either version 2 of the
- *     License, or (at your option) any later version.
- *
- *     This library is distributed in the hope that it will be useful,
- *     but WITHOUT ANY WARRANTY; without even the implied warranty of
- *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- *     GNU General Public License for more details.
- *
- * Or, alternatively,
- *
- *  b) Permission is hereby granted, free of charge, to any person
- *     obtaining a copy of this software and associated documentation
- *     files (the "Software"), to deal in the Software without
- *     restriction, including without limitation the rights to use,
- *     copy, modify, merge, publish, distribute, sublicense, and/or
- *     sell copies of the Software, and to permit persons to whom the
- *     Software is furnished to do so, subject to the following
- *     conditions:
- *
- *     The above copyright notice and this permission notice shall be
- *     included in all copies or substantial portions of the Software.
- *
- *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
- *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
- *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
- *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
- *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
- *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
- *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
- *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
 /dts-v1/;
 
-/include/ "fsl-ls2080a.dtsi"
+#include "fsl-ls2080a.dtsi"
 
 / {
 	model = "Freescale Layerscape 2080a software Simulator model";
 	compatible = "fsl,ls2080a-simu", "fsl,ls2080a";
 
-	aliases {
-		serial0 = &serial0;
-		serial1 = &serial1;
-	};
-
 	ethernet@2210000 {
 		compatible = "smsc,lan91c111";
 		reg = <0x0 0x2210000 0x0 0x100>;
--- a/arch/arm64/boot/dts/freescale/fsl-ls2080a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2080a.dtsi
@@ -1,739 +1,144 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 /*
  * Device Tree Include file for Freescale Layerscape-2080A family SoC.
  *
- * Copyright (C) 2014-2015, Freescale Semiconductor
+ * Copyright 2014-2016 Freescale Semiconductor, Inc.
  *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
  * Bhupesh Sharma <bhupesh.sharma@freescale.com>
  *
- * This file is dual-licensed: you can use it either under the terms
- * of the GPLv2 or the X11 license, at your option. Note that this dual
- * licensing only applies to this file, and not this project as a
- * whole.
- *
- *  a) This library is free software; you can redistribute it and/or
- *     modify it under the terms of the GNU General Public License as
- *     published by the Free Software Foundation; either version 2 of the
- *     License, or (at your option) any later version.
- *
- *     This library is distributed in the hope that it will be useful,
- *     but WITHOUT ANY WARRANTY; without even the implied warranty of
- *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- *     GNU General Public License for more details.
- *
- * Or, alternatively,
- *
- *  b) Permission is hereby granted, free of charge, to any person
- *     obtaining a copy of this software and associated documentation
- *     files (the "Software"), to deal in the Software without
- *     restriction, including without limitation the rights to use,
- *     copy, modify, merge, publish, distribute, sublicense, and/or
- *     sell copies of the Software, and to permit persons to whom the
- *     Software is furnished to do so, subject to the following
- *     conditions:
- *
- *     The above copyright notice and this permission notice shall be
- *     included in all copies or substantial portions of the Software.
- *
- *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
- *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
- *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
- *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
- *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
- *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
- *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
- *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
-/ {
-	compatible = "fsl,ls2080a";
-	interrupt-parent = <&gic>;
-	#address-cells = <2>;
-	#size-cells = <2>;
-
-	cpus {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
-		/*
-		 * We expect the enable-method for cpu's to be "psci", but this
-		 * is dependent on the SoC FW, which will fill this in.
-		 *
-		 * Currently supported enable-method is psci v0.2
-		 */
-
-		/* We have 4 clusters having 2 Cortex-A57 cores each */
-		cpu@0 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x0>;
-			clocks = <&clockgen 1 0>;
-			next-level-cache = <&cluster0_l2>;
-		};
-
-		cpu@1 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x1>;
-			clocks = <&clockgen 1 0>;
-			next-level-cache = <&cluster0_l2>;
-		};
-
-		cpu@100 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x100>;
-			clocks = <&clockgen 1 1>;
-			next-level-cache = <&cluster1_l2>;
-		};
-
-		cpu@101 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x101>;
-			clocks = <&clockgen 1 1>;
-			next-level-cache = <&cluster1_l2>;
-		};
-
-		cpu@200 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x200>;
-			clocks = <&clockgen 1 2>;
-			next-level-cache = <&cluster2_l2>;
-		};
-
-		cpu@201 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x201>;
-			clocks = <&clockgen 1 2>;
-			next-level-cache = <&cluster2_l2>;
-		};
-
-		cpu@300 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x300>;
-			clocks = <&clockgen 1 3>;
-			next-level-cache = <&cluster3_l2>;
-		};
-
-		cpu@301 {
-			device_type = "cpu";
-			compatible = "arm,cortex-a57";
-			reg = <0x301>;
-			clocks = <&clockgen 1 3>;
-			next-level-cache = <&cluster3_l2>;
-		};
-
-		cluster0_l2: l2-cache0 {
-			compatible = "cache";
-		};
-
-		cluster1_l2: l2-cache1 {
-			compatible = "cache";
-		};
-
-		cluster2_l2: l2-cache2 {
-			compatible = "cache";
-		};
-
-		cluster3_l2: l2-cache3 {
-			compatible = "cache";
-		};
-	};
-
-	memory@80000000 {
-		device_type = "memory";
-		reg = <0x00000000 0x80000000 0 0x80000000>;
-		      /* DRAM space - 1, size : 2 GB DRAM */
-	};
-
-	sysclk: sysclk {
-		compatible = "fixed-clock";
-		#clock-cells = <0>;
-		clock-frequency = <100000000>;
-		clock-output-names = "sysclk";
-	};
-
-	gic: interrupt-controller@6000000 {
-		compatible = "arm,gic-v3";
-		reg = <0x0 0x06000000 0 0x10000>, /* GIC Dist */
-			<0x0 0x06100000 0 0x100000>, /* GICR (RD_base + SGI_base) */
-			<0x0 0x0c0c0000 0 0x2000>, /* GICC */
-			<0x0 0x0c0d0000 0 0x1000>, /* GICH */
-			<0x0 0x0c0e0000 0 0x20000>; /* GICV */
-		#interrupt-cells = <3>;
-		#address-cells = <2>;
-		#size-cells = <2>;
-		ranges;
-		interrupt-controller;
-		interrupts = <1 9 0x4>;
-
-		its: gic-its@6020000 {
-			compatible = "arm,gic-v3-its";
-			msi-controller;
-			reg = <0x0 0x6020000 0 0x20000>;
-		};
-	};
-
-	rstcr: syscon@1e60000 {
-		compatible = "fsl,ls2080a-rstcr", "syscon";
-		reg = <0x0 0x1e60000 0x0 0x4>;
-	};
-
-	reboot {
-		compatible ="syscon-reboot";
-		regmap = <&rstcr>;
-		offset = <0x0>;
-		mask = <0x2>;
-	};
-
-	timer {
-		compatible = "arm,armv8-timer";
-		interrupts = <1 13 4>, /* Physical Secure PPI, active-low */
-			     <1 14 4>, /* Physical Non-Secure PPI, active-low */
-			     <1 11 4>, /* Virtual PPI, active-low */
-			     <1 10 4>; /* Hypervisor PPI, active-low */
-		fsl,erratum-a008585;
-	};
-
-	pmu {
-		compatible = "arm,armv8-pmuv3";
-		interrupts = <1 7 0x8>; /* PMU PPI, Level low type */
-	};
-
-	soc {
-		compatible = "simple-bus";
-		#address-cells = <2>;
-		#size-cells = <2>;
-		ranges;
-
-		clockgen: clocking@1300000 {
-			compatible = "fsl,ls2080a-clockgen";
-			reg = <0 0x1300000 0 0xa0000>;
-			#clock-cells = <2>;
-			clocks = <&sysclk>;
-		};
-
-		serial0: serial@21c0500 {
-			compatible = "fsl,ns16550", "ns16550a";
-			reg = <0x0 0x21c0500 0x0 0x100>;
-			clocks = <&clockgen 4 3>;
-			interrupts = <0 32 0x4>; /* Level high type */
-		};
-
-		serial1: serial@21c0600 {
-			compatible = "fsl,ns16550", "ns16550a";
-			reg = <0x0 0x21c0600 0x0 0x100>;
-			clocks = <&clockgen 4 3>;
-			interrupts = <0 32 0x4>; /* Level high type */
-		};
-
-		cluster1_core0_watchdog: wdt@c000000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc000000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		cluster1_core1_watchdog: wdt@c010000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc010000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		cluster2_core0_watchdog: wdt@c100000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc100000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		cluster2_core1_watchdog: wdt@c110000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc110000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		cluster3_core0_watchdog: wdt@c200000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc200000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		cluster3_core1_watchdog: wdt@c210000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc210000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		cluster4_core0_watchdog: wdt@c300000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc300000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		cluster4_core1_watchdog: wdt@c310000 {
-			compatible = "arm,sp805-wdt", "arm,primecell";
-			reg = <0x0 0xc310000 0x0 0x1000>;
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "apb_pclk", "wdog_clk";
-		};
-
-		fsl_mc: fsl-mc@80c000000 {
-			compatible = "fsl,qoriq-mc";
-			reg = <0x00000008 0x0c000000 0 0x40>,	 /* MC portal base */
-			      <0x00000000 0x08340000 0 0x40000>; /* MC control reg */
-			msi-parent = <&its>;
-			#address-cells = <3>;
-			#size-cells = <1>;
-
-			/*
-			 * Region type 0x0 - MC portals
-			 * Region type 0x1 - QBMAN portals
-			 */
-			ranges = <0x0 0x0 0x0 0x8 0x0c000000 0x4000000
-				  0x1 0x0 0x0 0x8 0x18000000 0x8000000>;
-
-			/*
-			 * Define the maximum number of MACs present on the SoC.
-			 */
-			dpmacs {
-				#address-cells = <1>;
-				#size-cells = <0>;
-
-				dpmac1: dpmac@1 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x1>;
-				};
-
-				dpmac2: dpmac@2 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x2>;
-				};
-
-				dpmac3: dpmac@3 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x3>;
-				};
-
-				dpmac4: dpmac@4 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x4>;
-				};
-
-				dpmac5: dpmac@5 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x5>;
-				};
-
-				dpmac6: dpmac@6 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x6>;
-				};
-
-				dpmac7: dpmac@7 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x7>;
-				};
-
-				dpmac8: dpmac@8 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x8>;
-				};
-
-				dpmac9: dpmac@9 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x9>;
-				};
-
-				dpmac10: dpmac@a {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0xa>;
-				};
-
-				dpmac11: dpmac@b {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0xb>;
-				};
-
-				dpmac12: dpmac@c {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0xc>;
-				};
-
-				dpmac13: dpmac@d {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0xd>;
-				};
-
-				dpmac14: dpmac@e {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0xe>;
-				};
-
-				dpmac15: dpmac@f {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0xf>;
-				};
-
-				dpmac16: dpmac@10 {
-					compatible = "fsl,qoriq-mc-dpmac";
-					reg = <0x10>;
-				};
-			};
-		};
-
-		smmu: iommu@5000000 {
-			compatible = "arm,mmu-500";
-			reg = <0 0x5000000 0 0x800000>;
-			#global-interrupts = <12>;
-			interrupts = <0 13 4>, /* global secure fault */
-				     <0 14 4>, /* combined secure interrupt */
-				     <0 15 4>, /* global non-secure fault */
-				     <0 16 4>, /* combined non-secure interrupt */
-				/* performance counter interrupts 0-7 */
-				     <0 211 4>, <0 212 4>,
-				     <0 213 4>, <0 214 4>,
-				     <0 215 4>, <0 216 4>,
-				     <0 217 4>, <0 218 4>,
-				/* per context interrupt, 64 interrupts */
-				     <0 146 4>, <0 147 4>,
-				     <0 148 4>, <0 149 4>,
-				     <0 150 4>, <0 151 4>,
-				     <0 152 4>, <0 153 4>,
-				     <0 154 4>, <0 155 4>,
-				     <0 156 4>, <0 157 4>,
-				     <0 158 4>, <0 159 4>,
-				     <0 160 4>, <0 161 4>,
-				     <0 162 4>, <0 163 4>,
-				     <0 164 4>, <0 165 4>,
-				     <0 166 4>, <0 167 4>,
-				     <0 168 4>, <0 169 4>,
-				     <0 170 4>, <0 171 4>,
-				     <0 172 4>, <0 173 4>,
-				     <0 174 4>, <0 175 4>,
-				     <0 176 4>, <0 177 4>,
-				     <0 178 4>, <0 179 4>,
-				     <0 180 4>, <0 181 4>,
-				     <0 182 4>, <0 183 4>,
-				     <0 184 4>, <0 185 4>,
-				     <0 186 4>, <0 187 4>,
-				     <0 188 4>, <0 189 4>,
-				     <0 190 4>, <0 191 4>,
-				     <0 192 4>, <0 193 4>,
-				     <0 194 4>, <0 195 4>,
-				     <0 196 4>, <0 197 4>,
-				     <0 198 4>, <0 199 4>,
-				     <0 200 4>, <0 201 4>,
-				     <0 202 4>, <0 203 4>,
-				     <0 204 4>, <0 205 4>,
-				     <0 206 4>, <0 207 4>,
-				     <0 208 4>, <0 209 4>;
-			mmu-masters = <&fsl_mc 0x300 0>;
-		};
-
-		dspi: dspi@2100000 {
-			status = "disabled";
-			compatible = "fsl,ls2080a-dspi", "fsl,ls2085a-dspi";
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x0 0x2100000 0x0 0x10000>;
-			interrupts = <0 26 0x4>; /* Level high type */
-			clocks = <&clockgen 4 3>;
-			clock-names = "dspi";
-			spi-num-chipselects = <5>;
-			bus-num = <0>;
-		};
-
-		esdhc: esdhc@2140000 {
-			status = "disabled";
-			compatible = "fsl,ls2080a-esdhc", "fsl,esdhc";
-			reg = <0x0 0x2140000 0x0 0x10000>;
-			interrupts = <0 28 0x4>; /* Level high type */
-			clock-frequency = <0>;	/* Updated by bootloader */
-			voltage-ranges = <1800 1800 3300 3300>;
-			sdhci,auto-cmd12;
-			little-endian;
-			bus-width = <4>;
-		};
-
-		gpio0: gpio@2300000 {
-			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
-			reg = <0x0 0x2300000 0x0 0x10000>;
-			interrupts = <0 36 0x4>; /* Level high type */
-			gpio-controller;
-			little-endian;
-			#gpio-cells = <2>;
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		gpio1: gpio@2310000 {
-			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
-			reg = <0x0 0x2310000 0x0 0x10000>;
-			interrupts = <0 36 0x4>; /* Level high type */
-			gpio-controller;
-			little-endian;
-			#gpio-cells = <2>;
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		gpio2: gpio@2320000 {
-			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
-			reg = <0x0 0x2320000 0x0 0x10000>;
-			interrupts = <0 37 0x4>; /* Level high type */
-			gpio-controller;
-			little-endian;
-			#gpio-cells = <2>;
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		gpio3: gpio@2330000 {
-			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
-			reg = <0x0 0x2330000 0x0 0x10000>;
-			interrupts = <0 37 0x4>; /* Level high type */
-			gpio-controller;
-			little-endian;
-			#gpio-cells = <2>;
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		i2c0: i2c@2000000 {
-			status = "disabled";
-			compatible = "fsl,vf610-i2c";
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x0 0x2000000 0x0 0x10000>;
-			interrupts = <0 34 0x4>; /* Level high type */
-			clock-names = "i2c";
-			clocks = <&clockgen 4 3>;
-		};
-
-		i2c1: i2c@2010000 {
-			status = "disabled";
-			compatible = "fsl,vf610-i2c";
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x0 0x2010000 0x0 0x10000>;
-			interrupts = <0 34 0x4>; /* Level high type */
-			clock-names = "i2c";
-			clocks = <&clockgen 4 3>;
-		};
-
-		i2c2: i2c@2020000 {
-			status = "disabled";
-			compatible = "fsl,vf610-i2c";
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x0 0x2020000 0x0 0x10000>;
-			interrupts = <0 35 0x4>; /* Level high type */
-			clock-names = "i2c";
-			clocks = <&clockgen 4 3>;
-		};
-
-		i2c3: i2c@2030000 {
-			status = "disabled";
-			compatible = "fsl,vf610-i2c";
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x0 0x2030000 0x0 0x10000>;
-			interrupts = <0 35 0x4>; /* Level high type */
-			clock-names = "i2c";
-			clocks = <&clockgen 4 3>;
-		};
-
-		ifc: ifc@2240000 {
-			compatible = "fsl,ifc", "simple-bus";
-			reg = <0x0 0x2240000 0x0 0x20000>;
-			interrupts = <0 21 0x4>; /* Level high type */
-			little-endian;
-			#address-cells = <2>;
-			#size-cells = <1>;
-
-			ranges = <0 0 0x5 0x80000000 0x08000000
-				  2 0 0x5 0x30000000 0x00010000
-				  3 0 0x5 0x20000000 0x00010000>;
-		};
-
-		qspi: quadspi@20c0000 {
-			status = "disabled";
-			compatible = "fsl,ls2080a-qspi", "fsl,ls1021a-qspi";
-			#address-cells = <1>;
-			#size-cells = <0>;
-			reg = <0x0 0x20c0000 0x0 0x10000>,
-			      <0x0 0x20000000 0x0 0x10000000>;
-			reg-names = "QuadSPI", "QuadSPI-memory";
-			interrupts = <0 25 0x4>; /* Level high type */
-			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
-			clock-names = "qspi_en", "qspi";
-		};
-
-		pcie@3400000 {
-			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
-				     "snps,dw-pcie";
-			reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
-			       0x10 0x00000000 0x0 0x00002000>; /* configuration space */
-			reg-names = "regs", "config";
-			interrupts = <0 108 0x4>; /* Level high type */
-			interrupt-names = "intr";
-			#address-cells = <3>;
-			#size-cells = <2>;
-			device_type = "pci";
-			dma-coherent;
-			num-lanes = <4>;
-			bus-range = <0x0 0xff>;
-			ranges = <0x81000000 0x0 0x00000000 0x10 0x00010000 0x0 0x00010000   /* downstream I/O */
-				  0x82000000 0x0 0x40000000 0x10 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&its>;
-			#interrupt-cells = <1>;
-			interrupt-map-mask = <0 0 0 7>;
-			interrupt-map = <0000 0 0 1 &gic 0 0 0 109 4>,
-					<0000 0 0 2 &gic 0 0 0 110 4>,
-					<0000 0 0 3 &gic 0 0 0 111 4>,
-					<0000 0 0 4 &gic 0 0 0 112 4>;
-		};
-
-		pcie@3500000 {
-			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
-				     "snps,dw-pcie";
-			reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
-			       0x12 0x00000000 0x0 0x00002000>; /* configuration space */
-			reg-names = "regs", "config";
-			interrupts = <0 113 0x4>; /* Level high type */
-			interrupt-names = "intr";
-			#address-cells = <3>;
-			#size-cells = <2>;
-			device_type = "pci";
-			dma-coherent;
-			num-lanes = <4>;
-			bus-range = <0x0 0xff>;
-			ranges = <0x81000000 0x0 0x00000000 0x12 0x00010000 0x0 0x00010000   /* downstream I/O */
-				  0x82000000 0x0 0x40000000 0x12 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&its>;
-			#interrupt-cells = <1>;
-			interrupt-map-mask = <0 0 0 7>;
-			interrupt-map = <0000 0 0 1 &gic 0 0 0 114 4>,
-					<0000 0 0 2 &gic 0 0 0 115 4>,
-					<0000 0 0 3 &gic 0 0 0 116 4>,
-					<0000 0 0 4 &gic 0 0 0 117 4>;
-		};
-
-		pcie@3600000 {
-			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
-				     "snps,dw-pcie";
-			reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
-			       0x14 0x00000000 0x0 0x00002000>; /* configuration space */
-			reg-names = "regs", "config";
-			interrupts = <0 118 0x4>; /* Level high type */
-			interrupt-names = "intr";
-			#address-cells = <3>;
-			#size-cells = <2>;
-			device_type = "pci";
-			dma-coherent;
-			num-lanes = <8>;
-			bus-range = <0x0 0xff>;
-			ranges = <0x81000000 0x0 0x00000000 0x14 0x00010000 0x0 0x00010000   /* downstream I/O */
-				  0x82000000 0x0 0x40000000 0x14 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&its>;
-			#interrupt-cells = <1>;
-			interrupt-map-mask = <0 0 0 7>;
-			interrupt-map = <0000 0 0 1 &gic 0 0 0 119 4>,
-					<0000 0 0 2 &gic 0 0 0 120 4>,
-					<0000 0 0 3 &gic 0 0 0 121 4>,
-					<0000 0 0 4 &gic 0 0 0 122 4>;
-		};
-
-		pcie@3700000 {
-			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
-				     "snps,dw-pcie";
-			reg = <0x00 0x03700000 0x0 0x00100000   /* controller registers */
-			       0x16 0x00000000 0x0 0x00002000>; /* configuration space */
-			reg-names = "regs", "config";
-			interrupts = <0 123 0x4>; /* Level high type */
-			interrupt-names = "intr";
-			#address-cells = <3>;
-			#size-cells = <2>;
-			device_type = "pci";
-			dma-coherent;
-			num-lanes = <4>;
-			bus-range = <0x0 0xff>;
-			ranges = <0x81000000 0x0 0x00000000 0x16 0x00010000 0x0 0x00010000   /* downstream I/O */
-				  0x82000000 0x0 0x40000000 0x16 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&its>;
-			#interrupt-cells = <1>;
-			interrupt-map-mask = <0 0 0 7>;
-			interrupt-map = <0000 0 0 1 &gic 0 0 0 124 4>,
-					<0000 0 0 2 &gic 0 0 0 125 4>,
-					<0000 0 0 3 &gic 0 0 0 126 4>,
-					<0000 0 0 4 &gic 0 0 0 127 4>;
-		};
-
-		sata0: sata@3200000 {
-			status = "disabled";
-			compatible = "fsl,ls2080a-ahci";
-			reg = <0x0 0x3200000 0x0 0x10000>;
-			interrupts = <0 133 0x4>; /* Level high type */
-			clocks = <&clockgen 4 3>;
-			dma-coherent;
-		};
-
-		sata1: sata@3210000 {
-			status = "disabled";
-			compatible = "fsl,ls2080a-ahci";
-			reg = <0x0 0x3210000 0x0 0x10000>;
-			interrupts = <0 136 0x4>; /* Level high type */
-			clocks = <&clockgen 4 3>;
-			dma-coherent;
-		};
-
-		usb0: usb3@3100000 {
-			status = "disabled";
-			compatible = "snps,dwc3";
-			reg = <0x0 0x3100000 0x0 0x10000>;
-			interrupts = <0 80 0x4>; /* Level high type */
-			dr_mode = "host";
-			snps,quirk-frame-length-adjustment = <0x20>;
-			snps,dis_rxdet_inp3_quirk;
-		};
-
-		usb1: usb3@3110000 {
-			status = "disabled";
-			compatible = "snps,dwc3";
-			reg = <0x0 0x3110000 0x0 0x10000>;
-			interrupts = <0 81 0x4>; /* Level high type */
-			dr_mode = "host";
-			snps,quirk-frame-length-adjustment = <0x20>;
-			snps,dis_rxdet_inp3_quirk;
-		};
-
-		ccn@4000000 {
-			compatible = "arm,ccn-504";
-			reg = <0x0 0x04000000 0x0 0x01000000>;
-			interrupts = <0 12 4>;
-		};
-	};
-
-	ddr1: memory-controller@1080000 {
-		compatible = "fsl,qoriq-memory-controller";
-		reg = <0x0 0x1080000 0x0 0x1000>;
-		interrupts = <0 17 0x4>;
-		little-endian;
-	};
-
-	ddr2: memory-controller@1090000 {
-		compatible = "fsl,qoriq-memory-controller";
-		reg = <0x0 0x1090000 0x0 0x1000>;
-		interrupts = <0 18 0x4>;
-		little-endian;
+#include "fsl-ls208xa.dtsi"
+
+&cpu {
+	cpu0: cpu@0 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x0>;
+		clocks = <&clockgen 1 0>;
+		next-level-cache = <&cluster0_l2>;
+		#cooling-cells = <2>;
+	};
+
+	cpu1: cpu@1 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x1>;
+		clocks = <&clockgen 1 0>;
+		next-level-cache = <&cluster0_l2>;
+	};
+
+	cpu2: cpu@100 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x100>;
+		clocks = <&clockgen 1 1>;
+		next-level-cache = <&cluster1_l2>;
+		#cooling-cells = <2>;
+	};
+
+	cpu3: cpu@101 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x101>;
+		clocks = <&clockgen 1 1>;
+		next-level-cache = <&cluster1_l2>;
+	};
+
+	cpu4: cpu@200 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x200>;
+		clocks = <&clockgen 1 2>;
+		next-level-cache = <&cluster2_l2>;
+		#cooling-cells = <2>;
+	};
+
+	cpu5: cpu@201 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x201>;
+		clocks = <&clockgen 1 2>;
+		next-level-cache = <&cluster2_l2>;
+	};
+
+	cpu6: cpu@300 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x300>;
+		clocks = <&clockgen 1 3>;
+		next-level-cache = <&cluster3_l2>;
+		#cooling-cells = <2>;
+	};
+
+	cpu7: cpu@301 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a57";
+		reg = <0x301>;
+		clocks = <&clockgen 1 3>;
+		next-level-cache = <&cluster3_l2>;
 	};
+
+	cluster0_l2: l2-cache0 {
+		compatible = "cache";
+	};
+
+	cluster1_l2: l2-cache1 {
+		compatible = "cache";
+	};
+
+	cluster2_l2: l2-cache2 {
+		compatible = "cache";
+	};
+
+	cluster3_l2: l2-cache3 {
+		compatible = "cache";
+	};
+};
+
+&usb0 {
+	snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+	snps,dma-snooping;
+};
+
+&usb1 {
+	snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+	snps,dma-snooping;
+};
+
+&timer {
+	fsl,erratum-a008585;
+};
+
+&pcie1 {
+	reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
+	       0x10 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x10 0x00010000 0x0 0x00010000   /* downstream I/O */
+		  0x82000000 0x0 0x40000000 0x10 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+};
+
+&pcie2 {
+	reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
+	       0x12 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x12 0x00010000 0x0 0x00010000   /* downstream I/O */
+		  0x82000000 0x0 0x40000000 0x12 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+};
+
+&pcie3 {
+	reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
+	       0x14 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x14 0x00010000 0x0 0x00010000   /* downstream I/O */
+		  0x82000000 0x0 0x40000000 0x14 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+};
+
+&pcie4 {
+	reg = <0x00 0x03700000 0x0 0x00100000   /* controller registers */
+	       0x16 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x16 0x00010000 0x0 0x00010000   /* downstream I/O */
+		  0x82000000 0x0 0x40000000 0x16 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
 };
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2081a-rdb.dts
@@ -0,0 +1,161 @@
+/*
+ * Device Tree file for NXP LS2081A RDB Board.
+ *
+ * Copyright 2017 NXP
+ *
+ * Priyanka Jain <priyanka.jain@nxp.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+
+#include "fsl-ls2088a.dtsi"
+
+/ {
+	model = "NXP Layerscape 2081A RDB Board";
+	compatible = "fsl,ls2081a-rdb", "fsl,ls2081a";
+
+	aliases {
+		serial0 = &serial0;
+		serial1 = &serial1;
+	};
+
+	chosen {
+		stdout-path = "serial1:115200n8";
+	};
+};
+
+&esdhc {
+	status = "okay";
+};
+
+&ifc {
+	status = "disabled";
+};
+
+&i2c0 {
+	status = "okay";
+	pca9547@75 {
+		compatible = "nxp,pca9547";
+		reg = <0x75>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		i2c@1 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x01>;
+			rtc@51 {
+				compatible = "nxp,pcf2129";
+				reg = <0x51>;
+			};
+		};
+
+		i2c@2 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x02>;
+
+			ina220@40 {
+				compatible = "ti,ina220";
+				reg = <0x40>;
+				shunt-resistor = <500>;
+			};
+		};
+
+		i2c@3 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x3>;
+
+			adt7481@4c {
+				compatible = "adi,adt7461";
+				reg = <0x4c>;
+			};
+		};
+	};
+};
+
+&dspi {
+	status = "okay";
+	dflash0: n25q512a {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "st,m25p80";
+		spi-max-frequency = <3000000>;
+		reg = <0>;
+	};
+};
+
+&qspi {
+	status = "okay";
+	fsl,qspi-has-second-chip;
+	flash0: s25fs512s@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "spansion,m25p80";
+		m25p,fast-read;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+	flash1: s25fs512s@1 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "spansion,m25p80";
+		m25p,fast-read;
+		spi-max-frequency = <20000000>;
+		reg = <1>;
+	};
+};
+
+&sata0 {
+	status = "okay";
+};
+
+&sata1 {
+	status = "okay";
+};
+
+&usb0 {
+	status = "okay";
+};
+
+&usb1 {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2088a-qds.dts
@@ -0,0 +1,126 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for Freescale LS2088A QDS Board.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
+ *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
+ *
+ */
+
+/dts-v1/;
+
+#include "fsl-ls2088a.dtsi"
+#include "fsl-ls208xa-qds.dtsi"
+
+/ {
+	model = "Freescale Layerscape 2088A QDS Board";
+	compatible = "fsl,ls2088a-qds", "fsl,ls2088a";
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+};
+
+&ifc {
+	boardctrl: board-control@3,0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "fsl,tetra-fpga", "fsl,fpga-qixis", "simple-bus";
+		reg = <3 0 0x300>;		/* TODO check address */
+		ranges = <0 3 0 0x300>;
+
+		mdio_mux_emi1 {
+			compatible = "mdio-mux-mmioreg", "mdio-mux";
+			mdio-parent-bus = <&emdio1>;
+			reg = <0x54 1>;		/* BRDCFG4 */
+			mux-mask = <0xe0>;	/* EMI1_MDIO */
+
+			#address-cells=<1>;
+			#size-cells = <0>;
+
+			/* Child MDIO buses, one for each riser card:
+			 * reg = 0x0, 0x20, 0x40, 0x60, 0x80, 0xa0.
+			 * VSC8234 PHYs on the riser cards.
+			 */
+
+			mdio_mux3: mdio@60 {
+				reg = <0x60>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				mdio0_phy12: mdio_phy0@1c {
+					reg = <0x1c>;
+					phy-connection-type = "sgmii";
+				};
+				mdio0_phy13: mdio_phy1@1d {
+					reg = <0x1d>;
+					phy-connection-type = "sgmii";
+				};
+				mdio0_phy14: mdio_phy2@1e {
+					reg = <0x1e>;
+					phy-connection-type = "sgmii";
+				};
+				mdio0_phy15: mdio_phy3@1f {
+					reg = <0x1f>;
+					phy-connection-type = "sgmii";
+				};
+			};
+		};
+	};
+};
+
+&pcs_mdio1 {
+		pcs_phy1: ethernet-phy@0 {
+		backplane-mode = "10gbase-kr";
+		compatible = "ethernet-phy-ieee802.3-c45";
+		reg = <0x0>;
+		fsl,lane-handle = <&serdes1>;
+		fsl,lane-reg = <0x9C0 0x40>;/* lane H */
+	};
+};
+
+&pcs_mdio2 {
+		pcs_phy2: ethernet-phy@0 {
+		backplane-mode = "10gbase-kr";
+		compatible = "ethernet-phy-ieee802.3-c45";
+		reg = <0x0>;
+		fsl,lane-handle = <&serdes1>;
+		fsl,lane-reg = <0x980 0x40>;/* lane G */
+	};
+};
+
+&pcs_mdio3 {
+		pcs_phy3: ethernet-phy@0 {
+		backplane-mode = "10gbase-kr";
+		compatible = "ethernet-phy-ieee802.3-c45";
+		reg = <0x0>;
+		fsl,lane-handle = <&serdes1>;
+		fsl,lane-reg = <0x940 0x40>;/* lane F */
+	};
+};
+
+&pcs_mdio4 {
+		pcs_phy4: ethernet-phy@0 {
+		backplane-mode = "10gbase-kr";
+		compatible = "ethernet-phy-ieee802.3-c45";
+		reg = <0x0>;
+		fsl,lane-handle = <&serdes1>;
+		fsl,lane-reg = <0x900 0x40>;/* lane E */
+	};
+};
+
+/* Update DPMAC connections to external PHYs, under SerDes 0x2a_0x49. */
+&dpmac9 {
+	phy-handle = <&mdio0_phy12>;
+};
+&dpmac10 {
+	phy-handle = <&mdio0_phy13>;
+};
+&dpmac11 {
+	phy-handle = <&mdio0_phy14>;
+};
+&dpmac12 {
+	phy-handle = <&mdio0_phy15>;
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2088a-rdb.dts
@@ -0,0 +1,104 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for Freescale LS2088A RDB Board.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
+ *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
+ *
+ */
+
+/dts-v1/;
+
+#include "fsl-ls2088a.dtsi"
+#include "fsl-ls208xa-rdb.dtsi"
+
+/ {
+	model = "Freescale Layerscape 2088A RDB Board";
+	compatible = "fsl,ls2088a-rdb", "fsl,ls2088a";
+
+	chosen {
+		stdout-path = "serial1:115200n8";
+	};
+};
+
+&emdio1 {
+	status = "disabled";
+	/* CS4340 PHYs */
+	mdio1_phy1: emdio1_phy@1 {
+		reg = <0x10>;
+		phy-connection-type = "xfi";
+	};
+	mdio1_phy2: emdio1_phy@2 {
+		reg = <0x11>;
+		phy-connection-type = "xfi";
+	};
+	mdio1_phy3: emdio1_phy@3 {
+		reg = <0x12>;
+		phy-connection-type = "xfi";
+	};
+	mdio1_phy4: emdio1_phy@4 {
+		reg = <0x13>;
+		phy-connection-type = "xfi";
+	};
+};
+
+&emdio2 {
+	/* AQR405 PHYs */
+	mdio2_phy1: emdio2_phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 1 0x4>; /* Level high type */
+		reg = <0x0>;
+		phy-connection-type = "xfi";
+	};
+	mdio2_phy2: emdio2_phy@2 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 2 0x4>; /* Level high type */
+		reg = <0x1>;
+		phy-connection-type = "xfi";
+	};
+	mdio2_phy3: emdio2_phy@3 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 4 0x4>; /* Level high type */
+		reg = <0x2>;
+		phy-connection-type = "xfi";
+	};
+	mdio2_phy4: emdio2_phy@4 {
+		compatible = "ethernet-phy-ieee802.3-c45";
+		interrupts = <0 5 0x4>; /* Level high type */
+		reg = <0x3>;
+		phy-connection-type = "xfi";
+	};
+};
+
+/* Update DPMAC connections to external PHYs, under the assumption of
+ * SerDes 0x2a_0x41. This is currently the only SerDes supported on the board.
+ */
+/* Leave Cortina PHYs commented out until proper driver is integrated
+ *&dpmac1 {
+ *	phy-handle = <&mdio1_phy1>;
+ *};
+ *&dpmac2 {
+ *	phy-handle = <&mdio1_phy2>;
+ *};
+ *&dpmac3 {
+ *	phy-handle = <&mdio1_phy3>;
+ *};
+ *&dpmac4 {
+ *	phy-handle = <&mdio1_phy4>;
+ *};
+ */
+
+&dpmac5 {
+	phy-handle = <&mdio2_phy1>;
+};
+&dpmac6 {
+	phy-handle = <&mdio2_phy2>;
+};
+&dpmac7 {
+	phy-handle = <&mdio2_phy3>;
+};
+&dpmac8 {
+	phy-handle = <&mdio2_phy4>;
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2088a.dtsi
@@ -0,0 +1,159 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Freescale Layerscape-2088A family SoC.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
+ *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
+ *
+ */
+
+#include "fsl-ls208xa.dtsi"
+
+&cpu {
+	cpu0: cpu@0 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x0>;
+		clocks = <&clockgen 1 0>;
+		next-level-cache = <&cluster0_l2>;
+		#cooling-cells = <2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	cpu1: cpu@1 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x1>;
+		clocks = <&clockgen 1 0>;
+		next-level-cache = <&cluster0_l2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	cpu2: cpu@100 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x100>;
+		clocks = <&clockgen 1 1>;
+		next-level-cache = <&cluster1_l2>;
+		#cooling-cells = <2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	cpu3: cpu@101 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x101>;
+		clocks = <&clockgen 1 1>;
+		next-level-cache = <&cluster1_l2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	cpu4: cpu@200 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x200>;
+		clocks = <&clockgen 1 2>;
+		next-level-cache = <&cluster2_l2>;
+		#cooling-cells = <2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	cpu5: cpu@201 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x201>;
+		clocks = <&clockgen 1 2>;
+		next-level-cache = <&cluster2_l2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	cpu6: cpu@300 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x300>;
+		clocks = <&clockgen 1 3>;
+		next-level-cache = <&cluster3_l2>;
+		#cooling-cells = <2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	cpu7: cpu@301 {
+		device_type = "cpu";
+		compatible = "arm,cortex-a72";
+		reg = <0x301>;
+		clocks = <&clockgen 1 3>;
+		next-level-cache = <&cluster3_l2>;
+		cpu-idle-states = <&CPU_PH20>;
+	};
+
+	idle-states {
+		/*
+		 * PSCI node is not added default, U-boot will add missing
+		 * parts if it determines to use PSCI.
+		 */
+		entry-method = "arm,psci";
+
+		CPU_PH20: cpu-ph20 {
+			compatible = "arm,idle-state";
+			idle-state-name = "PH20";
+			arm,psci-suspend-param = <0x0>;
+			entry-latency-us = <1000>;
+			exit-latency-us = <1000>;
+			min-residency-us = <3000>;
+		};
+	};
+
+	cluster0_l2: l2-cache0 {
+		compatible = "cache";
+	};
+
+	cluster1_l2: l2-cache1 {
+		compatible = "cache";
+	};
+
+	cluster2_l2: l2-cache2 {
+		compatible = "cache";
+	};
+
+	cluster3_l2: l2-cache3 {
+		compatible = "cache";
+	};
+};
+
+&pcie1 {
+	compatible = "fsl,ls2088a-pcie", "snps,dw-pcie";
+	reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
+	       0x20 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x20 0x00010000 0x0 0x00010000
+		  0x82000000 0x0 0x40000000 0x20 0x40000000 0x0 0x40000000>;
+};
+
+&pcie2 {
+	compatible = "fsl,ls2088a-pcie", "snps,dw-pcie";
+	reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
+	       0x28 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x28 0x00010000 0x0 0x00010000
+		  0x82000000 0x0 0x40000000 0x28 0x40000000 0x0 0x40000000>;
+};
+
+&pcie3 {
+	compatible = "fsl,ls2088a-pcie", "snps,dw-pcie";
+	reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
+	       0x30 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x30 0x00010000 0x0 0x00010000
+		  0x82000000 0x0 0x40000000 0x30 0x40000000 0x0 0x40000000>;
+};
+
+&pcie4 {
+	compatible = "fsl,ls2088a-pcie", "snps,dw-pcie";
+	reg = <0x00 0x03700000 0x0 0x00100000   /* controller registers */
+	       0x38 0x00000000 0x0 0x00002000>; /* configuration space */
+
+	ranges = <0x81000000 0x0 0x00000000 0x38 0x00010000 0x0 0x00010000
+		  0x82000000 0x0 0x40000000 0x38 0x40000000 0x0 0x40000000>;
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls208xa-qds.dtsi
@@ -0,0 +1,162 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for Freescale LS2080A QDS Board.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
+ *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
+ *
+ */
+
+&esdhc {
+	mmc-hs200-1_8v;
+	status = "okay";
+};
+
+&ifc {
+	status = "okay";
+	#address-cells = <2>;
+	#size-cells = <1>;
+	ranges = <0x0 0x0 0x5 0x80000000 0x08000000
+		  0x2 0x0 0x5 0x30000000 0x00010000
+		  0x3 0x0 0x5 0x20000000 0x00010000>;
+
+	nor@0,0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "cfi-flash";
+		reg = <0x0 0x0 0x8000000>;
+		bank-width = <2>;
+		device-width = <1>;
+	};
+
+	nand@2,0 {
+	     compatible = "fsl,ifc-nand";
+	     reg = <0x2 0x0 0x10000>;
+	};
+
+	cpld@3,0 {
+	     reg = <0x3 0x0 0x10000>;
+	     compatible = "fsl,ls2080aqds-fpga", "fsl,fpga-qixis";
+	};
+};
+
+&i2c0 {
+	status = "okay";
+	pca9547@77 {
+		compatible = "nxp,pca9547";
+		reg = <0x77>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		i2c@0 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x00>;
+			rtc@68 {
+				compatible = "dallas,ds3232";
+				reg = <0x68>;
+			};
+		};
+
+		i2c@2 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x02>;
+
+			ina220@40 {
+				compatible = "ti,ina220";
+				reg = <0x40>;
+				shunt-resistor = <500>;
+			};
+
+			ina220@41 {
+				compatible = "ti,ina220";
+				reg = <0x41>;
+				shunt-resistor = <1000>;
+			};
+		};
+
+		i2c@3 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x3>;
+
+			adt7481@4c {
+				compatible = "adi,adt7461";
+				reg = <0x4c>;
+			};
+		};
+	};
+};
+
+&i2c1 {
+	status = "disabled";
+};
+
+&i2c2 {
+	status = "disabled";
+};
+
+&i2c3 {
+	status = "disabled";
+};
+
+&dspi {
+	status = "okay";
+	dflash0: n25q128a {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "st,m25p80";
+		spi-max-frequency = <3000000>;
+		reg = <0>;
+	};
+	dflash1: sst25wf040b {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "st,m25p80";
+		spi-max-frequency = <3000000>;
+		reg = <1>;
+	};
+	dflash2: en25s64 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "st,m25p80";
+		spi-max-frequency = <3000000>;
+		reg = <2>;
+	};
+};
+
+&qspi {
+	status = "okay";
+	flash0: s25fl256s1@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "st,m25p80";
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+	flash2: s25fl256s1@2 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "st,m25p80";
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+};
+
+&sata0 {
+	status = "okay";
+};
+
+&sata1 {
+	status = "okay";
+};
+
+&usb0 {
+	status = "okay";
+};
+
+&usb1 {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls208xa-rdb.dtsi
@@ -0,0 +1,136 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree file for Freescale LS2080A RDB Board.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
+ *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
+ *
+ */
+
+&esdhc {
+	status = "okay";
+};
+
+&ifc {
+	status = "okay";
+	#address-cells = <2>;
+	#size-cells = <1>;
+	ranges = <0x0 0x0 0x5 0x80000000 0x08000000
+		  0x2 0x0 0x5 0x30000000 0x00010000
+		  0x3 0x0 0x5 0x20000000 0x00010000>;
+
+	nor@0,0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "cfi-flash";
+		reg = <0x0 0x0 0x8000000>;
+		bank-width = <2>;
+		device-width = <1>;
+	};
+
+	nand@2,0 {
+	     compatible = "fsl,ifc-nand";
+	     reg = <0x2 0x0 0x10000>;
+	};
+
+	cpld@3,0 {
+	     reg = <0x3 0x0 0x10000>;
+	     compatible = "fsl,ls2080aqds-fpga", "fsl,fpga-qixis";
+	};
+
+};
+
+&i2c0 {
+	status = "okay";
+	pca9547@75 {
+		compatible = "nxp,pca9547";
+		reg = <0x75>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		i2c-mux-never-disable;
+		i2c@1 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x01>;
+			rtc@68 {
+				compatible = "dallas,ds3232";
+				reg = <0x68>;
+			};
+		};
+
+		i2c@2 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x02>;
+			ina220@40 {
+				compatible = "ti,ina220";
+				reg = <0x40>;
+				shunt-resistor = <500>;
+			};
+		};
+
+		i2c@3 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x3>;
+
+			adt7481@4c {
+				compatible = "adi,adt7461";
+				reg = <0x4c>;
+			};
+		};
+	};
+};
+
+&i2c1 {
+	status = "disabled";
+};
+
+&i2c2 {
+	status = "disabled";
+};
+
+&i2c3 {
+	status = "disabled";
+};
+
+&dspi {
+	status = "okay";
+	dflash0: n25q512a {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "st,m25p80";
+		spi-max-frequency = <3000000>;
+		reg = <0>;
+	};
+};
+
+&qspi {
+	status = "okay";
+	flash0: s25fs512s@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "spansion,m25p80";
+		m25p,fast-read;
+		spi-max-frequency = <20000000>;
+		reg = <0>;
+	};
+};
+
+&sata0 {
+	status = "okay";
+};
+
+&sata1 {
+	status = "okay";
+};
+
+&usb0 {
+	status = "okay";
+};
+
+&usb1 {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
@@ -0,0 +1,885 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Freescale Layerscape-2080A family SoC.
+ *
+ * Copyright 2016 Freescale Semiconductor, Inc.
+ * Copyright 2017 NXP
+ *
+ * Abhimanyu Saini <abhimanyu.saini@nxp.com>
+ *
+ */
+
+#include <dt-bindings/thermal/thermal.h>
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+
+/ {
+	compatible = "fsl,ls2080a";
+	interrupt-parent = <&gic>;
+	#address-cells = <2>;
+	#size-cells = <2>;
+
+	aliases {
+		crypto = &crypto;
+		serial0 = &serial0;
+		serial1 = &serial1;
+	};
+
+	cpu: cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+	};
+
+	memory@80000000 {
+		device_type = "memory";
+		reg = <0x00000000 0x80000000 0 0x80000000>;
+		      /* DRAM space - 1, size : 2 GB DRAM */
+	};
+
+	sysclk: sysclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <100000000>;
+		clock-output-names = "sysclk";
+	};
+
+	gic: interrupt-controller@6000000 {
+		compatible = "arm,gic-v3";
+		reg = <0x0 0x06000000 0 0x10000>, /* GIC Dist */
+			<0x0 0x06100000 0 0x100000>, /* GICR (RD_base + SGI_base) */
+			<0x0 0x0c0c0000 0 0x2000>, /* GICC */
+			<0x0 0x0c0d0000 0 0x1000>, /* GICH */
+			<0x0 0x0c0e0000 0 0x20000>; /* GICV */
+		#interrupt-cells = <3>;
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		interrupt-controller;
+		interrupts = <1 9 0x4>;
+
+		its: gic-its@6020000 {
+			compatible = "arm,gic-v3-its";
+			msi-controller;
+			reg = <0x0 0x6020000 0 0x20000>;
+		};
+	};
+
+	rstcr: syscon@1e60000 {
+		compatible = "fsl,ls2080a-rstcr", "syscon";
+		reg = <0x0 0x1e60000 0x0 0x4>;
+	};
+
+	reboot {
+		compatible ="syscon-reboot";
+		regmap = <&rstcr>;
+		offset = <0x0>;
+		mask = <0x2>;
+	};
+
+	timer: timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <1 13 4>, /* Physical Secure PPI, active-low */
+			     <1 14 4>, /* Physical Non-Secure PPI, active-low */
+			     <1 11 4>, /* Virtual PPI, active-low */
+			     <1 10 4>; /* Hypervisor PPI, active-low */
+	};
+
+	pmu {
+		compatible = "arm,armv8-pmuv3";
+		interrupts = <1 7 0x8>; /* PMU PPI, Level low type */
+	};
+
+	soc {
+		compatible = "simple-bus";
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+		dma-ranges = <0x0 0x0 0x0 0x0 0x10000 0x00000000>;
+
+		clockgen: clocking@1300000 {
+			compatible = "fsl,ls2080a-clockgen";
+			reg = <0 0x1300000 0 0xa0000>;
+			#clock-cells = <2>;
+			clocks = <&sysclk>;
+		};
+
+		dcfg: dcfg@1e00000 {
+			compatible = "fsl,ls2080a-dcfg", "syscon";
+			reg = <0x0 0x1e00000 0x0 0x10000>;
+			little-endian;
+		};
+
+		tmu: tmu@1f80000 {
+			compatible = "fsl,qoriq-tmu";
+			reg = <0x0 0x1f80000 0x0 0x10000>;
+			interrupts = <0 23 0x4>;
+			fsl,tmu-range = <0xb0000 0x9002a 0x6004c 0x30062>;
+			fsl,tmu-calibration = <0x00000000 0x00000026
+					       0x00000001 0x0000002d
+					       0x00000002 0x00000032
+					       0x00000003 0x00000039
+					       0x00000004 0x0000003f
+					       0x00000005 0x00000046
+					       0x00000006 0x0000004d
+					       0x00000007 0x00000054
+					       0x00000008 0x0000005a
+					       0x00000009 0x00000061
+					       0x0000000a 0x0000006a
+					       0x0000000b 0x00000071
+
+					       0x00010000 0x00000025
+					       0x00010001 0x0000002c
+					       0x00010002 0x00000035
+					       0x00010003 0x0000003d
+					       0x00010004 0x00000045
+					       0x00010005 0x0000004e
+					       0x00010006 0x00000057
+					       0x00010007 0x00000061
+					       0x00010008 0x0000006b
+					       0x00010009 0x00000076
+
+					       0x00020000 0x00000029
+					       0x00020001 0x00000033
+					       0x00020002 0x0000003d
+					       0x00020003 0x00000049
+					       0x00020004 0x00000056
+					       0x00020005 0x00000061
+					       0x00020006 0x0000006d
+
+					       0x00030000 0x00000021
+					       0x00030001 0x0000002a
+					       0x00030002 0x0000003c
+					       0x00030003 0x0000004e>;
+			little-endian;
+			#thermal-sensor-cells = <1>;
+		};
+
+		thermal-zones {
+			cpu_thermal: cpu-thermal {
+				polling-delay-passive = <1000>;
+				polling-delay = <5000>;
+
+				thermal-sensors = <&tmu 4>;
+
+				trips {
+					cpu_alert: cpu-alert {
+						temperature = <75000>;
+						hysteresis = <2000>;
+						type = "passive";
+					};
+					cpu_crit: cpu-crit {
+						temperature = <85000>;
+						hysteresis = <2000>;
+						type = "critical";
+					};
+				};
+
+				cooling-maps {
+					map0 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu0 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+					map1 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu2 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+					map2 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu4 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+					map3 {
+						trip = <&cpu_alert>;
+						cooling-device =
+							<&cpu6 THERMAL_NO_LIMIT
+							THERMAL_NO_LIMIT>;
+					};
+				};
+			};
+		};
+
+		serial0: serial@21c0500 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21c0500 0x0 0x100>;
+			clocks = <&clockgen 4 3>;
+			interrupts = <0 32 0x4>; /* Level high type */
+		};
+
+		serial1: serial@21c0600 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21c0600 0x0 0x100>;
+			clocks = <&clockgen 4 3>;
+			interrupts = <0 32 0x4>; /* Level high type */
+		};
+
+		cluster1_core0_watchdog: wdt@c000000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc000000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster1_core1_watchdog: wdt@c010000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc010000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster2_core0_watchdog: wdt@c100000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc100000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster2_core1_watchdog: wdt@c110000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc110000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster3_core0_watchdog: wdt@c200000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc200000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster3_core1_watchdog: wdt@c210000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc210000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster4_core0_watchdog: wdt@c300000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc300000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		cluster4_core1_watchdog: wdt@c310000 {
+			compatible = "arm,sp805-wdt", "arm,primecell";
+			reg = <0x0 0xc310000 0x0 0x1000>;
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "apb_pclk", "wdog_clk";
+		};
+
+		crypto: crypto@8000000 {
+			compatible = "fsl,sec-v5.0", "fsl,sec-v4.0";
+			fsl,sec-era = <8>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0x0 0x00 0x8000000 0x100000>;
+			reg = <0x00 0x8000000 0x0 0x100000>;
+			interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
+			dma-coherent;
+
+			sec_jr0: jr@10000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x10000 0x10000>;
+				interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr1: jr@20000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x20000 0x10000>;
+				interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr2: jr@30000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x30000 0x10000>;
+				interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
+			};
+
+			sec_jr3: jr@40000 {
+				compatible = "fsl,sec-v5.0-job-ring",
+					     "fsl,sec-v4.0-job-ring";
+				reg	   = <0x40000 0x10000>;
+				interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
+			};
+		};
+
+		fsl_mc: fsl-mc@80c000000 {
+			compatible = "fsl,qoriq-mc";
+			reg = <0x00000008 0x0c000000 0 0x40>,	 /* MC portal base */
+			      <0x00000000 0x08340000 0 0x40000>; /* MC control reg */
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 0>;	/* This is fixed-up by u-boot */
+			dma-coherent;
+			#address-cells = <3>;
+			#size-cells = <1>;
+
+			/*
+			 * Region type 0x0 - MC portals
+			 * Region type 0x1 - QBMAN portals
+			 */
+			ranges = <0x0 0x0 0x0 0x8 0x0c000000 0x4000000
+				  0x1 0x0 0x0 0x8 0x18000000 0x8000000>;
+
+			/*
+			 * Define the maximum number of MACs present on the SoC.
+			 */
+			dpmacs {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				dpmac1: dpmac@1 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x1>;
+				};
+
+				dpmac2: dpmac@2 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x2>;
+				};
+
+				dpmac3: dpmac@3 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x3>;
+				};
+
+				dpmac4: dpmac@4 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x4>;
+				};
+
+				dpmac5: dpmac@5 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x5>;
+				};
+
+				dpmac6: dpmac@6 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x6>;
+				};
+
+				dpmac7: dpmac@7 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x7>;
+				};
+
+				dpmac8: dpmac@8 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x8>;
+				};
+
+				dpmac9: dpmac@9 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x9>;
+				};
+
+				dpmac10: dpmac@a {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0xa>;
+				};
+
+				dpmac11: dpmac@b {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0xb>;
+				};
+
+				dpmac12: dpmac@c {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0xc>;
+				};
+
+				dpmac13: dpmac@d {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0xd>;
+				};
+
+				dpmac14: dpmac@e {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0xe>;
+				};
+
+				dpmac15: dpmac@f {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0xf>;
+				};
+
+				dpmac16: dpmac@10 {
+					compatible = "fsl,qoriq-mc-dpmac";
+					reg = <0x10>;
+				};
+			};
+		};
+
+		smmu: iommu@5000000 {
+			compatible = "arm,mmu-500";
+			reg = <0 0x5000000 0 0x800000>;
+			#global-interrupts = <12>;
+			#iommu-cells = <1>;
+			stream-match-mask = <0x7C00>;
+			interrupts = <0 13 4>, /* global secure fault */
+				     <0 14 4>, /* combined secure interrupt */
+				     <0 15 4>, /* global non-secure fault */
+				     <0 16 4>, /* combined non-secure interrupt */
+				/* performance counter interrupts 0-7 */
+				     <0 211 4>, <0 212 4>,
+				     <0 213 4>, <0 214 4>,
+				     <0 215 4>, <0 216 4>,
+				     <0 217 4>, <0 218 4>,
+				/* per context interrupt, 64 interrupts */
+				     <0 146 4>, <0 147 4>,
+				     <0 148 4>, <0 149 4>,
+				     <0 150 4>, <0 151 4>,
+				     <0 152 4>, <0 153 4>,
+				     <0 154 4>, <0 155 4>,
+				     <0 156 4>, <0 157 4>,
+				     <0 158 4>, <0 159 4>,
+				     <0 160 4>, <0 161 4>,
+				     <0 162 4>, <0 163 4>,
+				     <0 164 4>, <0 165 4>,
+				     <0 166 4>, <0 167 4>,
+				     <0 168 4>, <0 169 4>,
+				     <0 170 4>, <0 171 4>,
+				     <0 172 4>, <0 173 4>,
+				     <0 174 4>, <0 175 4>,
+				     <0 176 4>, <0 177 4>,
+				     <0 178 4>, <0 179 4>,
+				     <0 180 4>, <0 181 4>,
+				     <0 182 4>, <0 183 4>,
+				     <0 184 4>, <0 185 4>,
+				     <0 186 4>, <0 187 4>,
+				     <0 188 4>, <0 189 4>,
+				     <0 190 4>, <0 191 4>,
+				     <0 192 4>, <0 193 4>,
+				     <0 194 4>, <0 195 4>,
+				     <0 196 4>, <0 197 4>,
+				     <0 198 4>, <0 199 4>,
+				     <0 200 4>, <0 201 4>,
+				     <0 202 4>, <0 203 4>,
+				     <0 204 4>, <0 205 4>,
+				     <0 206 4>, <0 207 4>,
+				     <0 208 4>, <0 209 4>;
+		};
+
+		dspi: dspi@2100000 {
+			status = "disabled";
+			compatible = "fsl,ls2080a-dspi", "fsl,ls2085a-dspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2100000 0x0 0x10000>;
+			interrupts = <0 26 0x4>; /* Level high type */
+			clocks = <&clockgen 4 3>;
+			clock-names = "dspi";
+			spi-num-chipselects = <5>;
+			bus-num = <0>;
+		};
+
+		esdhc: esdhc@2140000 {
+			status = "disabled";
+			compatible = "fsl,ls2080a-esdhc", "fsl,esdhc";
+			reg = <0x0 0x2140000 0x0 0x10000>;
+			interrupts = <0 28 0x4>; /* Level high type */
+			clocks = <&clockgen 4 1>;
+			voltage-ranges = <1800 1800 3300 3300>;
+			sdhci,auto-cmd12;
+			little-endian;
+			bus-width = <4>;
+		};
+
+		gpio0: gpio@2300000 {
+			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
+			reg = <0x0 0x2300000 0x0 0x10000>;
+			interrupts = <0 36 0x4>; /* Level high type */
+			gpio-controller;
+			little-endian;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio1: gpio@2310000 {
+			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
+			reg = <0x0 0x2310000 0x0 0x10000>;
+			interrupts = <0 36 0x4>; /* Level high type */
+			gpio-controller;
+			little-endian;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio2: gpio@2320000 {
+			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
+			reg = <0x0 0x2320000 0x0 0x10000>;
+			interrupts = <0 37 0x4>; /* Level high type */
+			gpio-controller;
+			little-endian;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio3: gpio@2330000 {
+			compatible = "fsl,ls2080a-gpio", "fsl,qoriq-gpio";
+			reg = <0x0 0x2330000 0x0 0x10000>;
+			interrupts = <0 37 0x4>; /* Level high type */
+			gpio-controller;
+			little-endian;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		/* TODO: WRIOP (CCSR?) */
+		emdio1: mdio@0x8B96000 { /* WRIOP0: 0x8B8_0000,
+					  * E-MDIO1: 0x1_6000
+					  */
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8B96000 0x0 0x1000>;
+			device_type = "mdio";	/* TODO: is this necessary? */
+			little-endian;	/* force the driver in LE mode */
+
+			/* Not necessary on the QDS, but needed on the RDB */
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		emdio2: mdio@0x8B97000 { /* WRIOP0: 0x8B8_0000,
+					  * E-MDIO2: 0x1_7000
+					  */
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8B97000 0x0 0x1000>;
+			device_type = "mdio";	/* TODO: is this necessary? */
+			little-endian;	/* force the driver in LE mode */
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio1: mdio@0x8c07000 {
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c07000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio2: mdio@0x8c0b000 {
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c0b000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio3: mdio@0x8c0f000 {
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c0f000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio4: mdio@0x8c13000 {
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c13000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio5: mdio@0x8c17000 {
+			status = "disabled";
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c17000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio6: mdio@0x8c1b000 {
+			status = "disabled";
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c1b000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio7: mdio@0x8c1f000 {
+			status = "disabled";
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c1f000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		pcs_mdio8: mdio@0x8c23000 {
+			status = "disabled";
+			compatible = "fsl,fman-memac-mdio";
+			reg = <0x0 0x8c23000 0x0 0x1000>;
+			device_type = "mdio";
+			little-endian;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c0: i2c@2000000 {
+			status = "disabled";
+			compatible = "fsl,vf610-i2c", "fsl,ls208xa-vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2000000 0x0 0x10000>;
+			interrupts = <0 34 0x4>; /* Level high type */
+			clock-names = "i2c";
+			clocks = <&clockgen 4 1>;
+			fsl-scl-gpio = <&gpio3 10 0>;
+		};
+
+		i2c1: i2c@2010000 {
+			status = "disabled";
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2010000 0x0 0x10000>;
+			interrupts = <0 34 0x4>; /* Level high type */
+			clock-names = "i2c";
+			clocks = <&clockgen 4 1>;
+		};
+
+		i2c2: i2c@2020000 {
+			status = "disabled";
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2020000 0x0 0x10000>;
+			interrupts = <0 35 0x4>; /* Level high type */
+			clock-names = "i2c";
+			clocks = <&clockgen 4 1>;
+		};
+
+		i2c3: i2c@2030000 {
+			status = "disabled";
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2030000 0x0 0x10000>;
+			interrupts = <0 35 0x4>; /* Level high type */
+			clock-names = "i2c";
+			clocks = <&clockgen 4 1>;
+		};
+
+		ifc: ifc@2240000 {
+			compatible = "fsl,ifc", "simple-bus";
+			reg = <0x0 0x2240000 0x0 0x20000>;
+			interrupts = <0 21 0x4>; /* Level high type */
+			little-endian;
+			#address-cells = <2>;
+			#size-cells = <1>;
+
+			ranges = <0 0 0x5 0x80000000 0x08000000
+				  2 0 0x5 0x30000000 0x00010000
+				  3 0 0x5 0x20000000 0x00010000>;
+		};
+
+		qspi: quadspi@20c0000 {
+			status = "disabled";
+			compatible = "fsl,ls2080a-qspi", "fsl,ls1021a-qspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x20c0000 0x0 0x10000>,
+			      <0x0 0x20000000 0x0 0x10000000>;
+			reg-names = "QuadSPI", "QuadSPI-memory";
+			interrupts = <0 25 0x4>; /* Level high type */
+			clocks = <&clockgen 4 3>, <&clockgen 4 3>;
+			clock-names = "qspi_en", "qspi";
+		};
+
+		pcie1: pcie@3400000 {
+			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
+				     "snps,dw-pcie";
+			reg-names = "regs", "config";
+			interrupts = <0 108 0x4>; /* aer interrupt */
+			interrupt-names = "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 1>;	/* This is fixed-up by u-boot */
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 0 0 109 4>,
+					<0000 0 0 2 &gic 0 0 0 110 4>,
+					<0000 0 0 3 &gic 0 0 0 111 4>,
+					<0000 0 0 4 &gic 0 0 0 112 4>;
+		};
+
+		pcie2: pcie@3500000 {
+			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
+				     "snps,dw-pcie";
+			reg-names = "regs", "config";
+			interrupts = <0 113 0x4>; /* aer interrupt */
+			interrupt-names = "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 1>;	/* This is fixed-up by u-boot */
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 0 0 114 4>,
+					<0000 0 0 2 &gic 0 0 0 115 4>,
+					<0000 0 0 3 &gic 0 0 0 116 4>,
+					<0000 0 0 4 &gic 0 0 0 117 4>;
+		};
+
+		pcie3: pcie@3600000 {
+			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
+				     "snps,dw-pcie";
+			reg-names = "regs", "config";
+			interrupts = <0 118 0x4>; /* aer interrupt */
+			interrupt-names = "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <8>;
+			bus-range = <0x0 0xff>;
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 1>;	/* This is fixed-up by u-boot */
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 0 0 119 4>,
+					<0000 0 0 2 &gic 0 0 0 120 4>,
+					<0000 0 0 3 &gic 0 0 0 121 4>,
+					<0000 0 0 4 &gic 0 0 0 122 4>;
+		};
+
+		pcie4: pcie@3700000 {
+			compatible = "fsl,ls2080a-pcie", "fsl,ls2085a-pcie",
+				     "snps,dw-pcie";
+			reg-names = "regs", "config";
+			interrupts = <0 123 0x4>; /* aer interrupt */
+			interrupt-names = "aer";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			dma-coherent;
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			msi-parent = <&its>;
+			iommu-map = <0 &smmu 0 1>;	/* This is fixed-up by u-boot */
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 0 0 124 4>,
+					<0000 0 0 2 &gic 0 0 0 125 4>,
+					<0000 0 0 3 &gic 0 0 0 126 4>,
+					<0000 0 0 4 &gic 0 0 0 127 4>;
+		};
+
+		sata0: sata@3200000 {
+			status = "disabled";
+			compatible = "fsl,ls2080a-ahci";
+			reg = <0x0 0x3200000 0x0 0x10000>;
+			interrupts = <0 133 0x4>; /* Level high type */
+			clocks = <&clockgen 4 3>;
+			dma-coherent;
+		};
+
+		sata1: sata@3210000 {
+			status = "disabled";
+			compatible = "fsl,ls2080a-ahci";
+			reg = <0x0 0x3210000 0x0 0x10000>;
+			interrupts = <0 136 0x4>; /* Level high type */
+			clocks = <&clockgen 4 3>;
+			dma-coherent;
+		};
+
+		usb0: usb3@3100000 {
+			status = "disabled";
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3100000 0x0 0x10000>;
+			interrupts = <0 80 0x4>; /* Level high type */
+			dr_mode = "host";
+			snps,quirk-frame-length-adjustment = <0x20>;
+			snps,dis_rxdet_inp3_quirk;
+		};
+
+		usb1: usb3@3110000 {
+			status = "disabled";
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3110000 0x0 0x10000>;
+			interrupts = <0 81 0x4>; /* Level high type */
+			dr_mode = "host";
+			snps,quirk-frame-length-adjustment = <0x20>;
+			snps,dis_rxdet_inp3_quirk;
+		};
+
+		serdes1: serdes@1ea0000 {
+				reg = <0x0 0x1ea0000 0 0x00002000>;
+		};
+
+		ccn@4000000 {
+			compatible = "arm,ccn-504";
+			reg = <0x0 0x04000000 0x0 0x01000000>;
+			interrupts = <0 12 4>;
+		};
+
+		ftm0: ftm0@2800000 {
+			compatible = "fsl,ls208xa-ftm";
+			reg = <0x0 0x2800000 0x0 0x10000>,
+			      <0x0 0x1e34050 0x0 0x4>;
+			interrupts = <0 44 4>;
+			reg-names = "ftm", "FlexTimer1";
+		};
+	};
+
+	ddr1: memory-controller@1080000 {
+		compatible = "fsl,qoriq-memory-controller";
+		reg = <0x0 0x1080000 0x0 0x1000>;
+		interrupts = <0 17 0x4>;
+		little-endian;
+	};
+
+	ddr2: memory-controller@1090000 {
+		compatible = "fsl,qoriq-memory-controller";
+		reg = <0x0 0x1090000 0x0 0x1000>;
+		interrupts = <0 18 0x4>;
+		little-endian;
+	};
+
+	firmware {
+		optee {
+			compatible = "linaro,optee-tz";
+			method = "smc";
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-bman-portals-sdk.dtsi
@@ -0,0 +1,55 @@
+/*
+ * QorIQ BMan SDK Portals device tree nodes
+ *
+ * Copyright 2011-2016 Freescale Semiconductor Inc.
+ * Copyright 2017 NXP
+ *
+ * SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+ */
+
+&bportals {
+	bman-portal@0 {
+		cell-index = <0>;
+	};
+
+	bman-portal@10000 {
+		cell-index = <1>;
+	};
+
+	bman-portal@20000 {
+		cell-index = <2>;
+	};
+
+	bman-portal@30000 {
+		cell-index = <3>;
+	};
+
+	bman-portal@40000 {
+		cell-index = <4>;
+	};
+
+	bman-portal@50000 {
+		cell-index = <5>;
+	};
+
+	bman-portal@60000 {
+		cell-index = <6>;
+	};
+
+	bman-portal@70000 {
+		cell-index = <7>;
+	};
+
+	bman-portal@80000 {
+		cell-index = <8>;
+	};
+
+	bman-portal@90000 {
+		cell-index = <9>;
+	};
+
+	 bman-bpids@0 {
+		compatible = "fsl,bpid-range";
+		fsl,bpid-range = <32 32>;
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-bman-portals.dtsi
@@ -0,0 +1,77 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ BMan Portals device tree
+ *
+ * Copyright 2011-2016 Freescale Semiconductor Inc.
+ *
+ */
+
+&bportals {
+	#address-cells = <1>;
+	#size-cells = <1>;
+	compatible = "simple-bus";
+
+	bman-portal@0 {
+		/*
+		 * bootloader fix-ups are expected to provide the
+		 * "fsl,bman-portal-<hardware revision>" compatible
+		 */
+		compatible = "fsl,bman-portal";
+		reg = <0x0 0x4000>, <0x4000000 0x4000>;
+		interrupts = <GIC_SPI 173 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@10000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x10000 0x4000>, <0x4010000 0x4000>;
+		interrupts = <GIC_SPI 175 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@20000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x20000 0x4000>, <0x4020000 0x4000>;
+		interrupts = <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@30000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x30000 0x4000>, <0x4030000 0x4000>;
+		interrupts = <GIC_SPI 179 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@40000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x40000 0x4000>, <0x4040000 0x4000>;
+		interrupts = <GIC_SPI 181 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@50000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x50000 0x4000>, <0x4050000 0x4000>;
+		interrupts = <GIC_SPI 183 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@60000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x60000 0x4000>, <0x4060000 0x4000>;
+		interrupts = <GIC_SPI 185 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@70000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x70000 0x4000>, <0x4070000 0x4000>;
+		interrupts = <GIC_SPI 187 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@80000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x80000 0x4000>, <0x4080000 0x4000>;
+		interrupts = <GIC_SPI 189 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	bman-portal@90000 {
+		compatible = "fsl,bman-portal";
+		reg = <0x90000 0x4000>, <0x4090000 0x4000>;
+		interrupts = <GIC_SPI 191 IRQ_TYPE_LEVEL_HIGH>;
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-dpaa-eth.dtsi
@@ -0,0 +1,73 @@
+/*
+ * QorIQ FMan v3 10g port #1 device tree stub [ controller @ offset 0x400000 ]
+ *
+ * Copyright 2012 - 2015 Freescale Semiconductor Inc.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions are met:
+ *     * Redistributions of source code must retain the above copyright
+ *       notice, this list of conditions and the following disclaimer.
+ *     * Redistributions in binary form must reproduce the above copyright
+ *       notice, this list of conditions and the following disclaimer in the
+ *       documentation and/or other materials provided with the distribution.
+ *     * Neither the name of Freescale Semiconductor nor the
+ *       names of its contributors may be used to endorse or promote products
+ *       derived from this software without specific prior written permission.
+ *
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") as published by the Free Software
+ * Foundation, either version 2 of that License or (at your option) any
+ * later version.
+ *
+ * THIS SOFTWARE IS PROVIDED BY Freescale Semiconductor ``AS IS'' AND ANY
+ * EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
+ * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
+ * DISCLAIMED. IN NO EVENT SHALL Freescale Semiconductor BE LIABLE FOR ANY
+ * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
+ * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
+ * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
+ * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+fsldpaa: fsl,dpaa {
+	compatible = "fsl,ls1043a-dpaa", "simple-bus", "fsl,dpaa";
+	ethernet@0 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet0>;
+		dma-coherent;
+	};
+	ethernet@1 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet1>;
+		dma-coherent;
+	};
+	ethernet@2 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet2>;
+		dma-coherent;
+	};
+	ethernet@3 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet3>;
+		dma-coherent;
+	};
+	ethernet@4 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet4>;
+		dma-coherent;
+	};
+	ethernet@5 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet5>;
+		dma-coherent;
+	};
+	ethernet@8 {
+		compatible = "fsl,dpa-ethernet";
+		fsl,fman-mac = <&enet6>;
+		dma-coherent;
+	};
+};
+
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-10g-0.dtsi
@@ -0,0 +1,43 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 10g port #0 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x10: port@90000 {
+		cell-index = <0x10>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-10g-rx";
+		reg = <0x90000 0x1000>;
+		fsl,fman-10g-port;
+	};
+
+	fman0_tx_0x30: port@b0000 {
+		cell-index = <0x30>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-10g-tx";
+		reg = <0xb0000 0x1000>;
+		fsl,fman-10g-port;
+		fsl,qman-channel-id = <0x800>;
+	};
+
+	ethernet@f0000 {
+		cell-index = <0x8>;
+		compatible = "fsl,fman-memac";
+		reg = <0xf0000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x10 &fman0_tx_0x30>;
+		pcsphy-handle = <&pcsphy6>;
+	};
+
+	mdio@f1000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xf1000 0x1000>;
+
+		pcsphy6: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-10g-1.dtsi
@@ -0,0 +1,43 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 10g port #1 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x11: port@91000 {
+		cell-index = <0x11>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-10g-rx";
+		reg = <0x91000 0x1000>;
+		fsl,fman-10g-port;
+	};
+
+	fman0_tx_0x31: port@b1000 {
+		cell-index = <0x31>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-10g-tx";
+		reg = <0xb1000 0x1000>;
+		fsl,fman-10g-port;
+		fsl,qman-channel-id = <0x801>;
+	};
+
+	ethernet@f2000 {
+		cell-index = <0x9>;
+		compatible = "fsl,fman-memac";
+		reg = <0xf2000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x11 &fman0_tx_0x31>;
+		pcsphy-handle = <&pcsphy7>;
+	};
+
+	mdio@f3000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xf3000 0x1000>;
+
+		pcsphy7: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-0.dtsi
@@ -0,0 +1,42 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 1g port #0 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x08: port@88000 {
+		cell-index = <0x8>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-1g-rx";
+		reg = <0x88000 0x1000>;
+	};
+
+	fman0_tx_0x28: port@a8000 {
+		cell-index = <0x28>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-1g-tx";
+		reg = <0xa8000 0x1000>;
+		fsl,qman-channel-id = <0x802>;
+	};
+
+	ethernet@e0000 {
+		cell-index = <0>;
+		compatible = "fsl,fman-memac";
+		reg = <0xe0000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x08 &fman0_tx_0x28>;
+		ptp-timer = <&ptp_timer0>;
+		pcsphy-handle = <&pcsphy0>;
+	};
+
+	mdio@e1000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xe1000 0x1000>;
+
+		pcsphy0: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-1.dtsi
@@ -0,0 +1,42 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 1g port #1 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x09: port@89000 {
+		cell-index = <0x9>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-1g-rx";
+		reg = <0x89000 0x1000>;
+	};
+
+	fman0_tx_0x29: port@a9000 {
+		cell-index = <0x29>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-1g-tx";
+		reg = <0xa9000 0x1000>;
+		fsl,qman-channel-id = <0x803>;
+	};
+
+	ethernet@e2000 {
+		cell-index = <1>;
+		compatible = "fsl,fman-memac";
+		reg = <0xe2000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x09 &fman0_tx_0x29>;
+		ptp-timer = <&ptp_timer0>;
+		pcsphy-handle = <&pcsphy1>;
+	};
+
+	mdio@e3000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xe3000 0x1000>;
+
+		pcsphy1: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-2.dtsi
@@ -0,0 +1,42 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 1g port #2 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x0a: port@8a000 {
+		cell-index = <0xa>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-1g-rx";
+		reg = <0x8a000 0x1000>;
+	};
+
+	fman0_tx_0x2a: port@aa000 {
+		cell-index = <0x2a>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-1g-tx";
+		reg = <0xaa000 0x1000>;
+		fsl,qman-channel-id = <0x804>;
+	};
+
+	ethernet@e4000 {
+		cell-index = <2>;
+		compatible = "fsl,fman-memac";
+		reg = <0xe4000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x0a &fman0_tx_0x2a>;
+		ptp-timer = <&ptp_timer0>;
+		pcsphy-handle = <&pcsphy2>;
+	};
+
+	mdio@e5000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xe5000 0x1000>;
+
+		pcsphy2: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-3.dtsi
@@ -0,0 +1,42 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 1g port #3 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x0b: port@8b000 {
+		cell-index = <0xb>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-1g-rx";
+		reg = <0x8b000 0x1000>;
+	};
+
+	fman0_tx_0x2b: port@ab000 {
+		cell-index = <0x2b>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-1g-tx";
+		reg = <0xab000 0x1000>;
+		fsl,qman-channel-id = <0x805>;
+	};
+
+	ethernet@e6000 {
+		cell-index = <3>;
+		compatible = "fsl,fman-memac";
+		reg = <0xe6000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x0b &fman0_tx_0x2b>;
+		ptp-timer = <&ptp_timer0>;
+		pcsphy-handle = <&pcsphy3>;
+	};
+
+	mdio@e7000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xe7000 0x1000>;
+
+		pcsphy3: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-4.dtsi
@@ -0,0 +1,42 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 1g port #4 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x0c: port@8c000 {
+		cell-index = <0xc>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-1g-rx";
+		reg = <0x8c000 0x1000>;
+	};
+
+	fman0_tx_0x2c: port@ac000 {
+		cell-index = <0x2c>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-1g-tx";
+		reg = <0xac000 0x1000>;
+		fsl,qman-channel-id = <0x806>;
+	};
+
+	ethernet@e8000 {
+		cell-index = <4>;
+		compatible = "fsl,fman-memac";
+		reg = <0xe8000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x0c &fman0_tx_0x2c>;
+		ptp-timer = <&ptp_timer0>;
+		pcsphy-handle = <&pcsphy4>;
+	};
+
+	mdio@e9000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xe9000 0x1000>;
+
+		pcsphy4: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-1g-5.dtsi
@@ -0,0 +1,42 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 1g port #5 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman@1a00000 {
+	fman0_rx_0x0d: port@8d000 {
+		cell-index = <0xd>;
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-1g-rx";
+		reg = <0x8d000 0x1000>;
+	};
+
+	fman0_tx_0x2d: port@ad000 {
+		cell-index = <0x2d>;
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-1g-tx";
+		reg = <0xad000 0x1000>;
+		fsl,qman-channel-id = <0x807>;
+	};
+
+	ethernet@ea000 {
+		cell-index = <5>;
+		compatible = "fsl,fman-memac";
+		reg = <0xea000 0x1000>;
+		fsl,fman-ports = <&fman0_rx_0x0d &fman0_tx_0x2d>;
+		ptp-timer = <&ptp_timer0>;
+		pcsphy-handle = <&pcsphy5>;
+	};
+
+	mdio@eb000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xeb000 0x1000>;
+
+		pcsphy5: ethernet-phy@0 {
+			reg = <0x0>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0-6oh.dtsi
@@ -0,0 +1,47 @@
+/*
+ * QorIQ FMan v3 OH ports device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ * SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+ */
+
+fman@1a00000 {
+
+	fman0_oh1: port@82000 {
+		cell-index = <0>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x82000 0x1000>;
+	};
+
+	fman0_oh2: port@83000 {
+		cell-index = <1>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x83000 0x1000>;
+	};
+
+	fman0_oh3: port@84000 {
+		cell-index = <2>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x84000 0x1000>;
+	};
+
+	fman0_oh4: port@85000 {
+		cell-index = <3>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x85000 0x1000>;
+	};
+
+	fman0_oh5: port@86000 {
+		cell-index = <4>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x86000 0x1000>;
+	};
+
+	fman0_oh6: port@87000 {
+		cell-index = <5>;
+		compatible = "fsl,fman-port-oh";
+		reg = <0x87000 0x1000>;
+	};
+
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-fman3-0.dtsi
@@ -0,0 +1,130 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ FMan v3 device tree
+ *
+ * Copyright 2012-2015 Freescale Semiconductor Inc.
+ *
+ */
+
+fman0: fman@1a00000 {
+	#address-cells = <1>;
+	#size-cells = <1>;
+	cell-index = <0>;
+	compatible = "fsl,fman";
+	ranges = <0x0 0x00 0x1a00000 0x100000>;
+	reg = <0x0 0x1a00000 0x0 0x100000>;
+	interrupts = <0 44 0x4>, <0 45 0x4>;
+	clocks = <&clockgen 3 0>;
+	clock-names = "fmanclk";
+	fsl,qman-channel-range = <0x800 0x10>;
+
+	cc {
+		compatible = "fsl,fman-cc";
+	};
+
+	muram@0 {
+		compatible = "fsl,fman-muram";
+		reg = <0x0 0x60000>;
+	};
+
+	bmi@80000 {
+		compatible = "fsl,fman-bmi";
+		reg = <0x80000 0x400>;
+	};
+
+	qmi@80400 {
+		compatible = "fsl,fman-qmi";
+		reg = <0x80400 0x400>;
+	};
+
+	fman0_oh_0x2: port@82000 {
+		cell-index = <0x2>;
+		compatible = "fsl,fman-v3-port-oh";
+		reg = <0x82000 0x1000>;
+		fsl,qman-channel-id = <0x809>;
+	};
+
+	fman0_oh_0x3: port@83000 {
+		cell-index = <0x3>;
+		compatible = "fsl,fman-v3-port-oh";
+		reg = <0x83000 0x1000>;
+		fsl,qman-channel-id = <0x80a>;
+	};
+
+	fman0_oh_0x4: port@84000 {
+		cell-index = <0x4>;
+		compatible = "fsl,fman-v3-port-oh";
+		reg = <0x84000 0x1000>;
+		fsl,qman-channel-id = <0x80b>;
+	};
+
+	fman0_oh_0x5: port@85000 {
+		cell-index = <0x5>;
+		compatible = "fsl,fman-v3-port-oh";
+		reg = <0x85000 0x1000>;
+		fsl,qman-channel-id = <0x80c>;
+	};
+
+	fman0_oh_0x6: port@86000 {
+		cell-index = <0x6>;
+		compatible = "fsl,fman-v3-port-oh";
+		reg = <0x86000 0x1000>;
+		fsl,qman-channel-id = <0x80d>;
+	};
+
+	fman0_oh_0x7: port@87000 {
+		cell-index = <0x7>;
+		compatible = "fsl,fman-v3-port-oh";
+		reg = <0x87000 0x1000>;
+		fsl,qman-channel-id = <0x80e>;
+	};
+
+	policer@c0000 {
+		compatible = "fsl,fman-policer";
+		reg = <0xc0000 0x1000>;
+	};
+
+	keygen@c1000 {
+		compatible = "fsl,fman-keygen";
+		reg = <0xc1000 0x1000>;
+	};
+
+	dma@c2000 {
+		compatible = "fsl,fman-dma";
+		reg = <0xc2000 0x1000>;
+	};
+
+	fpm@c3000 {
+		compatible = "fsl,fman-fpm";
+		reg = <0xc3000 0x1000>;
+	};
+
+	parser@c7000 {
+		compatible = "fsl,fman-parser";
+		reg = <0xc7000 0x1000>;
+	};
+
+	vsps@dc000 {
+		compatible = "fsl,fman-vsps";
+		reg = <0xdc000 0x1000>;
+	};
+
+	mdio0: mdio@fc000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xfc000 0x1000>;
+	};
+
+	xmdio0: mdio@fd000 {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		compatible = "fsl,fman-memac-mdio", "fsl,fman-xmdio";
+		reg = <0xfd000 0x1000>;
+	};
+
+	ptp_timer0: ptp-timer@fe000 {
+		compatible = "fsl,fman-ptp-timer", "fsl,fman-rtc";
+		reg = <0xfe000 0x1000>;
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-qman-portals-sdk.dtsi
@@ -0,0 +1,38 @@
+/*
+ * QorIQ QMan SDK Portals device tree nodes
+ *
+ * Copyright 2011-2016 Freescale Semiconductor Inc.
+ * Copyright 2017 NXP
+ *
+ * SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+ */
+
+&qportals {
+	qman-fqids@0 {
+		compatible = "fsl,fqid-range";
+		fsl,fqid-range = <256 256>;
+	};
+
+	qman-fqids@1 {
+		compatible = "fsl,fqid-range";
+		fsl,fqid-range = <32768 32768>;
+	};
+
+	qman-pools@0 {
+		compatible = "fsl,pool-channel-range";
+		fsl,pool-channel-range = <0x401 0xf>;
+	};
+
+	qman-cgrids@0 {
+		compatible = "fsl,cgrid-range";
+		fsl,cgrid-range = <0 256>;
+	};
+
+	qman-ceetm@0 {
+		compatible = "fsl,qman-ceetm";
+		fsl,ceetm-lfqid-range = <0xf00000 0x1000>;
+		fsl,ceetm-sp-range = <0 16>;
+		fsl,ceetm-lni-range = <0 8>;
+		fsl,ceetm-channel-range = <0 32>;
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-qman-portals.dtsi
@@ -0,0 +1,87 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * QorIQ QMan Portals device tree
+ *
+ * Copyright 2011-2016 Freescale Semiconductor Inc.
+ *
+ */
+
+&qportals {
+	#address-cells = <1>;
+	#size-cells = <1>;
+	compatible = "simple-bus";
+
+	qportal0: qman-portal@0 {
+		/*
+		 * bootloader fix-ups are expected to provide the
+		 * "fsl,bman-portal-<hardware revision>" compatible
+		 */
+		compatible = "fsl,qman-portal";
+		reg = <0x0 0x4000>, <0x4000000 0x4000>;
+		interrupts = <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <0>;
+	};
+
+	qportal1: qman-portal@10000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x10000 0x4000>, <0x4010000 0x4000>;
+		interrupts = <GIC_SPI 174 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <1>;
+	};
+
+	qportal2: qman-portal@20000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x20000 0x4000>, <0x4020000 0x4000>;
+		interrupts = <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <2>;
+	};
+
+	qportal3: qman-portal@30000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x30000 0x4000>, <0x4030000 0x4000>;
+		interrupts = <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <3>;
+	};
+
+	qportal4: qman-portal@40000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x40000 0x4000>, <0x4040000 0x4000>;
+		interrupts = <GIC_SPI 180 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <4>;
+	};
+
+	qportal5: qman-portal@50000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x50000 0x4000>, <0x4050000 0x4000>;
+		interrupts = <GIC_SPI 182 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <5>;
+	};
+
+	qportal6: qman-portal@60000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x60000 0x4000>, <0x4060000 0x4000>;
+		interrupts = <GIC_SPI 184 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <6>;
+	};
+
+	qportal7: qman-portal@70000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x70000 0x4000>, <0x4070000 0x4000>;
+		interrupts = <GIC_SPI 186 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <7>;
+	};
+
+	qportal8: qman-portal@80000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x80000 0x4000>, <0x4080000 0x4000>;
+		interrupts = <GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <8>;
+	};
+
+	qportal9: qman-portal@90000 {
+		compatible = "fsl,qman-portal";
+		reg = <0x90000 0x4000>, <0x4090000 0x4000>;
+		interrupts = <GIC_SPI 190 IRQ_TYPE_LEVEL_HIGH>;
+		cell-index = <9>;
+	};
+};
--- a/arch/powerpc/boot/dts/fsl/qoriq-bman1-portals.dtsi
+++ b/arch/powerpc/boot/dts/fsl/qoriq-bman1-portals.dtsi
@@ -38,51 +38,61 @@
 	compatible = "simple-bus";
 
 	bman-portal@0 {
+		cell-index = <0>;
 		compatible = "fsl,bman-portal";
 		reg = <0x0 0x4000>, <0x100000 0x1000>;
 		interrupts = <105 2 0 0>;
 	};
 	bman-portal@4000 {
+		cell-index = <1>;
 		compatible = "fsl,bman-portal";
 		reg = <0x4000 0x4000>, <0x101000 0x1000>;
 		interrupts = <107 2 0 0>;
 	};
 	bman-portal@8000 {
+		cell-index = <2>;
 		compatible = "fsl,bman-portal";
 		reg = <0x8000 0x4000>, <0x102000 0x1000>;
 		interrupts = <109 2 0 0>;
 	};
 	bman-portal@c000 {
+		cell-index = <3>;
 		compatible = "fsl,bman-portal";
 		reg = <0xc000 0x4000>, <0x103000 0x1000>;
 		interrupts = <111 2 0 0>;
 	};
 	bman-portal@10000 {
+		cell-index = <4>;
 		compatible = "fsl,bman-portal";
 		reg = <0x10000 0x4000>, <0x104000 0x1000>;
 		interrupts = <113 2 0 0>;
 	};
 	bman-portal@14000 {
+		cell-index = <5>;
 		compatible = "fsl,bman-portal";
 		reg = <0x14000 0x4000>, <0x105000 0x1000>;
 		interrupts = <115 2 0 0>;
 	};
 	bman-portal@18000 {
+		cell-index = <6>;
 		compatible = "fsl,bman-portal";
 		reg = <0x18000 0x4000>, <0x106000 0x1000>;
 		interrupts = <117 2 0 0>;
 	};
 	bman-portal@1c000 {
+		cell-index = <7>;
 		compatible = "fsl,bman-portal";
 		reg = <0x1c000 0x4000>, <0x107000 0x1000>;
 		interrupts = <119 2 0 0>;
 	};
 	bman-portal@20000 {
+		cell-index = <8>;
 		compatible = "fsl,bman-portal";
 		reg = <0x20000 0x4000>, <0x108000 0x1000>;
 		interrupts = <121 2 0 0>;
 	};
 	bman-portal@24000 {
+		cell-index = <9>;
 		compatible = "fsl,bman-portal";
 		reg = <0x24000 0x4000>, <0x109000 0x1000>;
 		interrupts = <123 2 0 0>;
--- a/arch/powerpc/boot/dts/fsl/qoriq-fman3-0-10g-0.dtsi
+++ b/arch/powerpc/boot/dts/fsl/qoriq-fman3-0-10g-0.dtsi
@@ -35,14 +35,14 @@
 fman@400000 {
 	fman0_rx_0x10: port@90000 {
 		cell-index = <0x10>;
-		compatible = "fsl,fman-v3-port-rx";
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-10g-rx";
 		reg = <0x90000 0x1000>;
 		fsl,fman-10g-port;
 	};
 
 	fman0_tx_0x30: port@b0000 {
 		cell-index = <0x30>;
-		compatible = "fsl,fman-v3-port-tx";
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-10g-tx";
 		reg = <0xb0000 0x1000>;
 		fsl,fman-10g-port;
 	};
--- a/arch/powerpc/boot/dts/fsl/qoriq-fman3-0-10g-1.dtsi
+++ b/arch/powerpc/boot/dts/fsl/qoriq-fman3-0-10g-1.dtsi
@@ -35,14 +35,14 @@
 fman@400000 {
 	fman0_rx_0x11: port@91000 {
 		cell-index = <0x11>;
-		compatible = "fsl,fman-v3-port-rx";
+		compatible = "fsl,fman-v3-port-rx", "fsl,fman-port-10g-rx";
 		reg = <0x91000 0x1000>;
 		fsl,fman-10g-port;
 	};
 
 	fman0_tx_0x31: port@b1000 {
 		cell-index = <0x31>;
-		compatible = "fsl,fman-v3-port-tx";
+		compatible = "fsl,fman-v3-port-tx", "fsl,fman-port-10g-tx";
 		reg = <0xb1000 0x1000>;
 		fsl,fman-10g-port;
 	};
