From ea009d063f7a3d70831788046c7285a4af4ab82d Mon Sep 17 00:00:00 2001
From: Chen Zhong <chen.zhong@mediatek.com>
Date: Thu, 5 Oct 2017 11:50:25 +0800
Subject: [PATCH 149/224] clk: mediatek: add clocks dt-bindings required header
 for MT7622 SoC

Add the required header for the entire clocks dt-bindings exported
from topckgen, apmixedsys, infracfg, pericfg, ethsys, pciesys, ssusbsys
and audsys which could be found on MT7622 SoC.

Signed-off-by: Chen Zhong <chen.zhong@mediatek.com>
Signed-off-by: Sean Wang <sean.wang@mediatek.com>
Signed-off-by: Stephen Boyd <sboyd@codeaurora.org>
---
 include/dt-bindings/clock/mt7622-clk.h | 289 +++++++++++++++++++++++++++++++++
 1 file changed, 289 insertions(+)
 create mode 100644 include/dt-bindings/clock/mt7622-clk.h

--- /dev/null
+++ b/include/dt-bindings/clock/mt7622-clk.h
@@ -0,0 +1,289 @@
+/*
+ * Copyright (c) 2017 MediaTek Inc.
+ * Author: Chen Zhong <chen.zhong@mediatek.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+
+#ifndef _DT_BINDINGS_CLK_MT7622_H
+#define _DT_BINDINGS_CLK_MT7622_H
+
+/* TOPCKGEN */
+
+#define CLK_TOP_TO_U2_PHY		0
+#define CLK_TOP_TO_U2_PHY_1P		1
+#define CLK_TOP_PCIE0_PIPE_EN		2
+#define CLK_TOP_PCIE1_PIPE_EN		3
+#define CLK_TOP_SSUSB_TX250M		4
+#define CLK_TOP_SSUSB_EQ_RX250M		5
+#define CLK_TOP_SSUSB_CDR_REF		6
+#define CLK_TOP_SSUSB_CDR_FB		7
+#define CLK_TOP_SATA_ASIC		8
+#define CLK_TOP_SATA_RBC		9
+#define CLK_TOP_TO_USB3_SYS		10
+#define CLK_TOP_P1_1MHZ			11
+#define CLK_TOP_4MHZ			12
+#define CLK_TOP_P0_1MHZ			13
+#define CLK_TOP_TXCLK_SRC_PRE		14
+#define CLK_TOP_RTC			15
+#define CLK_TOP_MEMPLL			16
+#define CLK_TOP_DMPLL			17
+#define CLK_TOP_SYSPLL_D2		18
+#define CLK_TOP_SYSPLL1_D2		19
+#define CLK_TOP_SYSPLL1_D4		20
+#define CLK_TOP_SYSPLL1_D8		21
+#define CLK_TOP_SYSPLL2_D4		22
+#define CLK_TOP_SYSPLL2_D8		23
+#define CLK_TOP_SYSPLL_D5		24
+#define CLK_TOP_SYSPLL3_D2		25
+#define CLK_TOP_SYSPLL3_D4		26
+#define CLK_TOP_SYSPLL4_D2		27
+#define CLK_TOP_SYSPLL4_D4		28
+#define CLK_TOP_SYSPLL4_D16		29
+#define CLK_TOP_UNIVPLL			30
+#define CLK_TOP_UNIVPLL_D2		31
+#define CLK_TOP_UNIVPLL1_D2		32
+#define CLK_TOP_UNIVPLL1_D4		33
+#define CLK_TOP_UNIVPLL1_D8		34
+#define CLK_TOP_UNIVPLL1_D16		35
+#define CLK_TOP_UNIVPLL2_D2		36
+#define CLK_TOP_UNIVPLL2_D4		37
+#define CLK_TOP_UNIVPLL2_D8		38
+#define CLK_TOP_UNIVPLL2_D16		39
+#define CLK_TOP_UNIVPLL_D5		40
+#define CLK_TOP_UNIVPLL3_D2		41
+#define CLK_TOP_UNIVPLL3_D4		42
+#define CLK_TOP_UNIVPLL3_D16		43
+#define CLK_TOP_UNIVPLL_D7		44
+#define CLK_TOP_UNIVPLL_D80_D4		45
+#define CLK_TOP_UNIV48M			46
+#define CLK_TOP_SGMIIPLL		47
+#define CLK_TOP_SGMIIPLL_D2		48
+#define CLK_TOP_AUD1PLL			49
+#define CLK_TOP_AUD2PLL			50
+#define CLK_TOP_AUD_I2S2_MCK		51
+#define CLK_TOP_TO_USB3_REF		52
+#define CLK_TOP_PCIE1_MAC_EN		53
+#define CLK_TOP_PCIE0_MAC_EN		54
+#define CLK_TOP_ETH_500M		55
+#define CLK_TOP_AXI_SEL			56
+#define CLK_TOP_MEM_SEL			57
+#define CLK_TOP_DDRPHYCFG_SEL		58
+#define CLK_TOP_ETH_SEL			59
+#define CLK_TOP_PWM_SEL			60
+#define CLK_TOP_F10M_REF_SEL		61
+#define CLK_TOP_NFI_INFRA_SEL		62
+#define CLK_TOP_FLASH_SEL		63
+#define CLK_TOP_UART_SEL		64
+#define CLK_TOP_SPI0_SEL		65
+#define CLK_TOP_SPI1_SEL		66
+#define CLK_TOP_MSDC50_0_SEL		67
+#define CLK_TOP_MSDC30_0_SEL		68
+#define CLK_TOP_MSDC30_1_SEL		69
+#define CLK_TOP_A1SYS_HP_SEL		70
+#define CLK_TOP_A2SYS_HP_SEL		71
+#define CLK_TOP_INTDIR_SEL		72
+#define CLK_TOP_AUD_INTBUS_SEL		73
+#define CLK_TOP_PMICSPI_SEL		74
+#define CLK_TOP_SCP_SEL			75
+#define CLK_TOP_ATB_SEL			76
+#define CLK_TOP_HIF_SEL			77
+#define CLK_TOP_AUDIO_SEL		78
+#define CLK_TOP_U2_SEL			79
+#define CLK_TOP_AUD1_SEL		80
+#define CLK_TOP_AUD2_SEL		81
+#define CLK_TOP_IRRX_SEL		82
+#define CLK_TOP_IRTX_SEL		83
+#define CLK_TOP_ASM_L_SEL		84
+#define CLK_TOP_ASM_M_SEL		85
+#define CLK_TOP_ASM_H_SEL		86
+#define CLK_TOP_APLL1_SEL		87
+#define CLK_TOP_APLL2_SEL		88
+#define CLK_TOP_I2S0_MCK_SEL		89
+#define CLK_TOP_I2S1_MCK_SEL		90
+#define CLK_TOP_I2S2_MCK_SEL		91
+#define CLK_TOP_I2S3_MCK_SEL		92
+#define CLK_TOP_APLL1_DIV		93
+#define CLK_TOP_APLL2_DIV		94
+#define CLK_TOP_I2S0_MCK_DIV		95
+#define CLK_TOP_I2S1_MCK_DIV		96
+#define CLK_TOP_I2S2_MCK_DIV		97
+#define CLK_TOP_I2S3_MCK_DIV		98
+#define CLK_TOP_A1SYS_HP_DIV		99
+#define CLK_TOP_A2SYS_HP_DIV		100
+#define CLK_TOP_APLL1_DIV_PD		101
+#define CLK_TOP_APLL2_DIV_PD		102
+#define CLK_TOP_I2S0_MCK_DIV_PD		103
+#define CLK_TOP_I2S1_MCK_DIV_PD		104
+#define CLK_TOP_I2S2_MCK_DIV_PD		105
+#define CLK_TOP_I2S3_MCK_DIV_PD		106
+#define CLK_TOP_A1SYS_HP_DIV_PD		107
+#define CLK_TOP_A2SYS_HP_DIV_PD		108
+#define CLK_TOP_NR_CLK			109
+
+/* INFRACFG */
+
+#define CLK_INFRA_MUX1_SEL		0
+#define CLK_INFRA_DBGCLK_PD		1
+#define CLK_INFRA_AUDIO_PD		2
+#define CLK_INFRA_IRRX_PD		3
+#define CLK_INFRA_APXGPT_PD		4
+#define CLK_INFRA_PMIC_PD		5
+#define CLK_INFRA_TRNG			6
+#define CLK_INFRA_NR_CLK		7
+
+/* PERICFG */
+
+#define CLK_PERIBUS_SEL			0
+#define CLK_PERI_THERM_PD		1
+#define CLK_PERI_PWM1_PD		2
+#define CLK_PERI_PWM2_PD		3
+#define CLK_PERI_PWM3_PD		4
+#define CLK_PERI_PWM4_PD		5
+#define CLK_PERI_PWM5_PD		6
+#define CLK_PERI_PWM6_PD		7
+#define CLK_PERI_PWM7_PD		8
+#define CLK_PERI_PWM_PD			9
+#define CLK_PERI_AP_DMA_PD		10
+#define CLK_PERI_MSDC30_0_PD		11
+#define CLK_PERI_MSDC30_1_PD		12
+#define CLK_PERI_UART0_PD		13
+#define CLK_PERI_UART1_PD		14
+#define CLK_PERI_UART2_PD		15
+#define CLK_PERI_UART3_PD		16
+#define CLK_PERI_UART4_PD		17
+#define CLK_PERI_BTIF_PD		18
+#define CLK_PERI_I2C0_PD		19
+#define CLK_PERI_I2C1_PD		20
+#define CLK_PERI_I2C2_PD		21
+#define CLK_PERI_SPI1_PD		22
+#define CLK_PERI_AUXADC_PD		23
+#define CLK_PERI_SPI0_PD		24
+#define CLK_PERI_SNFI_PD		25
+#define CLK_PERI_NFI_PD			26
+#define CLK_PERI_NFIECC_PD		27
+#define CLK_PERI_FLASH_PD		28
+#define CLK_PERI_IRTX_PD		29
+#define CLK_PERI_NR_CLK			30
+
+/* APMIXEDSYS */
+
+#define CLK_APMIXED_ARMPLL		0
+#define CLK_APMIXED_MAINPLL		1
+#define CLK_APMIXED_UNIV2PLL		2
+#define CLK_APMIXED_ETH1PLL		3
+#define CLK_APMIXED_ETH2PLL		4
+#define CLK_APMIXED_AUD1PLL		5
+#define CLK_APMIXED_AUD2PLL		6
+#define CLK_APMIXED_TRGPLL		7
+#define CLK_APMIXED_SGMIPLL		8
+#define CLK_APMIXED_MAIN_CORE_EN	9
+#define CLK_APMIXED_NR_CLK		10
+
+/* AUDIOSYS */
+
+#define CLK_AUDIO_AFE			0
+#define CLK_AUDIO_HDMI			1
+#define CLK_AUDIO_SPDF			2
+#define CLK_AUDIO_APLL			3
+#define CLK_AUDIO_I2SIN1		4
+#define CLK_AUDIO_I2SIN2		5
+#define CLK_AUDIO_I2SIN3		6
+#define CLK_AUDIO_I2SIN4		7
+#define CLK_AUDIO_I2SO1			8
+#define CLK_AUDIO_I2SO2			9
+#define CLK_AUDIO_I2SO3			10
+#define CLK_AUDIO_I2SO4			11
+#define CLK_AUDIO_ASRCI1		12
+#define CLK_AUDIO_ASRCI2		13
+#define CLK_AUDIO_ASRCO1		14
+#define CLK_AUDIO_ASRCO2		15
+#define CLK_AUDIO_INTDIR		16
+#define CLK_AUDIO_A1SYS			17
+#define CLK_AUDIO_A2SYS			18
+#define CLK_AUDIO_UL1			19
+#define CLK_AUDIO_UL2			20
+#define CLK_AUDIO_UL3			21
+#define CLK_AUDIO_UL4			22
+#define CLK_AUDIO_UL5			23
+#define CLK_AUDIO_UL6			24
+#define CLK_AUDIO_DL1			25
+#define CLK_AUDIO_DL2			26
+#define CLK_AUDIO_DL3			27
+#define CLK_AUDIO_DL4			28
+#define CLK_AUDIO_DL5			29
+#define CLK_AUDIO_DL6			30
+#define CLK_AUDIO_DLMCH			31
+#define CLK_AUDIO_ARB1			32
+#define CLK_AUDIO_AWB			33
+#define CLK_AUDIO_AWB2			34
+#define CLK_AUDIO_DAI			35
+#define CLK_AUDIO_MOD			36
+#define CLK_AUDIO_ASRCI3		37
+#define CLK_AUDIO_ASRCI4		38
+#define CLK_AUDIO_ASRCO3		39
+#define CLK_AUDIO_ASRCO4		40
+#define CLK_AUDIO_MEM_ASRC1		41
+#define CLK_AUDIO_MEM_ASRC2		42
+#define CLK_AUDIO_MEM_ASRC3		43
+#define CLK_AUDIO_MEM_ASRC4		44
+#define CLK_AUDIO_MEM_ASRC5		45
+#define CLK_AUDIO_NR_CLK		46
+
+/* SSUSBSYS */
+
+#define CLK_SSUSB_U2_PHY_1P_EN		0
+#define CLK_SSUSB_U2_PHY_EN		1
+#define CLK_SSUSB_REF_EN		2
+#define CLK_SSUSB_SYS_EN		3
+#define CLK_SSUSB_MCU_EN		4
+#define CLK_SSUSB_DMA_EN		5
+#define CLK_SSUSB_NR_CLK		6
+
+/* PCIESYS */
+
+#define CLK_PCIE_P1_AUX_EN		0
+#define CLK_PCIE_P1_OBFF_EN		1
+#define CLK_PCIE_P1_AHB_EN		2
+#define CLK_PCIE_P1_AXI_EN		3
+#define CLK_PCIE_P1_MAC_EN		4
+#define CLK_PCIE_P1_PIPE_EN		5
+#define CLK_PCIE_P0_AUX_EN		6
+#define CLK_PCIE_P0_OBFF_EN		7
+#define CLK_PCIE_P0_AHB_EN		8
+#define CLK_PCIE_P0_AXI_EN		9
+#define CLK_PCIE_P0_MAC_EN		10
+#define CLK_PCIE_P0_PIPE_EN		11
+#define CLK_SATA_AHB_EN			12
+#define CLK_SATA_AXI_EN			13
+#define CLK_SATA_ASIC_EN		14
+#define CLK_SATA_RBC_EN			15
+#define CLK_SATA_PM_EN			16
+#define CLK_PCIE_NR_CLK			17
+
+/* ETHSYS */
+
+#define CLK_ETH_HSDMA_EN		0
+#define CLK_ETH_ESW_EN			1
+#define CLK_ETH_GP2_EN			2
+#define CLK_ETH_GP1_EN			3
+#define CLK_ETH_GP0_EN			4
+#define CLK_ETH_NR_CLK			5
+
+/* SGMIISYS */
+
+#define CLK_SGMII_TX250M_EN		0
+#define CLK_SGMII_RX250M_EN		1
+#define CLK_SGMII_CDR_REF		2
+#define CLK_SGMII_CDR_FB		3
+#define CLK_SGMII_NR_CLK		4
+
+#endif /* _DT_BINDINGS_CLK_MT7622_H */
+
