#!/bin/sh
#
# Copyright (C) 2012-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

board_config_update

board=$(board_name)

case "$board" in
"cisco,on100")
	ucidef_set_interface_lan "eth0 eth1"
	;;
"cloudengines,pogoe02"|\
"cloudengines,pogoplugv4"|\
"iom,iconnect-1.1"|\
"iom,ix2-200"|\
"raidsonic,ib-nas62x0"|\
"seagate,dockstar"|\
"seagate,goflexhome"|\
"seagate,goflexnet")
	ucidef_set_interface_lan "eth0" "dhcp"
	;;
"linksys,audi"|\
"linksys,viper")
	ucidef_add_switch "switch0" \
		"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "5@eth0" "6@eth1"
	;;
"zyxel,nsa310b"|\
"zyxel,nsa325")
	ucidef_set_interface_lan "eth0" "dhcp"
	ucidef_set_interface_macaddr "lan" $( mtd_get_mac_ascii uboot_env ethaddr )
	;;
*)
	ucidef_set_interface_lan "eth0"
	;;
esac

board_config_flush

exit 0
