From 5f0bb9d0bc545ef53a83f7bd176fdc0736eed8e5 Mon Sep 17 00:00:00 2001
From: Jens Kuske <jenskuske@gmail.com>
Date: Tue, 27 Oct 2015 17:50:24 +0100
Subject: [PATCH] reset: sunxi: Add Allwinner H3 bus resets

The H3 bus resets have some holes between the registers, so we add
an of_xlate() function to skip them according to the datasheet.

Signed-off-by: Jens Kuske <jenskuske@gmail.com>
---
 .../bindings/reset/allwinner,sunxi-clock-reset.txt |  1 +
 drivers/reset/reset-sunxi.c                        | 30 +++++++++++++++++++---
 2 files changed, 28 insertions(+), 3 deletions(-)

--- a/Documentation/devicetree/bindings/reset/allwinner,sunxi-clock-reset.txt
+++ b/Documentation/devicetree/bindings/reset/allwinner,sunxi-clock-reset.txt
@@ -8,6 +8,7 @@ Required properties:
 - compatible: Should be one of the following:
   "allwinner,sun6i-a31-ahb1-reset"
   "allwinner,sun6i-a31-clock-reset"
+  "allwinner,sun8i-h3-bus-reset"
 - reg: should be register base and length as documented in the
   datasheet
 - #reset-cells: 1, see below
--- a/drivers/reset/reset-sunxi.c
+++ b/drivers/reset/reset-sunxi.c
@@ -77,7 +77,9 @@ static const struct reset_control_ops su
 	.deassert	= sunxi_reset_deassert,
 };
 
-static int sunxi_reset_init(struct device_node *np)
+static int sunxi_reset_init(struct device_node *np,
+			    int (*of_xlate)(struct reset_controller_dev *rcdev,
+				    const struct of_phandle_args *reset_spec))
 {
 	struct sunxi_reset_data *data;
 	struct resource res;
@@ -110,6 +112,7 @@ static int sunxi_reset_init(struct devic
 	data->rcdev.nr_resets = size * 8;
 	data->rcdev.ops = &sunxi_reset_ops;
 	data->rcdev.of_node = np;
+	data->rcdev.of_xlate = of_xlate;
 
 	return reset_controller_register(&data->rcdev);
 
@@ -118,6 +121,21 @@ err_alloc:
 	return ret;
 };
 
+static int sun8i_h3_bus_reset_xlate(struct reset_controller_dev *rcdev,
+				    const struct of_phandle_args *reset_spec)
+{
+	unsigned int index = reset_spec->args[0];
+
+	if (index < 96)
+		return index;
+	else if (index < 128)
+		return index + 32;
+	else if (index < 160)
+		return index + 64;
+	else
+		return -EINVAL;
+}
+
 /*
  * These are the reset controller we need to initialize early on in
  * our system, before we can even think of using a regular device
@@ -125,15 +143,21 @@ err_alloc:
  */
 static const struct of_device_id sunxi_early_reset_dt_ids[] __initconst = {
 	{ .compatible = "allwinner,sun6i-a31-ahb1-reset", },
+	{ .compatible = "allwinner,sun8i-h3-bus-reset", .data = sun8i_h3_bus_reset_xlate, },
 	{ /* sentinel */ },
 };
 
 void __init sun6i_reset_init(void)
 {
 	struct device_node *np;
-
-	for_each_matching_node(np, sunxi_early_reset_dt_ids)
-		sunxi_reset_init(np);
+	const struct of_device_id *match;
+	int (*of_xlate)(struct reset_controller_dev *rcdev,
+			const struct of_phandle_args *reset_spec);
+
+	for_each_matching_node_and_match(np, sunxi_early_reset_dt_ids, &match) {
+		of_xlate = match->data;
+		sunxi_reset_init(np, of_xlate);
+	}
 }
 
 /*
