From 44586947e86f67ad71fdd3afca51f04fc27f3872 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Tue, 17 Jan 2017 11:34:58 +0000
Subject: [PATCH] BCM270X_DT: Enable UART0 on CM3

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2710-rpi-cm3.dts | 4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
@@ -6,6 +6,10 @@
 	model = "Raspberry Pi Compute Module 3";
 };
 
+&uart0 {
+	status = "okay";
+};
+
 &gpio {
 	sdhost_pins: sdhost_pins {
 		brcm,pins = <48 49 50 51 52 53>;
