From e9156cd26a495a18706e796f02a81fee41ec14f4 Mon Sep 17 00:00:00 2001
From: James Hughes <james.hughes@raspberrypi.org>
Date: Wed, 19 Apr 2017 11:13:40 +0100
Subject: [PATCH] smsc95xx: Use skb_cow_head to deal with cloned skbs

The driver was failing to check that the SKB wasn't cloned
before adding checksum data.
Replace existing handling to extend/copy the header buffer
with skb_cow_head.

Signed-off-by: James Hughes <james.hughes@raspberrypi.org>
Acked-by: Eric Dumazet <edumazet@google.com>
Acked-by: Woojung Huh <Woojung.Huh@microchip.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/usb/smsc95xx.c | 12 ++++++------
 1 file changed, 6 insertions(+), 6 deletions(-)

--- a/drivers/net/usb/smsc95xx.c
+++ b/drivers/net/usb/smsc95xx.c
@@ -2004,13 +2004,13 @@ static struct sk_buff *smsc95xx_tx_fixup
 	/* We do not advertise SG, so skbs should be already linearized */
 	BUG_ON(skb_shinfo(skb)->nr_frags);
 
-	if (skb_headroom(skb) < overhead) {
-		struct sk_buff *skb2 = skb_copy_expand(skb,
-			overhead, 0, flags);
+	/* Make writable and expand header space by overhead if required */
+	if (skb_cow_head(skb, overhead)) {
+		/* Must deallocate here as returning NULL to indicate error
+		 * means the skb won't be deallocated in the caller.
+		 */
 		dev_kfree_skb_any(skb);
-		skb = skb2;
-		if (!skb)
-			return NULL;
+		return NULL;
 	}
 
 	if (csum) {
