From 6ad20165d376fa07919a70e4f43dfae564601829 Mon Sep 17 00:00:00 2001
From: Eric Dumazet <edumazet@google.com>
Date: Mon, 30 Jan 2017 08:22:01 -0800
Subject: drivers: net: generalize napi_complete_done()

napi_complete_done() allows to opt-in for gro_flush_timeout,
added back in linux-3.19, commit 3b47d30396ba
("net: gro: add a per device gro flush timer")

This allows for more efficient GRO aggregation without
sacrifying latencies.

Signed-off-by: Eric Dumazet <edumazet@google.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/can/at91_can.c                          |  2 +-
 drivers/net/can/c_can/c_can.c                       |  2 +-
 drivers/net/can/flexcan.c                           |  2 +-
 drivers/net/can/ifi_canfd/ifi_canfd.c               |  2 +-
 drivers/net/can/janz-ican3.c                        |  2 +-
 drivers/net/can/m_can/m_can.c                       |  2 +-
 drivers/net/can/rcar/rcar_can.c                     |  2 +-
 drivers/net/can/rcar/rcar_canfd.c                   |  2 +-
 drivers/net/can/xilinx_can.c                        |  2 +-
 drivers/net/ethernet/3com/typhoon.c                 |  2 +-
 drivers/net/ethernet/adi/bfin_mac.c                 |  2 +-
 drivers/net/ethernet/agere/et131x.c                 |  2 +-
 drivers/net/ethernet/altera/altera_tse_main.c       |  2 +-
 drivers/net/ethernet/apm/xgene/xgene_enet_main.c    |  2 +-
 drivers/net/ethernet/aquantia/atlantic/aq_vec.c     |  2 +-
 drivers/net/ethernet/arc/emac_main.c                |  2 +-
 drivers/net/ethernet/atheros/alx/main.c             |  2 +-
 drivers/net/ethernet/atheros/atl1c/atl1c_main.c     |  2 +-
 drivers/net/ethernet/atheros/atl1e/atl1e_main.c     |  2 +-
 drivers/net/ethernet/atheros/atlx/atl1.c            |  2 +-
 drivers/net/ethernet/broadcom/b44.c                 |  2 +-
 drivers/net/ethernet/broadcom/bcm63xx_enet.c        |  2 +-
 drivers/net/ethernet/broadcom/bgmac.c               |  2 +-
 drivers/net/ethernet/broadcom/bnx2.c                |  4 ++--
 drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c     |  2 +-
 drivers/net/ethernet/broadcom/bnxt/bnxt.c           |  2 +-
 drivers/net/ethernet/broadcom/sb1250-mac.c          |  2 +-
 drivers/net/ethernet/brocade/bna/bnad.c             |  2 +-
 drivers/net/ethernet/cadence/macb.c                 |  2 +-
 drivers/net/ethernet/calxeda/xgmac.c                |  2 +-
 drivers/net/ethernet/cavium/liquidio/lio_main.c     |  2 +-
 drivers/net/ethernet/cavium/liquidio/lio_vf_main.c  |  2 +-
 drivers/net/ethernet/cavium/octeon/octeon_mgmt.c    |  2 +-
 drivers/net/ethernet/cavium/thunder/nicvf_main.c    |  2 +-
 drivers/net/ethernet/chelsio/cxgb/sge.c             |  2 +-
 drivers/net/ethernet/chelsio/cxgb3/sge.c            |  4 ++--
 drivers/net/ethernet/chelsio/cxgb4vf/sge.c          |  2 +-
 drivers/net/ethernet/cisco/enic/enic_main.c         |  4 ++--
 drivers/net/ethernet/dec/tulip/interrupt.c          |  6 +++---
 drivers/net/ethernet/dnet.c                         |  2 +-
 drivers/net/ethernet/emulex/benet/be_main.c         |  2 +-
 drivers/net/ethernet/ethoc.c                        |  2 +-
 drivers/net/ethernet/ezchip/nps_enet.c              |  2 +-
 drivers/net/ethernet/freescale/dpaa/dpaa_eth.c      |  2 +-
 drivers/net/ethernet/freescale/fec_main.c           |  2 +-
 .../net/ethernet/freescale/fs_enet/fs_enet-main.c   |  2 +-
 drivers/net/ethernet/freescale/gianfar.c            |  4 ++--
 drivers/net/ethernet/freescale/ucc_geth.c           |  2 +-
 drivers/net/ethernet/hisilicon/hip04_eth.c          |  2 +-
 drivers/net/ethernet/hisilicon/hisi_femac.c         |  2 +-
 drivers/net/ethernet/hisilicon/hix5hd2_gmac.c       |  2 +-
 drivers/net/ethernet/ibm/ibmveth.c                  |  2 +-
 drivers/net/ethernet/ibm/ibmvnic.c                  |  2 +-
 drivers/net/ethernet/intel/e100.c                   |  2 +-
 drivers/net/ethernet/intel/ixgb/ixgb_main.c         |  2 +-
 drivers/net/ethernet/korina.c                       |  2 +-
 drivers/net/ethernet/lantiq_etop.c                  | 21 +++++++++------------
 drivers/net/ethernet/marvell/mv643xx_eth.c          |  2 +-
 drivers/net/ethernet/marvell/mvneta.c               |  6 ++----
 drivers/net/ethernet/marvell/mvpp2.c                |  2 +-
 drivers/net/ethernet/marvell/pxa168_eth.c           |  2 +-
 drivers/net/ethernet/moxa/moxart_ether.c            |  2 +-
 drivers/net/ethernet/myricom/myri10ge/myri10ge.c    |  2 +-
 drivers/net/ethernet/natsemi/natsemi.c              |  2 +-
 drivers/net/ethernet/neterion/s2io.c                |  4 ++--
 drivers/net/ethernet/neterion/vxge/vxge-main.c      |  6 +++---
 drivers/net/ethernet/nvidia/forcedeth.c             |  2 +-
 drivers/net/ethernet/nxp/lpc_eth.c                  |  2 +-
 .../net/ethernet/oki-semi/pch_gbe/pch_gbe_main.c    |  2 +-
 drivers/net/ethernet/pasemi/pasemi_mac.c            |  2 +-
 .../net/ethernet/qlogic/netxen/netxen_nic_main.c    |  2 +-
 drivers/net/ethernet/qlogic/qede/qede_fp.c          |  2 +-
 drivers/net/ethernet/qlogic/qlcnic/qlcnic_io.c      | 10 +++++-----
 drivers/net/ethernet/qlogic/qlge/qlge_main.c        |  2 +-
 drivers/net/ethernet/qualcomm/emac/emac.c           |  2 +-
 drivers/net/ethernet/realtek/r8169.c                |  2 +-
 drivers/net/ethernet/rocker/rocker_main.c           |  2 +-
 drivers/net/ethernet/samsung/sxgbe/sxgbe_main.c     |  2 +-
 drivers/net/ethernet/sfc/efx.c                      |  2 +-
 drivers/net/ethernet/sfc/falcon/efx.c               |  2 +-
 drivers/net/ethernet/smsc/smsc9420.c                |  2 +-
 drivers/net/ethernet/stmicro/stmmac/stmmac_main.c   |  2 +-
 drivers/net/ethernet/sun/niu.c                      |  2 +-
 drivers/net/ethernet/sun/sungem.c                   |  2 +-
 drivers/net/ethernet/sun/sunvnet_common.c           |  2 +-
 drivers/net/ethernet/tehuti/tehuti.c                |  2 +-
 drivers/net/ethernet/ti/cpsw.c                      |  2 +-
 drivers/net/ethernet/ti/davinci_emac.c              |  2 +-
 drivers/net/ethernet/ti/netcp_core.c                |  2 +-
 drivers/net/ethernet/tile/tilegx.c                  |  2 +-
 drivers/net/ethernet/tile/tilepro.c                 |  2 +-
 drivers/net/ethernet/toshiba/ps3_gelic_net.c        |  2 +-
 drivers/net/ethernet/toshiba/spider_net.c           |  2 +-
 drivers/net/ethernet/toshiba/tc35815.c              |  2 +-
 drivers/net/ethernet/tundra/tsi108_eth.c            |  2 +-
 drivers/net/ethernet/via/via-rhine.c                |  2 +-
 drivers/net/ethernet/via/via-velocity.c             |  2 +-
 drivers/net/ethernet/wiznet/w5100.c                 |  2 +-
 drivers/net/ethernet/wiznet/w5300.c                 |  2 +-
 drivers/net/fjes/fjes_main.c                        |  2 +-
 drivers/net/vmxnet3/vmxnet3_drv.c                   |  4 ++--
 drivers/net/wan/fsl_ucc_hdlc.c                      |  2 +-
 drivers/net/wan/hd64572.c                           |  2 +-
 drivers/net/wireless/ath/ath10k/pci.c               |  2 +-
 drivers/net/wireless/ath/wil6210/netdev.c           |  2 +-
 drivers/net/xen-netback/interface.c                 |  2 +-
 drivers/net/xen-netfront.c                          |  2 +-
 drivers/staging/octeon/ethernet-rx.c                |  2 +-
 drivers/staging/unisys/visornic/visornic_main.c     |  2 +-
 109 files changed, 132 insertions(+), 137 deletions(-)

--- a/drivers/net/can/at91_can.c
+++ b/drivers/net/can/at91_can.c
@@ -813,7 +813,7 @@ static int at91_poll(struct napi_struct
 		u32 reg_ier = AT91_IRQ_ERR_FRAME;
 		reg_ier |= get_irq_mb_rx(priv) & ~AT91_MB_MASK(priv->rx_next);
 
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		at91_write(priv, AT91_IER, reg_ier);
 	}
 
--- a/drivers/net/can/c_can/c_can.c
+++ b/drivers/net/can/c_can/c_can.c
@@ -1070,7 +1070,7 @@ static int c_can_poll(struct napi_struct
 
 end:
 	if (work_done < quota) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		/* enable all IRQs if we are not in bus off state */
 		if (priv->can.state != CAN_STATE_BUS_OFF)
 			c_can_irq_control(priv, true);
--- a/drivers/net/can/flexcan.c
+++ b/drivers/net/can/flexcan.c
@@ -703,7 +703,7 @@ static int flexcan_poll(struct napi_stru
 		work_done += flexcan_poll_bus_err(dev, reg_esr);
 
 	if (work_done < quota) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		/* enable IRQs */
 		flexcan_write(FLEXCAN_IFLAG_DEFAULT, &regs->imask1);
 		flexcan_write(priv->reg_ctrl_default, &regs->ctrl);
--- a/drivers/net/can/ifi_canfd/ifi_canfd.c
+++ b/drivers/net/can/ifi_canfd/ifi_canfd.c
@@ -589,7 +589,7 @@ static int ifi_canfd_poll(struct napi_st
 		work_done += ifi_canfd_do_rx_poll(ndev, quota - work_done);
 
 	if (work_done < quota) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		ifi_canfd_irq_enable(ndev, 1);
 	}
 
--- a/drivers/net/can/janz-ican3.c
+++ b/drivers/net/can/janz-ican3.c
@@ -1475,7 +1475,7 @@ static int ican3_napi(struct napi_struct
 	/* We have processed all packets that the adapter had, but it
 	 * was less than our budget, stop polling */
 	if (received < budget)
-		napi_complete(napi);
+		napi_complete_done(napi, received);
 
 	spin_lock_irqsave(&mod->lock, flags);
 
--- a/drivers/net/can/m_can/m_can.c
+++ b/drivers/net/can/m_can/m_can.c
@@ -730,7 +730,7 @@ static int m_can_poll(struct napi_struct
 		work_done += m_can_do_rx_poll(dev, (quota - work_done));
 
 	if (work_done < quota) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		m_can_enable_all_interrupts(priv);
 	}
 
--- a/drivers/net/can/rcar/rcar_can.c
+++ b/drivers/net/can/rcar/rcar_can.c
@@ -695,7 +695,7 @@ static int rcar_can_rx_poll(struct napi_
 	}
 	/* All packets processed */
 	if (num_pkts < quota) {
-		napi_complete(napi);
+		napi_complete_done(napi, num_pkts);
 		priv->ier |= RCAR_CAN_IER_RXFIE;
 		writeb(priv->ier, &priv->regs->ier);
 	}
--- a/drivers/net/can/rcar/rcar_canfd.c
+++ b/drivers/net/can/rcar/rcar_canfd.c
@@ -1512,7 +1512,7 @@ static int rcar_canfd_rx_poll(struct nap
 
 	/* All packets processed */
 	if (num_pkts < quota) {
-		napi_complete(napi);
+		napi_complete_done(napi, num_pkts);
 		/* Enable Rx FIFO interrupts */
 		rcar_canfd_set_bit(priv->base, RCANFD_RFCC(ridx),
 				   RCANFD_RFCC_RFIE);
--- a/drivers/net/can/xilinx_can.c
+++ b/drivers/net/can/xilinx_can.c
@@ -838,7 +838,7 @@ static int xcan_rx_poll(struct napi_stru
 	}
 
 	if (work_done < quota) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		ier = priv->read_reg(priv, XCAN_IER_OFFSET);
 		ier |= XCAN_IXR_RXNEMP_MASK;
 		priv->write_reg(priv, XCAN_IER_OFFSET, ier);
--- a/drivers/net/ethernet/3com/typhoon.c
+++ b/drivers/net/ethernet/3com/typhoon.c
@@ -1748,7 +1748,7 @@ typhoon_poll(struct napi_struct *napi, i
 	}
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		iowrite32(TYPHOON_INTR_NONE,
 				tp->ioaddr + TYPHOON_REG_INTR_MASK);
 		typhoon_post_pci_writes(tp->ioaddr);
--- a/drivers/net/ethernet/adi/bfin_mac.c
+++ b/drivers/net/ethernet/adi/bfin_mac.c
@@ -1274,7 +1274,7 @@ static int bfin_mac_poll(struct napi_str
 	}
 
 	if (i < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, i);
 		if (test_and_clear_bit(BFIN_MAC_RX_IRQ_DISABLED, &lp->flags))
 			enable_irq(IRQ_MAC_RX);
 	}
--- a/drivers/net/ethernet/agere/et131x.c
+++ b/drivers/net/ethernet/agere/et131x.c
@@ -3573,7 +3573,7 @@ static int et131x_poll(struct napi_struc
 	et131x_handle_send_pkts(adapter);
 
 	if (work_done < budget) {
-		napi_complete(&adapter->napi);
+		napi_complete_done(&adapter->napi, work_done);
 		et131x_enable_interrupts(adapter);
 	}
 
--- a/drivers/net/ethernet/altera/altera_tse_main.c
+++ b/drivers/net/ethernet/altera/altera_tse_main.c
@@ -491,7 +491,7 @@ static int tse_poll(struct napi_struct *
 
 	if (rxcomplete < budget) {
 
-		napi_complete(napi);
+		napi_complete_done(napi, rxcomplete);
 
 		netdev_dbg(priv->dev,
 			   "NAPI Complete, did %d packets with budget %d\n",
--- a/drivers/net/ethernet/apm/xgene/xgene_enet_main.c
+++ b/drivers/net/ethernet/apm/xgene/xgene_enet_main.c
@@ -658,7 +658,7 @@ static int xgene_enet_napi(struct napi_s
 	processed = xgene_enet_process_ring(ring, budget);
 
 	if (processed != budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, processed);
 		enable_irq(ring->irq);
 	}
 
--- a/drivers/net/ethernet/arc/emac_main.c
+++ b/drivers/net/ethernet/arc/emac_main.c
@@ -284,7 +284,7 @@ static int arc_emac_poll(struct napi_str
 
 	work_done = arc_emac_rx(ndev, budget);
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		arc_reg_or(priv, R_ENABLE, RXINT_MASK | TXINT_MASK);
 	}
 
--- a/drivers/net/ethernet/atheros/alx/main.c
+++ b/drivers/net/ethernet/atheros/alx/main.c
@@ -292,7 +292,7 @@ static int alx_poll(struct napi_struct *
 	if (!tx_complete || work == budget)
 		return budget;
 
-	napi_complete(&alx->napi);
+	napi_complete_done(&alx->napi, work);
 
 	/* enable interrupt */
 	if (alx->flags & ALX_FLAG_USING_MSIX) {
--- a/drivers/net/ethernet/atheros/atl1c/atl1c_main.c
+++ b/drivers/net/ethernet/atheros/atl1c/atl1c_main.c
@@ -1886,7 +1886,7 @@ static int atl1c_clean(struct napi_struc
 
 	if (work_done < budget) {
 quit_polling:
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		adapter->hw.intr_mask |= ISR_RX_PKT;
 		AT_WRITE_REG(&adapter->hw, REG_IMR, adapter->hw.intr_mask);
 	}
--- a/drivers/net/ethernet/atheros/atl1e/atl1e_main.c
+++ b/drivers/net/ethernet/atheros/atl1e/atl1e_main.c
@@ -1532,7 +1532,7 @@ static int atl1e_clean(struct napi_struc
 	/* If no Tx and not enough Rx work done, exit the polling mode */
 	if (work_done < budget) {
 quit_polling:
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		imr_data = AT_READ_REG(&adapter->hw, REG_IMR);
 		AT_WRITE_REG(&adapter->hw, REG_IMR, imr_data | ISR_RX_EVENT);
 		/* test debug */
--- a/drivers/net/ethernet/atheros/atlx/atl1.c
+++ b/drivers/net/ethernet/atheros/atlx/atl1.c
@@ -2457,7 +2457,7 @@ static int atl1_rings_clean(struct napi_
 	if (work_done >= budget)
 		return work_done;
 
-	napi_complete(napi);
+	napi_complete_done(napi, work_done);
 	/* re-enable Interrupt */
 	if (likely(adapter->int_enabled))
 		atlx_imr_set(adapter, IMR_NORMAL_MASK);
--- a/drivers/net/ethernet/broadcom/b44.c
+++ b/drivers/net/ethernet/broadcom/b44.c
@@ -902,7 +902,7 @@ static int b44_poll(struct napi_struct *
 	}
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		b44_enable_ints(bp);
 	}
 
--- a/drivers/net/ethernet/broadcom/bcm63xx_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm63xx_enet.c
@@ -511,7 +511,7 @@ static int bcm_enet_poll(struct napi_str
 
 	/* no more packet in rx/tx queue, remove device from poll
 	 * queue */
-	napi_complete(napi);
+	napi_complete_done(napi, rx_work_done);
 
 	/* restore rx/tx interrupt */
 	enet_dmac_writel(priv, priv->dma_chan_int_mask,
--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -1146,7 +1146,7 @@ static int bgmac_poll(struct napi_struct
 		return weight;
 
 	if (handled < weight) {
-		napi_complete(napi);
+		napi_complete_done(napi, handled);
 		bgmac_chip_intrs_on(bgmac);
 	}
 
--- a/drivers/net/ethernet/broadcom/bnx2.c
+++ b/drivers/net/ethernet/broadcom/bnx2.c
@@ -3522,7 +3522,7 @@ static int bnx2_poll_msix(struct napi_st
 		rmb();
 		if (likely(!bnx2_has_fast_work(bnapi))) {
 
-			napi_complete(napi);
+			napi_complete_done(napi, work_done);
 			BNX2_WR(bp, BNX2_PCICFG_INT_ACK_CMD, bnapi->int_num |
 				BNX2_PCICFG_INT_ACK_CMD_INDEX_VALID |
 				bnapi->last_status_idx);
@@ -3559,7 +3559,7 @@ static int bnx2_poll(struct napi_struct
 
 		rmb();
 		if (likely(!bnx2_has_work(bnapi))) {
-			napi_complete(napi);
+			napi_complete_done(napi, work_done);
 			if (likely(bp->flags & BNX2_FLAG_USING_MSI_OR_MSIX)) {
 				BNX2_WR(bp, BNX2_PCICFG_INT_ACK_CMD,
 					BNX2_PCICFG_INT_ACK_CMD_INDEX_VALID |
--- a/drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c
+++ b/drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c
@@ -3236,7 +3236,7 @@ static int bnx2x_poll(struct napi_struct
 		 * has been updated when NAPI was scheduled.
 		 */
 		if (IS_FCOE_FP(fp)) {
-			napi_complete(napi);
+			napi_complete_done(napi, rx_work_done);
 		} else {
 			bnx2x_update_fpsb_idx(fp);
 			/* bnx2x_has_rx_work() reads the status block,
--- a/drivers/net/ethernet/broadcom/bnxt/bnxt.c
+++ b/drivers/net/ethernet/broadcom/bnxt/bnxt.c
@@ -1781,7 +1781,7 @@ static int bnxt_poll_nitroa0(struct napi
 	}
 
 	if (!bnxt_has_work(bp, cpr) && rx_pkts < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rx_pkts);
 		BNXT_CP_DB_REARM(cpr->cp_doorbell, cpr->cp_raw_cons);
 	}
 	return rx_pkts;
--- a/drivers/net/ethernet/broadcom/sb1250-mac.c
+++ b/drivers/net/ethernet/broadcom/sb1250-mac.c
@@ -2545,7 +2545,7 @@ static int sbmac_poll(struct napi_struct
 	sbdma_tx_process(sc, &(sc->sbm_txdma), 1);
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 #ifdef CONFIG_SBMAC_COALESCE
 		__raw_writeq(((M_MAC_INT_EOP_COUNT | M_MAC_INT_EOP_TIMER) << S_MAC_TX_CH0) |
--- a/drivers/net/ethernet/brocade/bna/bnad.c
+++ b/drivers/net/ethernet/brocade/bna/bnad.c
@@ -1881,7 +1881,7 @@ bnad_napi_poll_rx(struct napi_struct *na
 		return rcvd;
 
 poll_exit:
-	napi_complete(napi);
+	napi_complete_done(napi, rcvd);
 
 	rx_ctrl->rx_complete++;
 
--- a/drivers/net/ethernet/cadence/macb.c
+++ b/drivers/net/ethernet/cadence/macb.c
@@ -1069,7 +1069,7 @@ static int macb_poll(struct napi_struct
 
 	work_done = bp->macbgem_ops.mog_rx(bp, budget);
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		/* Packets received while interrupts were disabled */
 		status = macb_readl(bp, RSR);
--- a/drivers/net/ethernet/calxeda/xgmac.c
+++ b/drivers/net/ethernet/calxeda/xgmac.c
@@ -1247,7 +1247,7 @@ static int xgmac_poll(struct napi_struct
 	work_done = xgmac_rx(priv, budget);
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		__raw_writel(DMA_INTR_DEFAULT_MASK, priv->base + XGMAC_DMA_INTR_ENA);
 	}
 	return work_done;
--- a/drivers/net/ethernet/cavium/liquidio/lio_main.c
+++ b/drivers/net/ethernet/cavium/liquidio/lio_main.c
@@ -2433,7 +2433,7 @@ static int liquidio_napi_poll(struct nap
 	}
 
 	if ((work_done < budget) && (tx_done)) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		octeon_process_droq_poll_cmd(droq->oct_dev, droq->q_no,
 					     POLL_EVENT_ENABLE_INTR, 0);
 		return 0;
--- a/drivers/net/ethernet/cavium/octeon/octeon_mgmt.c
+++ b/drivers/net/ethernet/cavium/octeon/octeon_mgmt.c
@@ -501,7 +501,7 @@ static int octeon_mgmt_napi_poll(struct
 
 	if (work_done < budget) {
 		/* We stopped because no more packets were available. */
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		octeon_mgmt_enable_rx_irq(p);
 	}
 	octeon_mgmt_update_rx_stats(netdev);
--- a/drivers/net/ethernet/cavium/thunder/nicvf_main.c
+++ b/drivers/net/ethernet/cavium/thunder/nicvf_main.c
@@ -737,7 +737,7 @@ static int nicvf_poll(struct napi_struct
 
 	if (work_done < budget) {
 		/* Slow packet rate, exit polling */
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		/* Re-enable interrupts */
 		cq_head = nicvf_queue_reg_read(nic, NIC_QSET_CQ_0_7_HEAD,
 					       cq->cq_idx);
--- a/drivers/net/ethernet/chelsio/cxgb/sge.c
+++ b/drivers/net/ethernet/chelsio/cxgb/sge.c
@@ -1605,7 +1605,7 @@ int t1_poll(struct napi_struct *napi, in
 	int work_done = process_responses(adapter, budget);
 
 	if (likely(work_done < budget)) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		writel(adapter->sge->respQ.cidx,
 		       adapter->regs + A_SG_SLEEPING);
 	}
--- a/drivers/net/ethernet/chelsio/cxgb3/sge.c
+++ b/drivers/net/ethernet/chelsio/cxgb3/sge.c
@@ -1843,7 +1843,7 @@ static int ofld_poll(struct napi_struct
 		__skb_queue_head_init(&queue);
 		skb_queue_splice_init(&q->rx_queue, &queue);
 		if (skb_queue_empty(&queue)) {
-			napi_complete(napi);
+			napi_complete_done(napi, work_done);
 			spin_unlock_irq(&q->lock);
 			return work_done;
 		}
@@ -2414,7 +2414,7 @@ static int napi_rx_handler(struct napi_s
 	int work_done = process_responses(adap, qs, budget);
 
 	if (likely(work_done < budget)) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		/*
 		 * Because we don't atomically flush the following
--- a/drivers/net/ethernet/chelsio/cxgb4vf/sge.c
+++ b/drivers/net/ethernet/chelsio/cxgb4vf/sge.c
@@ -1889,7 +1889,7 @@ static int napi_rx_handler(struct napi_s
 	u32 val;
 
 	if (likely(work_done < budget)) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		intr_params = rspq->next_intr_params;
 		rspq->next_intr_params = rspq->intr_params;
 	} else
--- a/drivers/net/ethernet/cisco/enic/enic_main.c
+++ b/drivers/net/ethernet/cisco/enic/enic_main.c
@@ -1339,7 +1339,7 @@ static int enic_poll(struct napi_struct
 		 * exit polling
 		 */
 
-		napi_complete(napi);
+		napi_complete_done(napi, rq_work_done);
 		if (enic->rx_coalesce_setting.use_adaptive_rx_coalesce)
 			enic_set_int_moderation(enic, &enic->rq[0]);
 		vnic_intr_unmask(&enic->intr[intr]);
@@ -1496,7 +1496,7 @@ static int enic_poll_msix_rq(struct napi
 		 * exit polling
 		 */
 
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		if (enic->rx_coalesce_setting.use_adaptive_rx_coalesce)
 			enic_set_int_moderation(enic, &enic->rq[rq]);
 		vnic_intr_unmask(&enic->intr[intr]);
--- a/drivers/net/ethernet/dec/tulip/interrupt.c
+++ b/drivers/net/ethernet/dec/tulip/interrupt.c
@@ -319,8 +319,8 @@ int tulip_poll(struct napi_struct *napi,
 
          /* Remove us from polling list and enable RX intr. */
 
-         napi_complete(napi);
-         iowrite32(tulip_tbl[tp->chip_id].valid_intrs, tp->base_addr+CSR7);
+	napi_complete_done(napi, work_done);
+	iowrite32(tulip_tbl[tp->chip_id].valid_intrs, tp->base_addr+CSR7);
 
          /* The last op happens after poll completion. Which means the following:
           * 1. it can race with disabling irqs in irq handler
@@ -355,7 +355,7 @@ int tulip_poll(struct napi_struct *napi,
           * before we did napi_complete(). See? We would lose it. */
 
          /* remove ourselves from the polling list */
-         napi_complete(napi);
+         napi_complete_done(napi, work_done);
 
          return work_done;
 }
--- a/drivers/net/ethernet/dnet.c
+++ b/drivers/net/ethernet/dnet.c
@@ -415,7 +415,7 @@ static int dnet_poll(struct napi_struct
 		/* We processed all packets available.  Tell NAPI it can
 		 * stop polling then re-enable rx interrupts.
 		 */
-		napi_complete(napi);
+		napi_complete_done(napi, npackets);
 		int_enable = dnet_readl(bp, INTR_ENB);
 		int_enable |= DNET_INTR_SRC_RX_CMDFIFOAF;
 		dnet_writel(bp, int_enable, INTR_ENB);
--- a/drivers/net/ethernet/emulex/benet/be_main.c
+++ b/drivers/net/ethernet/emulex/benet/be_main.c
@@ -3344,7 +3344,7 @@ int be_poll(struct napi_struct *napi, in
 		be_process_mcc(adapter);
 
 	if (max_work < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, max_work);
 
 		/* Skyhawk EQ_DB has a provision to set the rearm to interrupt
 		 * delay via a delay multiplier encoding value
--- a/drivers/net/ethernet/ethoc.c
+++ b/drivers/net/ethernet/ethoc.c
@@ -614,7 +614,7 @@ static int ethoc_poll(struct napi_struct
 	tx_work_done = ethoc_tx(priv->netdev, budget);
 
 	if (rx_work_done < budget && tx_work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rx_work_done);
 		ethoc_enable_irq(priv, INT_MASK_TX | INT_MASK_RX);
 	}
 
--- a/drivers/net/ethernet/ezchip/nps_enet.c
+++ b/drivers/net/ethernet/ezchip/nps_enet.c
@@ -192,7 +192,7 @@ static int nps_enet_poll(struct napi_str
 	if (work_done < budget) {
 		u32 buf_int_enable_value = 0;
 
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		/* set tx_done and rx_rdy bits */
 		buf_int_enable_value |= NPS_ENET_ENABLE << RX_RDY_SHIFT;
--- a/drivers/net/ethernet/freescale/fec_main.c
+++ b/drivers/net/ethernet/freescale/fec_main.c
@@ -1623,7 +1623,7 @@ static int fec_enet_rx_napi(struct napi_
 	fec_enet_tx(ndev);
 
 	if (pkts < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, pkts);
 		writel(FEC_DEFAULT_IMASK, fep->hwp + FEC_IMASK);
 	}
 	return pkts;
--- a/drivers/net/ethernet/freescale/fs_enet/fs_enet-main.c
+++ b/drivers/net/ethernet/freescale/fs_enet/fs_enet-main.c
@@ -301,7 +301,7 @@ static int fs_enet_napi(struct napi_stru
 
 	if (received < budget && tx_left) {
 		/* done */
-		napi_complete(napi);
+		napi_complete_done(napi, received);
 		(*fep->ops->napi_enable)(dev);
 
 		return received;
--- a/drivers/net/ethernet/freescale/gianfar.c
+++ b/drivers/net/ethernet/freescale/gianfar.c
@@ -3197,7 +3197,7 @@ static int gfar_poll_rx_sq(struct napi_s
 
 	if (work_done < budget) {
 		u32 imask;
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		/* Clear the halt bit in RSTAT */
 		gfar_write(&regs->rstat, gfargrp->rstat);
 
@@ -3286,7 +3286,7 @@ static int gfar_poll_rx(struct napi_stru
 
 	if (!num_act_queues) {
 		u32 imask;
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		/* Clear the halt bit in RSTAT */
 		gfar_write(&regs->rstat, gfargrp->rstat);
--- a/drivers/net/ethernet/freescale/ucc_geth.c
+++ b/drivers/net/ethernet/freescale/ucc_geth.c
@@ -3301,7 +3301,7 @@ static int ucc_geth_poll(struct napi_str
 		howmany += ucc_geth_rx(ugeth, i, budget - howmany);
 
 	if (howmany < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, howmany);
 		setbits32(ugeth->uccf->p_uccm, UCCE_RX_EVENTS | UCCE_TX_EVENTS);
 	}
 
--- a/drivers/net/ethernet/hisilicon/hip04_eth.c
+++ b/drivers/net/ethernet/hisilicon/hip04_eth.c
@@ -555,7 +555,7 @@ refill:
 		priv->reg_inten |= RCV_INT;
 		writel_relaxed(priv->reg_inten, priv->base + PPE_INTEN);
 	}
-	napi_complete(napi);
+	napi_complete_done(napi, rx);
 done:
 	/* clean up tx descriptors and start a new timer if necessary */
 	tx_remaining = hip04_tx_reclaim(ndev, false);
--- a/drivers/net/ethernet/hisilicon/hisi_femac.c
+++ b/drivers/net/ethernet/hisilicon/hisi_femac.c
@@ -330,7 +330,7 @@ static int hisi_femac_poll(struct napi_s
 	} while (ints & DEF_INT_MASK);
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		hisi_femac_irq_enable(priv, DEF_INT_MASK &
 					(~IRQ_INT_TX_PER_PACKET));
 	}
--- a/drivers/net/ethernet/hisilicon/hix5hd2_gmac.c
+++ b/drivers/net/ethernet/hisilicon/hix5hd2_gmac.c
@@ -578,7 +578,7 @@ static int hix5hd2_poll(struct napi_stru
 	} while (ints & DEF_INT_MASK);
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		hix5hd2_irq_enable(priv);
 	}
 
--- a/drivers/net/ethernet/ibm/ibmveth.c
+++ b/drivers/net/ethernet/ibm/ibmveth.c
@@ -1320,7 +1320,7 @@ restart_poll:
 	ibmveth_replenish_task(adapter);
 
 	if (frames_processed < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, frames_processed);
 
 		/* We think we are done - reenable interrupts,
 		 * then check once more to make sure we are done.
--- a/drivers/net/ethernet/ibm/ibmvnic.c
+++ b/drivers/net/ethernet/ibm/ibmvnic.c
@@ -1028,7 +1028,7 @@ restart_poll:
 
 	if (frames_processed < budget) {
 		enable_scrq_irq(adapter, adapter->rx_scrq[scrq_num]);
-		napi_complete(napi);
+		napi_complete_done(napi, frames_processed);
 		if (pending_scrq(adapter, adapter->rx_scrq[scrq_num]) &&
 		    napi_reschedule(napi)) {
 			disable_scrq_irq(adapter, adapter->rx_scrq[scrq_num]);
--- a/drivers/net/ethernet/intel/e100.c
+++ b/drivers/net/ethernet/intel/e100.c
@@ -2253,7 +2253,7 @@ static int e100_poll(struct napi_struct
 
 	/* If budget not fully consumed, exit the polling mode */
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		e100_enable_irq(nic);
 	}
 
--- a/drivers/net/ethernet/intel/ixgb/ixgb_main.c
+++ b/drivers/net/ethernet/intel/ixgb/ixgb_main.c
@@ -1825,7 +1825,7 @@ ixgb_clean(struct napi_struct *napi, int
 
 	/* If budget not fully consumed, exit the polling mode */
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		if (!test_bit(__IXGB_DOWN, &adapter->flags))
 			ixgb_irq_enable(adapter);
 	}
--- a/drivers/net/ethernet/korina.c
+++ b/drivers/net/ethernet/korina.c
@@ -464,7 +464,7 @@ static int korina_poll(struct napi_struc
 
 	work_done = korina_rx(dev, budget);
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		writel(readl(&lp->rx_dma_regs->dmasm) &
 			~(DMA_STAT_DONE | DMA_STAT_HALT | DMA_STAT_ERR),
--- a/drivers/net/ethernet/lantiq_etop.c
+++ b/drivers/net/ethernet/lantiq_etop.c
@@ -156,24 +156,21 @@ ltq_etop_poll_rx(struct napi_struct *nap
 {
 	struct ltq_etop_chan *ch = container_of(napi,
 				struct ltq_etop_chan, napi);
-	int rx = 0;
-	int complete = 0;
+	int work_done = 0;
 
-	while ((rx < budget) && !complete) {
+	while (work_done < budget) {
 		struct ltq_dma_desc *desc = &ch->dma.desc_base[ch->dma.desc];
 
-		if ((desc->ctl & (LTQ_DMA_OWN | LTQ_DMA_C)) == LTQ_DMA_C) {
-			ltq_etop_hw_receive(ch);
-			rx++;
-		} else {
-			complete = 1;
-		}
+		if ((desc->ctl & (LTQ_DMA_OWN | LTQ_DMA_C)) != LTQ_DMA_C)
+			break;
+		ltq_etop_hw_receive(ch);
+		work_done++;
 	}
-	if (complete || !rx) {
-		napi_complete(&ch->napi);
+	if (work_done < budget) {
+		napi_complete_done(&ch->napi, work_done);
 		ltq_dma_ack_irq(&ch->dma);
 	}
-	return rx;
+	return work_done;
 }
 
 static int
--- a/drivers/net/ethernet/marvell/mv643xx_eth.c
+++ b/drivers/net/ethernet/marvell/mv643xx_eth.c
@@ -2312,7 +2312,7 @@ static int mv643xx_eth_poll(struct napi_
 	if (work_done < budget) {
 		if (mp->oom)
 			mod_timer(&mp->rx_oom, jiffies + (HZ / 10));
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		wrlp(mp, INT_MASK, mp->int_mask);
 	}
 
--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -2702,11 +2702,9 @@ static int mvneta_poll(struct napi_struc
 			rx_done = mvneta_rx_swbm(pp, budget, &pp->rxqs[rx_queue]);
 	}
 
-	budget -= rx_done;
-
-	if (budget > 0) {
+	if (rx_done < budget) {
 		cause_rx_tx = 0;
-		napi_complete(&port->napi);
+		napi_complete_done(&port->napi, rx_done);
 		enable_percpu_irq(pp->dev->irq, 0);
 	}
 
--- a/drivers/net/ethernet/marvell/mvpp2.c
+++ b/drivers/net/ethernet/marvell/mvpp2.c
@@ -5406,7 +5406,7 @@ static int mvpp2_poll(struct napi_struct
 
 	if (budget > 0) {
 		cause_rx = 0;
-		napi_complete(napi);
+		napi_complete_done(napi, rx_done);
 
 		mvpp2_interrupts_enable(port);
 	}
--- a/drivers/net/ethernet/marvell/pxa168_eth.c
+++ b/drivers/net/ethernet/marvell/pxa168_eth.c
@@ -1264,7 +1264,7 @@ static int pxa168_rx_poll(struct napi_st
 	}
 	work_done = rxq_process(dev, budget);
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		wrl(pep, INT_MASK, ALL_INTS);
 	}
 
--- a/drivers/net/ethernet/moxa/moxart_ether.c
+++ b/drivers/net/ethernet/moxa/moxart_ether.c
@@ -270,7 +270,7 @@ rx_next:
 	}
 
 	if (rx < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rx);
 	}
 
 	priv->reg_imr |= RPKT_FINISH_M;
--- a/drivers/net/ethernet/myricom/myri10ge/myri10ge.c
+++ b/drivers/net/ethernet/myricom/myri10ge/myri10ge.c
@@ -1678,7 +1678,7 @@ static int myri10ge_poll(struct napi_str
 
 	myri10ge_ss_unlock_napi(ss);
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		put_be32(htonl(3), ss->irq_claim);
 	}
 	return work_done;
--- a/drivers/net/ethernet/natsemi/natsemi.c
+++ b/drivers/net/ethernet/natsemi/natsemi.c
@@ -2261,7 +2261,7 @@ static int natsemi_poll(struct napi_stru
 		np->intr_status = readl(ioaddr + IntrStatus);
 	} while (np->intr_status);
 
-	napi_complete(napi);
+	napi_complete_done(napi, work_done);
 
 	/* Reenable interrupts providing nothing is trying to shut
 	 * the chip down. */
--- a/drivers/net/ethernet/neterion/s2io.c
+++ b/drivers/net/ethernet/neterion/s2io.c
@@ -2783,7 +2783,7 @@ static int s2io_poll_msix(struct napi_st
 	s2io_chk_rx_buffers(nic, ring);
 
 	if (pkts_processed < budget_org) {
-		napi_complete(napi);
+		napi_complete_done(napi, pkts_processed);
 		/*Re Enable MSI-Rx Vector*/
 		addr = (u8 __iomem *)&bar0->xmsi_mask_reg;
 		addr += 7 - ring->ring_no;
@@ -2817,7 +2817,7 @@ static int s2io_poll_inta(struct napi_st
 			break;
 	}
 	if (pkts_processed < budget_org) {
-		napi_complete(napi);
+		napi_complete_done(napi, pkts_processed);
 		/* Re enable the Rx interrupts for the ring */
 		writeq(0, &bar0->rx_traffic_mask);
 		readl(&bar0->rx_traffic_mask);
--- a/drivers/net/ethernet/neterion/vxge/vxge-main.c
+++ b/drivers/net/ethernet/neterion/vxge/vxge-main.c
@@ -1823,8 +1823,8 @@ static int vxge_poll_msix(struct napi_st
 	vxge_hw_vpath_poll_rx(ring->handle);
 	pkts_processed = ring->pkts_processed;
 
-	if (ring->pkts_processed < budget_org) {
-		napi_complete(napi);
+	if (pkts_processed < budget_org) {
+		napi_complete_done(napi, pkts_processed);
 
 		/* Re enable the Rx interrupts for the vpath */
 		vxge_hw_channel_msix_unmask(
@@ -1863,7 +1863,7 @@ static int vxge_poll_inta(struct napi_st
 	VXGE_COMPLETE_ALL_TX(vdev);
 
 	if (pkts_processed < budget_org) {
-		napi_complete(napi);
+		napi_complete_done(napi, pkts_processed);
 		/* Re enable the Rx interrupts for the ring */
 		vxge_hw_device_unmask_all(hldev);
 		vxge_hw_device_flush_io(hldev);
--- a/drivers/net/ethernet/nvidia/forcedeth.c
+++ b/drivers/net/ethernet/nvidia/forcedeth.c
@@ -3756,7 +3756,7 @@ static int nv_napi_poll(struct napi_stru
 	if (rx_work < budget) {
 		/* re-enable interrupts
 		   (msix not enabled in napi) */
-		napi_complete(napi);
+		napi_complete_done(napi, rx_work);
 
 		writel(np->irqmask, base + NvRegIrqMask);
 	}
--- a/drivers/net/ethernet/nxp/lpc_eth.c
+++ b/drivers/net/ethernet/nxp/lpc_eth.c
@@ -999,7 +999,7 @@ static int lpc_eth_poll(struct napi_stru
 	rx_done = __lpc_handle_recv(ndev, budget);
 
 	if (rx_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rx_done);
 		lpc_eth_enable_int(pldat->net_base);
 	}
 
--- a/drivers/net/ethernet/oki-semi/pch_gbe/pch_gbe_main.c
+++ b/drivers/net/ethernet/oki-semi/pch_gbe/pch_gbe_main.c
@@ -2391,7 +2391,7 @@ static int pch_gbe_napi_poll(struct napi
 		poll_end_flag = true;
 
 	if (poll_end_flag) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		pch_gbe_irq_enable(adapter);
 	}
 
--- a/drivers/net/ethernet/pasemi/pasemi_mac.c
+++ b/drivers/net/ethernet/pasemi/pasemi_mac.c
@@ -1575,7 +1575,7 @@ static int pasemi_mac_poll(struct napi_s
 	pkts = pasemi_mac_clean_rx(rx_ring(mac), budget);
 	if (pkts < budget) {
 		/* all done, no more packets present */
-		napi_complete(napi);
+		napi_complete_done(napi, pkts);
 
 		pasemi_mac_restart_rx_intr(mac);
 		pasemi_mac_restart_tx_intr(mac);
--- a/drivers/net/ethernet/qlogic/netxen/netxen_nic_main.c
+++ b/drivers/net/ethernet/qlogic/netxen/netxen_nic_main.c
@@ -2391,7 +2391,7 @@ static int netxen_nic_poll(struct napi_s
 		work_done = budget;
 
 	if (work_done < budget) {
-		napi_complete(&sds_ring->napi);
+		napi_complete_done(&sds_ring->napi, work_done);
 		if (test_bit(__NX_DEV_UP, &adapter->state))
 			netxen_nic_enable_int(sds_ring);
 	}
--- a/drivers/net/ethernet/qlogic/qlcnic/qlcnic_io.c
+++ b/drivers/net/ethernet/qlogic/qlcnic/qlcnic_io.c
@@ -975,7 +975,7 @@ static int qlcnic_poll(struct napi_struc
 		work_done = budget;
 
 	if (work_done < budget) {
-		napi_complete(&sds_ring->napi);
+		napi_complete_done(&sds_ring->napi, work_done);
 		if (test_bit(__QLCNIC_DEV_UP, &adapter->state)) {
 			qlcnic_enable_sds_intr(adapter, sds_ring);
 			qlcnic_enable_tx_intr(adapter, tx_ring);
@@ -1019,7 +1019,7 @@ static int qlcnic_rx_poll(struct napi_st
 	work_done = qlcnic_process_rcv_ring(sds_ring, budget);
 
 	if (work_done < budget) {
-		napi_complete(&sds_ring->napi);
+		napi_complete_done(&sds_ring->napi, work_done);
 		if (test_bit(__QLCNIC_DEV_UP, &adapter->state))
 			qlcnic_enable_sds_intr(adapter, sds_ring);
 	}
@@ -1966,7 +1966,7 @@ static int qlcnic_83xx_msix_sriov_vf_pol
 		work_done = budget;
 
 	if (work_done < budget) {
-		napi_complete(&sds_ring->napi);
+		napi_complete_done(&sds_ring->napi, work_done);
 		qlcnic_enable_sds_intr(adapter, sds_ring);
 	}
 
@@ -1994,7 +1994,7 @@ static int qlcnic_83xx_poll(struct napi_
 		work_done = budget;
 
 	if (work_done < budget) {
-		napi_complete(&sds_ring->napi);
+		napi_complete_done(&sds_ring->napi, work_done);
 		qlcnic_enable_sds_intr(adapter, sds_ring);
 	}
 
@@ -2032,7 +2032,7 @@ static int qlcnic_83xx_rx_poll(struct na
 	adapter = sds_ring->adapter;
 	work_done = qlcnic_83xx_process_rcv_ring(sds_ring, budget);
 	if (work_done < budget) {
-		napi_complete(&sds_ring->napi);
+		napi_complete_done(&sds_ring->napi, work_done);
 		if (test_bit(__QLCNIC_DEV_UP, &adapter->state))
 			qlcnic_enable_sds_intr(adapter, sds_ring);
 	}
--- a/drivers/net/ethernet/qlogic/qlge/qlge_main.c
+++ b/drivers/net/ethernet/qlogic/qlge/qlge_main.c
@@ -2334,7 +2334,7 @@ static int ql_napi_poll_msix(struct napi
 	}
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		ql_enable_completion_interrupt(qdev, rx_ring->irq);
 	}
 	return work_done;
--- a/drivers/net/ethernet/qualcomm/emac/emac.c
+++ b/drivers/net/ethernet/qualcomm/emac/emac.c
@@ -129,7 +129,7 @@ static int emac_napi_rtx(struct napi_str
 	emac_mac_rx_process(adpt, rx_q, &work_done, budget);
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		irq->mask |= rx_q->intr;
 		writel(irq->mask, adpt->base + EMAC_INT_MASK);
--- a/drivers/net/ethernet/realtek/r8169.c
+++ b/drivers/net/ethernet/realtek/r8169.c
@@ -7576,7 +7576,7 @@ static int rtl8169_poll(struct napi_stru
 	}
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		rtl_irq_enable(tp, enable_mask);
 		mmiowb();
--- a/drivers/net/ethernet/rocker/rocker_main.c
+++ b/drivers/net/ethernet/rocker/rocker_main.c
@@ -2480,7 +2480,7 @@ static int rocker_port_poll_rx(struct na
 	}
 
 	if (credits < budget)
-		napi_complete(napi);
+		napi_complete_done(napi, credits);
 
 	rocker_dma_ring_credits_set(rocker, &rocker_port->rx_ring, credits);
 
--- a/drivers/net/ethernet/samsung/sxgbe/sxgbe_main.c
+++ b/drivers/net/ethernet/samsung/sxgbe/sxgbe_main.c
@@ -1578,7 +1578,7 @@ static int sxgbe_poll(struct napi_struct
 
 	work_done = sxgbe_rx(priv, budget);
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		priv->hw->dma->enable_dma_irq(priv->ioaddr, qnum);
 	}
 
--- a/drivers/net/ethernet/sfc/efx.c
+++ b/drivers/net/ethernet/sfc/efx.c
@@ -332,7 +332,7 @@ static int efx_poll(struct napi_struct *
 		 * since efx_nic_eventq_read_ack() will have no effect if
 		 * interrupts have already been disabled.
 		 */
-		napi_complete(napi);
+		napi_complete_done(napi, spent);
 		efx_nic_eventq_read_ack(channel);
 	}
 
--- a/drivers/net/ethernet/smsc/smsc9420.c
+++ b/drivers/net/ethernet/smsc/smsc9420.c
@@ -869,7 +869,7 @@ static int smsc9420_rx_poll(struct napi_
 	smsc9420_pci_flush_write(pd);
 
 	if (work_done < budget) {
-		napi_complete(&pd->napi);
+		napi_complete_done(&pd->napi, work_done);
 
 		/* re-enable RX DMA interrupts */
 		dma_intr_ena = smsc9420_reg_read(pd, DMAC_INTR_ENA);
--- a/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
+++ b/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
@@ -2706,7 +2706,7 @@ static int stmmac_poll(struct napi_struc
 
 	work_done = stmmac_rx(priv, budget);
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		stmmac_enable_dma_irq(priv);
 	}
 	return work_done;
--- a/drivers/net/ethernet/sun/niu.c
+++ b/drivers/net/ethernet/sun/niu.c
@@ -3785,7 +3785,7 @@ static int niu_poll(struct napi_struct *
 	work_done = niu_poll_core(np, lp, budget);
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		niu_ldg_rearm(np, lp, 1);
 	}
 	return work_done;
--- a/drivers/net/ethernet/sun/sungem.c
+++ b/drivers/net/ethernet/sun/sungem.c
@@ -924,7 +924,7 @@ static int gem_poll(struct napi_struct *
 		gp->status = readl(gp->regs + GREG_STAT);
 	} while (gp->status & GREG_STAT_NAPI);
 
-	napi_complete(napi);
+	napi_complete_done(napi, work_done);
 	gem_enable_ints(gp);
 
 	return work_done;
--- a/drivers/net/ethernet/sun/sunvnet_common.c
+++ b/drivers/net/ethernet/sun/sunvnet_common.c
@@ -850,7 +850,7 @@ int sunvnet_poll_common(struct napi_stru
 	int processed = vnet_event_napi(port, budget);
 
 	if (processed < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, processed);
 		port->rx_event &= ~LDC_EVENT_DATA_READY;
 		vio_set_intr(vio->vdev->rx_ino, HV_INTR_ENABLED);
 	}
--- a/drivers/net/ethernet/tehuti/tehuti.c
+++ b/drivers/net/ethernet/tehuti/tehuti.c
@@ -303,7 +303,7 @@ static int bdx_poll(struct napi_struct *
 		 * device lock and allow waiting tasks (eg rmmod) to advance) */
 		priv->napi_stop = 0;
 
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		bdx_enable_interrupts(priv);
 	}
 	return work_done;
--- a/drivers/net/ethernet/ti/cpsw.c
+++ b/drivers/net/ethernet/ti/cpsw.c
@@ -843,7 +843,7 @@ static int cpsw_rx_poll(struct napi_stru
 	}
 
 	if (num_rx < budget) {
-		napi_complete(napi_rx);
+		napi_complete_done(napi_rx, num_rx);
 		writel(0xff, &cpsw->wr_regs->rx_en);
 		if (cpsw->quirk_irq && cpsw->rx_irq_disabled) {
 			cpsw->rx_irq_disabled = false;
--- a/drivers/net/ethernet/ti/davinci_emac.c
+++ b/drivers/net/ethernet/ti/davinci_emac.c
@@ -1295,7 +1295,7 @@ static int emac_poll(struct napi_struct
 					&emac_rxhost_errcodes[cause][0], ch);
 		}
 	} else if (num_rx_pkts < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, num_rx_pkts);
 		emac_int_enable(priv);
 	}
 
--- a/drivers/net/ethernet/ti/netcp_core.c
+++ b/drivers/net/ethernet/ti/netcp_core.c
@@ -939,7 +939,7 @@ static int netcp_rx_poll(struct napi_str
 
 	netcp_rxpool_refill(netcp);
 	if (packets < budget) {
-		napi_complete(&netcp->rx_napi);
+		napi_complete_done(&netcp->rx_napi, packets);
 		knav_queue_enable_notify(netcp->rx_queue);
 	}
 
--- a/drivers/net/ethernet/tile/tilegx.c
+++ b/drivers/net/ethernet/tile/tilegx.c
@@ -678,7 +678,7 @@ static int tile_net_poll(struct napi_str
 	}
 
 	/* There are no packets left. */
-	napi_complete(&info_mpipe->napi);
+	napi_complete_done(&info_mpipe->napi, work);
 
 	md = &mpipe_data[instance];
 	/* Re-enable hypervisor interrupts. */
--- a/drivers/net/ethernet/tile/tilepro.c
+++ b/drivers/net/ethernet/tile/tilepro.c
@@ -842,7 +842,7 @@ static int tile_net_poll(struct napi_str
 		}
 	}
 
-	napi_complete(&info->napi);
+	napi_complete_done(&info->napi, work);
 
 	if (!priv->active)
 		goto done;
--- a/drivers/net/ethernet/toshiba/ps3_gelic_net.c
+++ b/drivers/net/ethernet/toshiba/ps3_gelic_net.c
@@ -1109,7 +1109,7 @@ static int gelic_net_poll(struct napi_st
 	}
 
 	if (packets_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, packets_done);
 		gelic_card_rx_irq_on(card);
 	}
 	return packets_done;
--- a/drivers/net/ethernet/toshiba/spider_net.c
+++ b/drivers/net/ethernet/toshiba/spider_net.c
@@ -1270,7 +1270,7 @@ static int spider_net_poll(struct napi_s
 	/* if all packets are in the stack, enable interrupts and return 0 */
 	/* if not, return 1 */
 	if (packets_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, packets_done);
 		spider_net_rx_irq_on(card);
 		card->ignore_rx_ramfull = 0;
 	}
--- a/drivers/net/ethernet/toshiba/tc35815.c
+++ b/drivers/net/ethernet/toshiba/tc35815.c
@@ -1639,7 +1639,7 @@ static int tc35815_poll(struct napi_stru
 	spin_unlock(&lp->rx_lock);
 
 	if (received < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, received);
 		/* enable interrupts */
 		tc_writel(tc_readl(&tr->DMA_Ctl) & ~DMA_IntMask, &tr->DMA_Ctl);
 	}
--- a/drivers/net/ethernet/tundra/tsi108_eth.c
+++ b/drivers/net/ethernet/tundra/tsi108_eth.c
@@ -887,7 +887,7 @@ static int tsi108_poll(struct napi_struc
 
 	if (num_received < budget) {
 		data->rxpending = 0;
-		napi_complete(napi);
+		napi_complete_done(napi, num_received);
 
 		TSI_WRITE(TSI108_EC_INTMASK,
 				     TSI_READ(TSI108_EC_INTMASK)
--- a/drivers/net/ethernet/via/via-rhine.c
+++ b/drivers/net/ethernet/via/via-rhine.c
@@ -861,7 +861,7 @@ static int rhine_napipoll(struct napi_st
 	}
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		iowrite16(enable_mask, ioaddr + IntrEnable);
 		mmiowb();
 	}
--- a/drivers/net/ethernet/via/via-velocity.c
+++ b/drivers/net/ethernet/via/via-velocity.c
@@ -2160,7 +2160,7 @@ static int velocity_poll(struct napi_str
 	velocity_tx_srv(vptr);
 	/* If budget not fully consumed, exit the polling mode */
 	if (rx_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rx_done);
 		mac_enable_int(vptr->mac_regs);
 	}
 	spin_unlock_irqrestore(&vptr->lock, flags);
--- a/drivers/net/ethernet/wiznet/w5100.c
+++ b/drivers/net/ethernet/wiznet/w5100.c
@@ -915,7 +915,7 @@ static int w5100_napi_poll(struct napi_s
 	}
 
 	if (rx_count < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rx_count);
 		w5100_enable_intr(priv);
 	}
 
--- a/drivers/net/ethernet/wiznet/w5300.c
+++ b/drivers/net/ethernet/wiznet/w5300.c
@@ -417,7 +417,7 @@ static int w5300_napi_poll(struct napi_s
 	}
 
 	if (rx_count < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rx_count);
 		w5300_write(priv, W5300_IMR, IR_S0);
 		mmiowb();
 	}
--- a/drivers/net/fjes/fjes_main.c
+++ b/drivers/net/fjes/fjes_main.c
@@ -1122,7 +1122,7 @@ static int fjes_poll(struct napi_struct
 	}
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		if (adapter->unset_rx_last) {
 			adapter->rx_last_jiffies = jiffies;
--- a/drivers/net/vmxnet3/vmxnet3_drv.c
+++ b/drivers/net/vmxnet3/vmxnet3_drv.c
@@ -1873,7 +1873,7 @@ vmxnet3_poll(struct napi_struct *napi, i
 	rxd_done = vmxnet3_do_poll(rx_queue->adapter, budget);
 
 	if (rxd_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rxd_done);
 		vmxnet3_enable_all_intrs(rx_queue->adapter);
 	}
 	return rxd_done;
@@ -1904,7 +1904,7 @@ vmxnet3_poll_rx_only(struct napi_struct
 	rxd_done = vmxnet3_rq_rx_complete(rq, adapter, budget);
 
 	if (rxd_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, rxd_done);
 		vmxnet3_enable_intr(adapter, rq->comp_ring.intr_idx);
 	}
 	return rxd_done;
--- a/drivers/net/wan/fsl_ucc_hdlc.c
+++ b/drivers/net/wan/fsl_ucc_hdlc.c
@@ -573,7 +573,7 @@ static int ucc_hdlc_poll(struct napi_str
 	howmany += hdlc_rx_done(priv, budget - howmany);
 
 	if (howmany < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, howmany);
 		qe_setbits32(priv->uccf->p_uccm,
 			     (UCCE_HDLC_RX_EVENTS | UCCE_HDLC_TX_EVENTS) << 16);
 	}
--- a/drivers/net/wan/hd64572.c
+++ b/drivers/net/wan/hd64572.c
@@ -341,7 +341,7 @@ static int sca_poll(struct napi_struct *
 		received = sca_rx_done(port, budget);
 
 	if (received < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, received);
 		enable_intr(port);
 	}
 
--- a/drivers/net/wireless/ath/ath10k/pci.c
+++ b/drivers/net/wireless/ath/ath10k/pci.c
@@ -2804,7 +2804,7 @@ static int ath10k_pci_napi_poll(struct n
 	done = ath10k_htt_txrx_compl_task(ar, budget);
 
 	if (done < budget) {
-		napi_complete(ctx);
+		napi_complete_done(ctx, done);
 		/* In case of MSI, it is possible that interrupts are received
 		 * while NAPI poll is inprogress. So pending interrupts that are
 		 * received after processing all copy engine pipes by NAPI poll
--- a/drivers/net/wireless/ath/wil6210/netdev.c
+++ b/drivers/net/wireless/ath/wil6210/netdev.c
@@ -84,7 +84,7 @@ static int wil6210_netdev_poll_rx(struct
 	done = budget - quota;
 
 	if (done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, done);
 		wil6210_unmask_irq_rx(wil);
 		wil_dbg_txrx(wil, "NAPI RX complete\n");
 	}
--- a/drivers/net/xen-netback/interface.c
+++ b/drivers/net/xen-netback/interface.c
@@ -104,7 +104,7 @@ static int xenvif_poll(struct napi_struc
 	work_done = xenvif_tx_action(queue, budget);
 
 	if (work_done < budget) {
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 		/* If the queue is rate-limited, it shall be
 		 * rescheduled in the timer callback.
 		 */
--- a/drivers/net/xen-netfront.c
+++ b/drivers/net/xen-netfront.c
@@ -1070,7 +1070,7 @@ err:
 	if (work_done < budget) {
 		int more_to_do = 0;
 
-		napi_complete(napi);
+		napi_complete_done(napi, work_done);
 
 		RING_FINAL_CHECK_FOR_RESPONSES(&queue->rx, more_to_do);
 		if (more_to_do)
--- a/drivers/staging/octeon/ethernet-rx.c
+++ b/drivers/staging/octeon/ethernet-rx.c
@@ -429,7 +429,7 @@ static int cvm_oct_napi_poll(struct napi
 
 	if (rx_count < budget) {
 		/* No more work */
-		napi_complete(napi);
+		napi_complete_done(napi, rx_count);
 		enable_irq(rx_group->irq);
 	}
 	return rx_count;
--- a/drivers/staging/unisys/visornic/visornic_main.c
+++ b/drivers/staging/unisys/visornic/visornic_main.c
@@ -1657,7 +1657,7 @@ static int visornic_poll(struct napi_str
 
 	/* If there aren't any more packets to receive stop the poll */
 	if (rx_count < budget)
-		napi_complete(napi);
+		napi_complete_done(napi, rx_count);
 
 	return rx_count;
 }
