From d30840e2b1cf79d90392e6051b0c0b6006d29d8b Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 9 Mar 2017 09:32:40 +0100
Subject: [PATCH 64/69] clk: clk-rpm fixes

Signed-off-by: John Crispin <john@phrozen.org>
---
 .../devicetree/bindings/clock/qcom,rpmcc.txt       |  1 +
 drivers/clk/qcom/clk-rpm.c                         | 35 ++++++++++++++++++++++
 include/dt-bindings/clock/qcom,rpmcc.h             |  4 +++
 3 files changed, 40 insertions(+)

--- a/Documentation/devicetree/bindings/clock/qcom,rpmcc.txt
+++ b/Documentation/devicetree/bindings/clock/qcom,rpmcc.txt
@@ -13,6 +13,7 @@ Required properties :
 			"qcom,rpmcc-msm8916", "qcom,rpmcc"
 			"qcom,rpmcc-msm8974", "qcom,rpmcc"
 			"qcom,rpmcc-apq8064", "qcom,rpmcc"
+			"qcom,rpmcc-ipq806x", "qcom,rpmcc"
 
 - #clock-cells : shall contain 1
 
--- a/drivers/clk/qcom/clk-rpm.c
+++ b/drivers/clk/qcom/clk-rpm.c
@@ -359,6 +359,16 @@ DEFINE_CLK_RPM(apq8064, sfab_clk, sfab_a
 DEFINE_CLK_RPM(apq8064, sfpb_clk, sfpb_a_clk, QCOM_RPM_SFPB_CLK);
 DEFINE_CLK_RPM(apq8064, qdss_clk, qdss_a_clk, QCOM_RPM_QDSS_CLK);
 
+/* ipq806x */
+DEFINE_CLK_RPM(ipq806x, afab_clk, afab_a_clk, QCOM_RPM_APPS_FABRIC_CLK);
+DEFINE_CLK_RPM(ipq806x, cfpb_clk, cfpb_a_clk, QCOM_RPM_CFPB_CLK);
+DEFINE_CLK_RPM(ipq806x, daytona_clk, daytona_a_clk, QCOM_RPM_DAYTONA_FABRIC_CLK);
+DEFINE_CLK_RPM(ipq806x, ebi1_clk, ebi1_a_clk, QCOM_RPM_EBI1_CLK);
+DEFINE_CLK_RPM(ipq806x, sfab_clk, sfab_a_clk, QCOM_RPM_SYS_FABRIC_CLK);
+DEFINE_CLK_RPM(ipq806x, sfpb_clk, sfpb_a_clk, QCOM_RPM_SFPB_CLK);
+DEFINE_CLK_RPM(ipq806x, nss_fabric_0_clk, nss_fabric_0_a_clk, QCOM_RPM_NSS_FABRIC_0_CLK);
+DEFINE_CLK_RPM(ipq806x, nss_fabric_1_clk, nss_fabric_1_a_clk, QCOM_RPM_NSS_FABRIC_1_CLK);
+
 static struct clk_rpm *apq8064_clks[] = {
 	[RPM_APPS_FABRIC_CLK] = &apq8064_afab_clk,
 	[RPM_APPS_FABRIC_A_CLK] = &apq8064_afab_a_clk,
@@ -380,13 +390,38 @@ static struct clk_rpm *apq8064_clks[] =
 	[RPM_QDSS_A_CLK] = &apq8064_qdss_a_clk,
 };
 
+static struct clk_rpm *ipq806x_clks[] = {
+	[RPM_APPS_FABRIC_CLK] = &ipq806x_afab_clk,
+	[RPM_APPS_FABRIC_A_CLK] = &ipq806x_afab_a_clk,
+	[RPM_CFPB_CLK] = &ipq806x_cfpb_clk,
+	[RPM_CFPB_A_CLK] = &ipq806x_cfpb_a_clk,
+	[RPM_DAYTONA_FABRIC_CLK] = &ipq806x_daytona_clk,
+	[RPM_DAYTONA_FABRIC_A_CLK] = &ipq806x_daytona_a_clk,
+	[RPM_EBI1_CLK] = &ipq806x_ebi1_clk,
+	[RPM_EBI1_A_CLK] = &ipq806x_ebi1_a_clk,
+	[RPM_SYS_FABRIC_CLK] = &ipq806x_sfab_clk,
+	[RPM_SYS_FABRIC_A_CLK] = &ipq806x_sfab_a_clk,
+	[RPM_SFPB_CLK] = &ipq806x_sfpb_clk,
+	[RPM_SFPB_A_CLK] = &ipq806x_sfpb_a_clk,
+	[RPM_NSS_FABRIC_0_CLK] = &ipq806x_nss_fabric_0_clk,
+	[RPM_NSS_FABRIC_0_A_CLK] = &ipq806x_nss_fabric_0_a_clk,
+	[RPM_NSS_FABRIC_1_CLK] = &ipq806x_nss_fabric_1_clk,
+	[RPM_NSS_FABRIC_1_A_CLK] = &ipq806x_nss_fabric_1_a_clk,
+};
+
 static const struct rpm_clk_desc rpm_clk_apq8064 = {
 	.clks = apq8064_clks,
 	.num_clks = ARRAY_SIZE(apq8064_clks),
 };
 
+static const struct rpm_clk_desc rpm_clk_ipq806x = {
+	.clks = ipq806x_clks,
+	.num_clks = ARRAY_SIZE(ipq806x_clks),
+};
+
 static const struct of_device_id rpm_clk_match_table[] = {
 	{ .compatible = "qcom,rpmcc-apq8064", .data = &rpm_clk_apq8064 },
+	{ .compatible = "qcom,rpmcc-ipq806x", .data = &rpm_clk_ipq806x },
 	{ }
 };
 MODULE_DEVICE_TABLE(of, rpm_clk_match_table);
--- a/include/dt-bindings/clock/qcom,rpmcc.h
+++ b/include/dt-bindings/clock/qcom,rpmcc.h
@@ -37,6 +37,10 @@
 #define RPM_SYS_FABRIC_A_CLK			19
 #define RPM_SFPB_CLK				20
 #define RPM_SFPB_A_CLK				21
+#define RPM_NSS_FABRIC_0_CLK				22
+#define RPM_NSS_FABRIC_0_A_CLK				23
+#define RPM_NSS_FABRIC_1_CLK				24
+#define RPM_NSS_FABRIC_1_A_CLK				25
 
 /* SMD RPM clocks */
 #define RPM_SMD_XO_CLK_SRC				0
