#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "ubiquiti,edgerouterx", "mediatek,mt7621-soc";

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x10000000>;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x22>;
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@80000 {
			label = "u-boot-env";
			reg = <0x80000 0x60000>;
			read-only;
		};

		factory: partition@e0000 {
			label = "factory";
			reg = <0xe0000 0x60000>;
		};

		partition@140000 {
			label = "kernel1";
			reg = <0x140000 0x300000>;
		};

		partition@440000 {
			label = "kernel2";
			reg = <0x440000 0x300000>;
		};

		partition@740000 {
			label = "ubi";
			reg = <0x740000 0xf7c0000>;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "uart2", "uart3", "i2c", "pcie", "rgmii2", "jtag";
			ralink,function = "gpio";
		};
	};
};

&spi0 {
	/*
	 * This board has 2Mb spi flash soldered in and visible
	 * from manufacturer's firmware.
	 * But this SoC shares spi and nand pins,
	 * and current driver doesn't handle this sharing well
	 */
	status = "disabled";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <1>;
		spi-max-frequency = <10000000>;
		m25p,chunked-io = <32>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "spi";
				reg = <0x0 0x200000>;
				read-only;
			};
		};
	};
};

&xhci {
	status = "disabled";
};
