From 25adaf94e0fcbf6c1b47cb610edb7f5c23c53139 Mon Sep 17 00:00:00 2001
From: Chunfeng Yun <chunfeng.yun@mediatek.com>
Date: Fri, 13 Oct 2017 16:26:37 +0800
Subject: [PATCH 130/224] usb: xhci-mtk: remove dummy wakeup debounce clocks

The wakeup debounce clocks for each ports in fact are not
needed, so remove them.

Signed-off-by: Chunfeng Yun <chunfeng.yun@mediatek.com>
Acked-by: Mathias Nyman <mathias.nyman@linux.intel.com>
Reviewed-by: Matthias Brugger <matthias.bgg@gmail.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/xhci-mtk.c | 33 ---------------------------------
 drivers/usb/host/xhci-mtk.h |  2 --
 2 files changed, 35 deletions(-)

--- a/drivers/usb/host/xhci-mtk.c
+++ b/drivers/usb/host/xhci-mtk.c
@@ -237,25 +237,8 @@ static int xhci_mtk_clks_enable(struct x
 		goto sys_clk_err;
 	}
 
-	if (mtk->wakeup_src) {
-		ret = clk_prepare_enable(mtk->wk_deb_p0);
-		if (ret) {
-			dev_err(mtk->dev, "failed to enable wk_deb_p0\n");
-			goto usb_p0_err;
-		}
-
-		ret = clk_prepare_enable(mtk->wk_deb_p1);
-		if (ret) {
-			dev_err(mtk->dev, "failed to enable wk_deb_p1\n");
-			goto usb_p1_err;
-		}
-	}
 	return 0;
 
-usb_p1_err:
-	clk_disable_unprepare(mtk->wk_deb_p0);
-usb_p0_err:
-	clk_disable_unprepare(mtk->sys_clk);
 sys_clk_err:
 	clk_disable_unprepare(mtk->ref_clk);
 ref_clk_err:
@@ -264,10 +247,6 @@ ref_clk_err:
 
 static void xhci_mtk_clks_disable(struct xhci_hcd_mtk *mtk)
 {
-	if (mtk->wakeup_src) {
-		clk_disable_unprepare(mtk->wk_deb_p1);
-		clk_disable_unprepare(mtk->wk_deb_p0);
-	}
 	clk_disable_unprepare(mtk->sys_clk);
 	clk_disable_unprepare(mtk->ref_clk);
 }
@@ -371,18 +350,6 @@ static int usb_wakeup_of_property_parse(
 	if (!mtk->wakeup_src)
 		return 0;
 
-	mtk->wk_deb_p0 = devm_clk_get(dev, "wakeup_deb_p0");
-	if (IS_ERR(mtk->wk_deb_p0)) {
-		dev_err(dev, "fail to get wakeup_deb_p0\n");
-		return PTR_ERR(mtk->wk_deb_p0);
-	}
-
-	mtk->wk_deb_p1 = devm_clk_get(dev, "wakeup_deb_p1");
-	if (IS_ERR(mtk->wk_deb_p1)) {
-		dev_err(dev, "fail to get wakeup_deb_p1\n");
-		return PTR_ERR(mtk->wk_deb_p1);
-	}
-
 	mtk->pericfg = syscon_regmap_lookup_by_phandle(dn,
 						"mediatek,syscon-wakeup");
 	if (IS_ERR(mtk->pericfg)) {
--- a/drivers/usb/host/xhci-mtk.h
+++ b/drivers/usb/host/xhci-mtk.h
@@ -126,8 +126,6 @@ struct xhci_hcd_mtk {
 	struct regulator *vbus;
 	struct clk *sys_clk;	/* sys and mac clock */
 	struct clk *ref_clk;
-	struct clk *wk_deb_p0;	/* port0's wakeup debounce clock */
-	struct clk *wk_deb_p1;
 	struct regmap *pericfg;
 	struct phy **phys;
 	int num_phys;
