/dts-v1/;

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "dlink,dir-810l", "ralink,mt7620a-soc";
	model = "D-Link DIR-810L";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		led_power_green: power {
			label = "dir-810l:green:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_HIGH>;
		};

		wan {
			label = "dir-810l:orange:wan";
			gpios = <&gpio0 12 GPIO_ACTIVE_HIGH>;
		};

		power2 {
			label = "dir-810l:orange:power";
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			factory5g: partition@50000 {
				label = "factory5g";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "Wolf_Config";
				reg = <0x60000 0x10000>;
				read-only;
			};

			partition@70000 {
				label = "MyDlink";
				reg = <0x70000 0x80000>;
				read-only;
			};

			partition@e0000 {
				label = "Jffs2";
				reg = <0xe0000 0x80000>;
				read-only;
			};

			partition@170000 {
				label = "firmware";
				reg = <0x170000 0x690000>;
			};
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "mdio", "rgmii1", "i2c", "wled", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
	mediatek,portmap = "llllw";
};

&gsw {
	mediatek,port4 = "ephy";
	pinctrl-names = "default";
	pinctrl-0 = <&ephy_pins>;
};

&pcie {
	status = "okay";
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};
