// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "ar7242.dtsi"

/ {
	compatible = "tplink,tl-wr2543-v1", "qca,ar7242";
	model = "TP-LINK TL-WR2543N/ND";

	aliases {
		led-boot = &system;
		led-failsafe = &system;
		led-running = &system;
		led-upgrade = &system;
	};

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <40000000>;
	};

	gpio-keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		system: wps {
			label = "tplink:green:wps";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			default-state = "off";
		};

		usb {
			label = "tplink:green:usb";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			default-state = "off";
			trigger-sources = <&hub_port>;
			linux,default-trigger = "usbport";
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan2g {
			label = "tplink:green:wlan2g";
			gpios = <&ath9k 0 GPIO_ACTIVE_LOW>;
			default-state = "off";
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "tplink:green:wlan5g";
			gpios = <&ath9k 1 GPIO_ACTIVE_LOW>;
			default-state = "off";
			linux,default-trigger = "phy0tpt";
		};
	};

	rtl8367 {
		compatible = "realtek,rtl8367";
		gpio-sda = <&gpio 1 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio 6 GPIO_ACTIVE_HIGH>;
		realtek,extif0 = <1 0 1 1 1 1 1 1 2>;

		mdio-bus {
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			phy0: ethernet-phy@0 {
				reg = <0>;
			};
		};
	};
};

&pll {
	clocks = <&extosc>;
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot:	partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x020000 0x7d0000>;
			};

			partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&uart {
	status = "okay";
};

&usb {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb_phy {
	status = "okay";
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		#gpio-cells = <2>;
		gpio-controller;
		qca,no-eeprom;
		mtd-mac-address = <&uboot 0x1fc00>;
	};
};

&eth0 {
	status = "okay";

	phy-mode = "rgmii";
	mtd-mac-address = <&uboot 0x1fc00>;

	phy-handle = <&phy0>;
	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};
