From 00e53d08bbe92051765c5bb94223b6f628cd3740 Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Wed, 11 Oct 2017 19:45:19 +0200
Subject: [PATCH 03/31] ARM: dts: Add TVE200 to the Gemini SoC DTSI

The Faraday TVE200 is present in the Gemini SoC, sometimes
under the name "TVC". Add it to the SoC DTSI file along with
its resources.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Signed-off-by: Arnd Bergmann <arnd@arndb.de>
---
 arch/arm/boot/dts/gemini.dtsi | 21 +++++++++++++++++++++
 1 file changed, 21 insertions(+)

--- a/arch/arm/boot/dts/gemini.dtsi
+++ b/arch/arm/boot/dts/gemini.dtsi
@@ -142,6 +142,12 @@
 						groups = "idegrp";
 					};
 				};
+				tvc_default_pins: pinctrl-tvc {
+					mux {
+						function = "tvc";
+						groups = "tvcgrp";
+					};
+				};
 			};
 		};
 
@@ -348,5 +354,20 @@
 			memcpy-bus-width = <32>;
 			#dma-cells = <2>;
 		};
+
+		display-controller@6a000000 {
+			compatible = "cortina,gemini-tvc", "faraday,tve200";
+			reg = <0x6a000000 0x1000>;
+			interrupts = <13 IRQ_TYPE_EDGE_RISING>;
+			resets = <&syscon GEMINI_RESET_TVC>;
+			clocks = <&syscon GEMINI_CLK_GATE_TVC>,
+				 <&syscon GEMINI_CLK_TVC>;
+			clock-names = "PCLK", "TVE";
+			pinctrl-names = "default";
+			pinctrl-0 = <&tvc_default_pins>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
 	};
 };
