From 8630b0b3fea31138c52ef83848ae1a047baa3855 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 23 Jan 2017 17:36:50 +0000
Subject: [PATCH] BCM270X_DT: Add reference to audio_pins to CM dtb

The CM1 dtb contains an empty audio_pins node, but no reference to it.
Adding the usual pinctrl reference from the audio node enables the
audremap overlay (and others) to easily turn on audio.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2708-rpi-cm.dts | 5 +++++
 1 file changed, 5 insertions(+)

--- a/arch/arm/boot/dts/bcm2708-rpi-cm.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dts
@@ -85,6 +85,11 @@
 	pinctrl-0 = <&i2s_pins>;
 };
 
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
 &hdmi {
 	hpd-gpios = <&gpio 46 GPIO_ACTIVE_HIGH>;
 };
