From 0c974b87829e007dc4fae94e20d488204e20e662 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 9 Mar 2017 08:16:10 +0100
Subject: [PATCH 30/69] clk: Disable i2c device on gsbi4

This patch was not annotated and comes from the v4.4 tree.

Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/clk/qcom/gcc-ipq806x.c | 5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

--- a/drivers/clk/qcom/gcc-ipq806x.c
+++ b/drivers/clk/qcom/gcc-ipq806x.c
@@ -294,7 +294,7 @@ static struct clk_rcg gsbi1_uart_src = {
 			.parent_names = gcc_pxo_pll8,
 			.num_parents = 2,
 			.ops = &clk_rcg_ops,
-			.flags = CLK_SET_PARENT_GATE,
+			.flags = CLK_SET_PARENT_GATE | CLK_IGNORE_UNUSED,
 		},
 	},
 };
@@ -312,7 +312,7 @@ static struct clk_branch gsbi1_uart_clk
 			},
 			.num_parents = 1,
 			.ops = &clk_branch_ops,
-			.flags = CLK_SET_RATE_PARENT,
+			.flags = CLK_SET_RATE_PARENT | CLK_IGNORE_UNUSED,
 		},
 	},
 };
@@ -890,6 +890,7 @@ static struct clk_branch gsbi1_h_clk = {
 		.hw.init = &(struct clk_init_data){
 			.name = "gsbi1_h_clk",
 			.ops = &clk_branch_ops,
+			.flags = CLK_IGNORE_UNUSED,
 		},
 	},
 };
