From c7af0732a25e5643979d55d304182309cff70ed9 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Mon, 1 Feb 2016 12:44:34 +0100
Subject: [PATCH] mtd: brcmnand: stop special treating ECC strength 1 (as
 Hamming)
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 drivers/mtd/nand/brcmnand/brcmnand.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/mtd/nand/brcmnand/brcmnand.c
+++ b/drivers/mtd/nand/brcmnand/brcmnand.c
@@ -1886,7 +1886,8 @@ static int brcmnand_setup_dev(struct brc
 
 	switch (chip->ecc.size) {
 	case 512:
-		if (chip->ecc.strength == 1) /* Hamming */
+		/* FIXME: We need to use strength 1 on DIR-885L */
+		if (0 && chip->ecc.strength == 1) /* Hamming */
 			cfg->ecc_level = 15;
 		else
 			cfg->ecc_level = chip->ecc.strength;
