From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Subject: [PATCH] Use "brcm,bcm947xx-cfe-partitions" binding for Broadcom
 partitions

---

--- a/arch/arm/boot/dts/bcm5301x-nand-cs0.dtsi
+++ b/arch/arm/boot/dts/bcm5301x-nand-cs0.dtsi
@@ -13,6 +13,10 @@
 			reg = <0>;
 			#address-cells = <1>;
 			#size-cells = <1>;
+
+			partitions {
+				compatible = "brcm,bcm947xx-cfe-partitions";
+			};
 		};
 	};
 };
--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -346,8 +346,11 @@
 				compatible = "jedec,spi-nor";
 				reg = <0>;
 				spi-max-frequency = <20000000>;
-				linux,part-probe = "ofpart", "bcm47xxpart";
 				status = "disabled";
+
+				partitions {
+					compatible = "brcm,bcm947xx-cfe-partitions";
+				};
 			};
 		};
 
--- a/drivers/mtd/bcm47xxpart.c
+++ b/drivers/mtd/bcm47xxpart.c
@@ -300,9 +300,16 @@ static int bcm47xxpart_parse(struct mtd_
 	return curr_part;
 };
 
+static const struct of_device_id bcm47xxpart_of_match_table[] = {
+	{ .compatible = "brcm,bcm947xx-cfe-partitions" },
+	{},
+};
+MODULE_DEVICE_TABLE(of, bcm47xxpart_of_match_table);
+
 static struct mtd_part_parser bcm47xxpart_mtd_parser = {
 	.parse_fn = bcm47xxpart_parse,
 	.name = "bcm47xxpart",
+	.of_match_table = bcm47xxpart_of_match_table,
 };
 module_mtd_part_parser(bcm47xxpart_mtd_parser);
 
