From b4ac5820bdc98ee24a2f73b8bd7fdf7f82db3a46 Mon Sep 17 00:00:00 2001
From: Marko Ratkaj <marko.ratkaj@sartura.hr>
Date: Fri, 7 Apr 2017 11:02:30 +0200
Subject: [PATCH 2/2] add ClearFog Base device tree files

Signed-off-by: Marko Ratkaj <marko.ratkaj@sartura.hr>
---
 arch/arm/boot/dts/Makefile                         |   1 +
 arch/arm/boot/dts/armada-388-clearfog-base.dts     | 161 ++++++++++++
 arch/arm/boot/dts/armada-388-clearfog.dtsi         | 282 +++++++++++++++++++++
 .../dts/armada-38x-solidrun-microsom-emmc.dtsi     |  62 +++++
 4 files changed, 506 insertions(+)
 create mode 100644 arch/arm/boot/dts/armada-388-clearfog-base.dts
 create mode 100644 arch/arm/boot/dts/armada-388-clearfog.dtsi
 create mode 100644 arch/arm/boot/dts/armada-38x-solidrun-microsom-emmc.dtsi

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -925,6 +925,7 @@ dtb-$(CONFIG_MACH_ARMADA_38X) += \
 	armada-385-linksys-shelby.dtb \
 	armada-388-clearfog.dtb \
 	armada-388-clearfog-pro.dtb \
+	armada-388-clearfog-base.dtb \
 	armada-388-db.dtb \
 	armada-388-gp.dtb \
 	armada-388-rd.dtb
--- /dev/null
+++ b/arch/arm/boot/dts/armada-388-clearfog-base.dts
@@ -0,0 +1,161 @@
+/*
+ * Device Tree file for SolidRun Clearfog Base revision A1 rev 2.0 (88F6828)
+ *
+ *  Copyright (C) 2015 Russell King
+ *
+ * This board is in development; the contents of this file work with
+ * the A1 rev 2.0 of the board, which does not represent final
+ * production board.  Things will change, don't expect this file to
+ * remain compatible info the future.
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License
+ *     version 2 as published by the Free Software Foundation.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "armada-388-clearfog.dtsi"
+#include "armada-38x-solidrun-microsom-emmc.dtsi"
+
+/ {
+	model = "SolidRun Clearfog Base A1";
+	compatible = "solidrun,clearfog-base-a1",
+		"solidrun,clearfog-a1", "marvell,armada388",
+		"marvell,armada385", "marvell,armada380";
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		pinctrl-0 = <&rear_button_pins>;
+		pinctrl-names = "default";
+
+		button_0 {
+			/* The rear SW3 button */
+			label = "Rear Button";
+			gpios = <&gpio1 12 GPIO_ACTIVE_LOW>;
+			linux,can-disable;
+			linux,code = <BTN_0>;
+		};
+	};
+};
+
+&eth1 {
+	phy = <&phy1>;
+};
+
+&gpio0 {
+	phy1_reset {
+		gpio-hog;
+		gpios = <19 GPIO_ACTIVE_LOW>;
+		output-low;
+		line-name = "phy1-reset";
+	};
+};
+
+&mdio {
+	pinctrl-0 = <&mdio_pins &microsom_phy_clk_pins &clearfog_phy_pins>;
+	phy1: ethernet-phy@1 {
+		/*
+		 * Annoyingly, the marvell phy driver configures the LED
+		 * register, rather than preserving reset-loaded setting.
+		 * We undo that rubbish here.
+		 */
+		marvell,reg-init = <3 16 0 0x101e>;
+		reg = <1>;
+	};
+};
+
+&pinctrl {
+	/* phy1 reset */
+	clearfog_phy_pins: clearfog-phy-pins {
+		marvell,pins = "mpp19";
+		marvell,function = "gpio";
+	};
+	rear_button_pins: rear-button-pins {
+		marvell,pins = "mpp44";
+		marvell,function = "gpio";
+	};
+};
+
+/*
+MPP
+18: pu	gpio		pca9655 int
+19:	gpio		phy reset
+20: pu	gpio		sd0 detect
+21:	sd0:cmd
+22: pd	gpio		mikro int
+23:
+
+24:	ua1:rxd		mikro rx
+25:	ua1:txd		mikro tx
+26: pu	i2c1:sck
+27: pu	i2c1:sda
+28:	sd0:clk
+29: pd	gpio		mikro rst
+30:
+31:
+
+32:
+33:
+34:
+35:
+36:
+37:	sd0:d3
+38:	sd0:d0
+39:	sd0:d1
+
+40:	sd0:d2
+41:
+42:
+43:	spi1:cs2	mikro cs
+44:	gpio		rear button sw3
+45:	ref:clk_out0	phy#0 clock
+46:	ref:clk_out1	phy#1 clock
+47:
+
+48:	gpio		J18 spare gpio
+49:	gpio		U10 I2C_IRQ(GNSS)
+50:	gpio		board id?
+51:
+52:
+53:
+54:	gpio		mikro pwm
+55:
+
+56: pu	spi1:mosi	mikro mosi
+57: pd	spi1:sck	mikro sck
+58:	spi1:miso	mikro miso
+59:
+*/
--- /dev/null
+++ b/arch/arm/boot/dts/armada-388-clearfog.dtsi
@@ -0,0 +1,282 @@
+/*
+ * Device Tree include file for SolidRun Clearfog 88F6828 based boards
+ *
+ *  Copyright (C) 2015 Russell King
+ *
+ * This board is in development; the contents of this file work with
+ * the A1 rev 2.0 of the board, which does not represent final
+ * production board.  Things will change, don't expect this file to
+ * remain compatible info the future.
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License
+ *     version 2 as published by the Free Software Foundation.
+ *
+ *     This file is distributed in the hope that it will be useful
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED , WITHOUT WARRANTY OF ANY KIND
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "armada-388.dtsi"
+#include "armada-38x-solidrun-microsom.dtsi"
+
+/ {
+	aliases {
+		/* So that mvebu u-boot can update the MAC addresses */
+		ethernet1 = &eth0;
+		ethernet2 = &eth1;
+		ethernet3 = &eth2;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	reg_3p3v: regulator-3p3v {
+		compatible = "regulator-fixed";
+		regulator-name = "3P3V";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-always-on;
+	};
+
+	soc {
+		internal-regs {
+			sata@a8000 {
+				/* pinctrl? */
+				status = "okay";
+			};
+
+			sata@e0000 {
+				/* pinctrl? */
+				status = "okay";
+			};
+
+			sdhci@d8000 {
+				bus-width = <4>;
+				cd-gpios = <&gpio0 20 GPIO_ACTIVE_LOW>;
+				no-1-8-v;
+				pinctrl-0 = <&microsom_sdhci_pins
+					     &clearfog_sdhci_cd_pins>;
+				pinctrl-names = "default";
+				status = "okay";
+				vmmc = <&reg_3p3v>;
+				wp-inverted;
+			};
+
+			usb@58000 {
+				/* CON3, nearest  power. */
+				status = "okay";
+			};
+
+			usb3@f8000 {
+				/* CON7 */
+				status = "okay";
+			};
+		};
+
+		pcie-controller {
+			status = "okay";
+			/*
+			 * The two PCIe units are accessible through
+			 * the mini-PCIe connectors on the board.
+			 */
+			pcie@2,0 {
+				/* Port 1, Lane 0. CON3, nearest power. */
+				reset-gpios = <&expander0 1 GPIO_ACTIVE_LOW>;
+				status = "okay";
+			};
+		};
+	};
+
+	sfp: sfp {
+		compatible = "sff,sfp";
+		i2c-bus = <&i2c1>;
+		los-gpio = <&expander0 12 GPIO_ACTIVE_HIGH>;
+		moddef0-gpio = <&expander0 15 GPIO_ACTIVE_LOW>;
+		sfp,ethernet = <&eth2>;
+		tx-disable-gpio = <&expander0 14 GPIO_ACTIVE_HIGH>;
+		tx-fault-gpio = <&expander0 13 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+&eth1 {
+	/* ethernet@30000 */
+	bm,pool-long = <2>;
+	bm,pool-short = <1>;
+	buffer-manager = <&bm>;
+	phy-mode = "sgmii";
+	status = "okay";
+};
+
+&eth2 {
+	/* ethernet@34000 */
+	bm,pool-long = <3>;
+	bm,pool-short = <1>;
+	buffer-manager = <&bm>;
+	managed = "in-band-status";
+	phy-mode = "sgmii";
+	status = "okay";
+};
+
+&i2c0 {
+	clock-frequency = <400000>;
+	pinctrl-0 = <&i2c0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	/*
+	 * PCA9655 GPIO expander, up to 1MHz clock.
+	 *  0-CON3 CLKREQ#
+	 *  1-CON3 PERST#
+	 *  2-
+	 *  3-CON3 W_DISABLE
+	 *  4-
+	 *  5-USB3 overcurrent
+	 *  6-USB3 power
+	 *  7-
+	 *  8-JP4 P1
+	 *  9-JP4 P4
+	 * 10-JP4 P5
+	 * 11-m.2 DEVSLP
+	 * 12-SFP_LOS
+	 * 13-SFP_TX_FAULT
+	 * 14-SFP_TX_DISABLE
+	 * 15-SFP_MOD_DEF0
+	 */
+	expander0: gpio-expander@20 {
+		/*
+		 * This is how it should be:
+		 * compatible = "onnn,pca9655", "nxp,pca9555";
+		 * but you can't do this because of the way I2C works.
+		 */
+		compatible = "nxp,pca9555";
+		gpio-controller;
+		#gpio-cells = <2>;
+		reg = <0x20>;
+
+		pcie1_0_clkreq {
+			gpio-hog;
+			gpios = <0 GPIO_ACTIVE_LOW>;
+			input;
+			line-name = "pcie1.0-clkreq";
+		};
+		pcie1_0_w_disable {
+			gpio-hog;
+			gpios = <3 GPIO_ACTIVE_LOW>;
+			output-low;
+			line-name = "pcie1.0-w-disable";
+		};
+		usb3_ilimit {
+			gpio-hog;
+			gpios = <5 GPIO_ACTIVE_LOW>;
+			input;
+			line-name = "usb3-current-limit";
+		};
+		usb3_power {
+			gpio-hog;
+			gpios = <6 GPIO_ACTIVE_HIGH>;
+			output-high;
+			line-name = "usb3-power";
+		};
+		m2_devslp {
+			gpio-hog;
+			gpios = <11 GPIO_ACTIVE_HIGH>;
+			output-low;
+			line-name = "m.2 devslp";
+		};
+	};
+
+	/* The MCP3021 supports standard and fast modes */
+	mikrobus_adc: mcp3021@4c {
+		compatible = "microchip,mcp3021";
+		reg = <0x4c>;
+	};
+};
+
+&i2c1 {
+	/*
+	 * Routed to SFP, mikrobus, and PCIe.
+	 * SFP limits this to 100kHz, and requires an AT24C01A/02/04 with
+	 *  address pins tied low, which takes addresses 0x50 and 0x51.
+	 * Mikrobus doesn't specify beyond an I2C bus being present.
+	 * PCIe uses ARP to assign addresses, or 0x63-0x64.
+	 */
+	clock-frequency = <100000>;
+	pinctrl-0 = <&clearfog_i2c1_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&pinctrl {
+	clearfog_i2c1_pins: i2c1-pins {
+		/* SFP, PCIe, mSATA, mikrobus */
+		marvell,pins = "mpp26", "mpp27";
+		marvell,function = "i2c1";
+	};
+	clearfog_sdhci_cd_pins: clearfog-sdhci-cd-pins {
+		marvell,pins = "mpp20";
+		marvell,function = "gpio";
+	};
+	mikro_pins: mikro-pins {
+		/* int: mpp22 rst: mpp29 */
+		marvell,pins = "mpp22", "mpp29";
+		marvell,function = "gpio";
+	};
+	mikro_spi_pins: mikro-spi-pins {
+		marvell,pins = "mpp43";
+		marvell,function = "spi1";
+	};
+	mikro_uart_pins: mikro-uart-pins {
+		marvell,pins = "mpp24", "mpp25";
+		marvell,function = "ua1";
+	};
+};
+
+&spi1 {
+	/*
+	 * Add SPI CS pins for clearfog:
+	 * CS0: W25Q32 (not populated on uSOM)
+	 * CS1: PIC microcontroller (Pro models)
+	 * CS2: mikrobus
+	 */
+	pinctrl-0 = <&spi1_pins &mikro_spi_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&uart1 {
+	/* mikrobus uart */
+	pinctrl-0 = <&mikro_uart_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm/boot/dts/armada-38x-solidrun-microsom-emmc.dtsi
@@ -0,0 +1,62 @@
+/*
+ * Device Tree file for SolidRun Armada 38x Microsom add-on for eMMC
+ *
+ *  Copyright (C) 2015 Russell King
+ *
+ * This board is in development; the contents of this file work with
+ * the A1 rev 2.0 of the board, which does not represent final
+ * production board.  Things will change, don't expect this file to
+ * remain compatible info the future.
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License
+ *     version 2 as published by the Free Software Foundation.
+ *
+ *     This file is distributed in the hope that it will be useful
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED , WITHOUT WARRANTY OF ANY KIND
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+/ {
+	soc {
+		internal-regs {
+			sdhci@d8000 {
+				bus-width = <4>;
+				no-1-8-v;
+				non-removable;
+				pinctrl-0 = <&microsom_sdhci_pins>;
+				pinctrl-names = "default";
+				status = "okay";
+				wp-inverted;
+			};
+		};
+	};
+};
