From 00179ef6e3c4e5db6258cd6e273e4063b8437d18 Mon Sep 17 00:00:00 2001
From: Christian Lamparter <chunkeey@gmail.com>
Date: Thu, 21 Dec 2017 15:10:18 +0100
Subject: [PATCH 3/6] crypto: crypto4xx - fix missing irq devname

crypto4xx_device's name variable is not set to anything.
The common devname for request_irq seems to be the module
name. This will fix the seemingly anonymous interrupt
entry in /proc/interrupts for crypto4xx.

Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
---
 drivers/crypto/amcc/crypto4xx_core.c | 2 +-
 drivers/crypto/amcc/crypto4xx_core.h | 1 -
 2 files changed, 1 insertion(+), 2 deletions(-)

--- a/drivers/crypto/amcc/crypto4xx_core.c
+++ b/drivers/crypto/amcc/crypto4xx_core.c
@@ -1370,7 +1370,7 @@ static int crypto4xx_probe(struct platfo
 	rc = request_irq(core_dev->irq, is_revb ?
 			 crypto4xx_ce_interrupt_handler_revb :
 			 crypto4xx_ce_interrupt_handler, 0,
-			 core_dev->dev->name, dev);
+			 KBUILD_MODNAME, dev);
 	if (rc)
 		goto err_request_irq;
 
--- a/drivers/crypto/amcc/crypto4xx_core.h
+++ b/drivers/crypto/amcc/crypto4xx_core.h
@@ -82,7 +82,6 @@ struct pd_uinfo {
 
 struct crypto4xx_device {
 	struct crypto4xx_core_device *core_dev;
-	char *name;
 	void __iomem *ce_base;
 	void __iomem *trng_base;
 
