From: Russell King <rmk+kernel@arm.linux.org.uk>
Date: Wed, 16 Sep 2015 21:27:10 +0100
Subject: [PATCH] net: mvneta: convert to phylink

Convert mvneta to use phylink, which models the MAC to PHY link in
a generic, reusable form.

Signed-off-by: Russell King <rmk+kernel@arm.linux.org.uk>
---

--- a/drivers/net/ethernet/marvell/Kconfig
+++ b/drivers/net/ethernet/marvell/Kconfig
@@ -57,7 +57,7 @@ config MVNETA
 	tristate "Marvell Armada 370/38x/XP network interface support"
 	depends on PLAT_ORION
 	select MVMDIO
-	select FIXED_PHY
+	select PHYLINK
 	---help---
 	  This driver supports the network interface units in the
 	  Marvell ARMADA XP, ARMADA 370 and ARMADA 38x SoC family.
--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -29,6 +29,7 @@
 #include <linux/of_net.h>
 #include <linux/phy.h>
 #include <linux/phy_fixed.h>
+#include <linux/phylink.h>
 #include <linux/platform_device.h>
 #include <linux/skbuff.h>
 #include <net/hwbm.h>
@@ -189,6 +190,7 @@
 #define MVNETA_GMAC_CTRL_0                       0x2c00
 #define      MVNETA_GMAC_MAX_RX_SIZE_SHIFT       2
 #define      MVNETA_GMAC_MAX_RX_SIZE_MASK        0x7ffc
+#define      MVNETA_GMAC0_PORT_1000BASE_X        BIT(1)
 #define      MVNETA_GMAC0_PORT_ENABLE            BIT(0)
 #define MVNETA_GMAC_CTRL_2                       0x2c08
 #define      MVNETA_GMAC2_INBAND_AN_ENABLE       BIT(0)
@@ -204,13 +206,19 @@
 #define      MVNETA_GMAC_TX_FLOW_CTRL_ENABLE     BIT(5)
 #define      MVNETA_GMAC_RX_FLOW_CTRL_ACTIVE     BIT(6)
 #define      MVNETA_GMAC_TX_FLOW_CTRL_ACTIVE     BIT(7)
+#define      MVNETA_GMAC_AN_COMPLETE             BIT(11)
+#define      MVNETA_GMAC_SYNC_OK                 BIT(14)
 #define MVNETA_GMAC_AUTONEG_CONFIG               0x2c0c
 #define      MVNETA_GMAC_FORCE_LINK_DOWN         BIT(0)
 #define      MVNETA_GMAC_FORCE_LINK_PASS         BIT(1)
 #define      MVNETA_GMAC_INBAND_AN_ENABLE        BIT(2)
+#define      MVNETA_GMAC_AN_BYPASS_ENABLE        BIT(3)
+#define      MVNETA_GMAC_INBAND_RESTART_AN       BIT(4)
 #define      MVNETA_GMAC_CONFIG_MII_SPEED        BIT(5)
 #define      MVNETA_GMAC_CONFIG_GMII_SPEED       BIT(6)
 #define      MVNETA_GMAC_AN_SPEED_EN             BIT(7)
+#define      MVNETA_GMAC_CONFIG_FLOW_CTRL        BIT(8)
+#define      MVNETA_GMAC_ADVERT_SYM_FLOW_CTRL    BIT(9)
 #define      MVNETA_GMAC_AN_FLOW_CTRL_EN         BIT(11)
 #define      MVNETA_GMAC_CONFIG_FULL_DUPLEX      BIT(12)
 #define      MVNETA_GMAC_AN_DUPLEX_EN            BIT(13)
@@ -400,14 +408,9 @@ struct mvneta_port {
 	u16 tx_ring_size;
 	u16 rx_ring_size;
 
-	struct mii_bus *mii_bus;
-	phy_interface_t phy_interface;
-	struct device_node *phy_node;
-	unsigned int link;
-	unsigned int duplex;
-	unsigned int speed;
+	struct device_node *dn;
 	unsigned int tx_csum_limit;
-	unsigned int use_inband_status:1;
+	struct phylink *phylink;
 
 	struct mvneta_bm *bm_priv;
 	struct mvneta_bm_pool *pool_long;
@@ -1182,10 +1185,6 @@ static void mvneta_port_disable(struct m
 	val &= ~MVNETA_GMAC0_PORT_ENABLE;
 	mvreg_write(pp, MVNETA_GMAC_CTRL_0, val);
 
-	pp->link = 0;
-	pp->duplex = -1;
-	pp->speed = 0;
-
 	udelay(200);
 }
 
@@ -1245,44 +1244,6 @@ static void mvneta_set_other_mcast_table
 		mvreg_write(pp, MVNETA_DA_FILT_OTH_MCAST + offset, val);
 }
 
-static void mvneta_set_autoneg(struct mvneta_port *pp, int enable)
-{
-	u32 val;
-
-	if (enable) {
-		val = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
-		val &= ~(MVNETA_GMAC_FORCE_LINK_PASS |
-			 MVNETA_GMAC_FORCE_LINK_DOWN |
-			 MVNETA_GMAC_AN_FLOW_CTRL_EN);
-		val |= MVNETA_GMAC_INBAND_AN_ENABLE |
-		       MVNETA_GMAC_AN_SPEED_EN |
-		       MVNETA_GMAC_AN_DUPLEX_EN;
-		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG, val);
-
-		val = mvreg_read(pp, MVNETA_GMAC_CLOCK_DIVIDER);
-		val |= MVNETA_GMAC_1MS_CLOCK_ENABLE;
-		mvreg_write(pp, MVNETA_GMAC_CLOCK_DIVIDER, val);
-
-		val = mvreg_read(pp, MVNETA_GMAC_CTRL_2);
-		val |= MVNETA_GMAC2_INBAND_AN_ENABLE;
-		mvreg_write(pp, MVNETA_GMAC_CTRL_2, val);
-	} else {
-		val = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
-		val &= ~(MVNETA_GMAC_INBAND_AN_ENABLE |
-		       MVNETA_GMAC_AN_SPEED_EN |
-		       MVNETA_GMAC_AN_DUPLEX_EN);
-		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG, val);
-
-		val = mvreg_read(pp, MVNETA_GMAC_CLOCK_DIVIDER);
-		val &= ~MVNETA_GMAC_1MS_CLOCK_ENABLE;
-		mvreg_write(pp, MVNETA_GMAC_CLOCK_DIVIDER, val);
-
-		val = mvreg_read(pp, MVNETA_GMAC_CTRL_2);
-		val &= ~MVNETA_GMAC2_INBAND_AN_ENABLE;
-		mvreg_write(pp, MVNETA_GMAC_CTRL_2, val);
-	}
-}
-
 static void mvneta_percpu_unmask_interrupt(void *arg)
 {
 	struct mvneta_port *pp = arg;
@@ -1430,7 +1391,6 @@ static void mvneta_defaults_set(struct m
 	val &= ~MVNETA_PHY_POLLING_ENABLE;
 	mvreg_write(pp, MVNETA_UNIT_CONTROL, val);
 
-	mvneta_set_autoneg(pp, pp->use_inband_status);
 	mvneta_set_ucast_table(pp, -1);
 	mvneta_set_special_mcast_table(pp, -1);
 	mvneta_set_other_mcast_table(pp, -1);
@@ -2635,26 +2595,11 @@ static irqreturn_t mvneta_isr(int irq, v
 	return IRQ_HANDLED;
 }
 
-static int mvneta_fixed_link_update(struct mvneta_port *pp,
-				    struct phy_device *phy)
+static void mvneta_link_change(struct mvneta_port *pp)
 {
-	struct fixed_phy_status status;
-	struct fixed_phy_status changed = {};
 	u32 gmac_stat = mvreg_read(pp, MVNETA_GMAC_STATUS);
 
-	status.link = !!(gmac_stat & MVNETA_GMAC_LINK_UP);
-	if (gmac_stat & MVNETA_GMAC_SPEED_1000)
-		status.speed = SPEED_1000;
-	else if (gmac_stat & MVNETA_GMAC_SPEED_100)
-		status.speed = SPEED_100;
-	else
-		status.speed = SPEED_10;
-	status.duplex = !!(gmac_stat & MVNETA_GMAC_FULL_DUPLEX);
-	changed.link = 1;
-	changed.speed = 1;
-	changed.duplex = 1;
-	fixed_phy_update_state(phy, &status, &changed);
-	return 0;
+	phylink_mac_change(pp->phylink, !!(gmac_stat & MVNETA_GMAC_LINK_UP));
 }
 
 /* NAPI handler
@@ -2670,7 +2615,6 @@ static int mvneta_poll(struct napi_struc
 	u32 cause_rx_tx;
 	int rx_queue;
 	struct mvneta_port *pp = netdev_priv(napi->dev);
-	struct net_device *ndev = pp->dev;
 	struct mvneta_pcpu_port *port = this_cpu_ptr(pp->ports);
 
 	if (!netif_running(pp->dev)) {
@@ -2684,12 +2628,11 @@ static int mvneta_poll(struct napi_struc
 		u32 cause_misc = mvreg_read(pp, MVNETA_INTR_MISC_CAUSE);
 
 		mvreg_write(pp, MVNETA_INTR_MISC_CAUSE, 0);
-		if (pp->use_inband_status && (cause_misc &
-				(MVNETA_CAUSE_PHY_STATUS_CHANGE |
-				 MVNETA_CAUSE_LINK_CHANGE |
-				 MVNETA_CAUSE_PSC_SYNC_CHANGE))) {
-			mvneta_fixed_link_update(pp, ndev->phydev);
-		}
+
+		if (cause_misc & (MVNETA_CAUSE_PHY_STATUS_CHANGE |
+				  MVNETA_CAUSE_LINK_CHANGE |
+				  MVNETA_CAUSE_PSC_SYNC_CHANGE))
+			mvneta_link_change(pp);
 	}
 
 	/* Release Tx descriptors */
@@ -2985,7 +2928,6 @@ static int mvneta_setup_txqs(struct mvne
 static void mvneta_start_dev(struct mvneta_port *pp)
 {
 	int cpu;
-	struct net_device *ndev = pp->dev;
 
 	mvneta_max_rx_size_set(pp, pp->pkt_size);
 	mvneta_txq_max_tx_size_set(pp, pp->pkt_size);
@@ -3008,16 +2950,15 @@ static void mvneta_start_dev(struct mvne
 		    MVNETA_CAUSE_LINK_CHANGE |
 		    MVNETA_CAUSE_PSC_SYNC_CHANGE);
 
-	phy_start(ndev->phydev);
+	phylink_start(pp->phylink);
 	netif_tx_start_all_queues(pp->dev);
 }
 
 static void mvneta_stop_dev(struct mvneta_port *pp)
 {
 	unsigned int cpu;
-	struct net_device *ndev = pp->dev;
 
-	phy_stop(ndev->phydev);
+	phylink_stop(pp->phylink);
 
 	for_each_online_cpu(cpu) {
 		struct mvneta_pcpu_port *port = per_cpu_ptr(pp->ports, cpu);
@@ -3187,99 +3128,210 @@ static int mvneta_set_mac_addr(struct ne
 	return 0;
 }
 
-static void mvneta_adjust_link(struct net_device *ndev)
+static void mvneta_validate_support(struct net_device *ndev, unsigned int mode,
+				    unsigned long *support)
+{
+	__ETHTOOL_DECLARE_LINK_MODE_MASK(mask) = { 0, };
+
+	/* Allow all the expected bits */
+	phylink_set(mask, Autoneg);
+	phylink_set(mask, TP);
+	phylink_set(mask, AUI);
+	phylink_set(mask, MII);
+	phylink_set(mask, FIBRE);
+	phylink_set(mask, BNC);
+	phylink_set(mask, Backplane);
+
+	/* Half-duplex at speeds higher than 100Mbit is unsupported */
+	phylink_set(mask, 1000baseT_Full);
+	phylink_set(mask, 1000baseX_Full);
+
+	if (mode != MLO_AN_8023Z) {
+		/* 10M and 100M are only supported in non-802.3z mode */
+		phylink_set(mask, 10baseT_Half);
+		phylink_set(mask, 10baseT_Full);
+		phylink_set(mask, 100baseT_Half);
+		phylink_set(mask, 100baseT_Full);
+	} else {
+		phylink_set(mask, Pause);
+	}
+
+	bitmap_and(support, support, mask, __ETHTOOL_LINK_MODE_MASK_NBITS);
+}
+
+static int mvneta_mac_link_state(struct net_device *ndev,
+				 struct phylink_link_state *state)
 {
 	struct mvneta_port *pp = netdev_priv(ndev);
-	struct phy_device *phydev = ndev->phydev;
-	int status_change = 0;
+	u32 gmac_stat;
 
-	if (phydev->link) {
-		if ((pp->speed != phydev->speed) ||
-		    (pp->duplex != phydev->duplex)) {
-			u32 val;
-
-			val = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
-			val &= ~(MVNETA_GMAC_CONFIG_MII_SPEED |
-				 MVNETA_GMAC_CONFIG_GMII_SPEED |
-				 MVNETA_GMAC_CONFIG_FULL_DUPLEX);
-
-			if (phydev->duplex)
-				val |= MVNETA_GMAC_CONFIG_FULL_DUPLEX;
-
-			if (phydev->speed == SPEED_1000)
-				val |= MVNETA_GMAC_CONFIG_GMII_SPEED;
-			else if (phydev->speed == SPEED_100)
-				val |= MVNETA_GMAC_CONFIG_MII_SPEED;
+	gmac_stat = mvreg_read(pp, MVNETA_GMAC_STATUS);
 
-			mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG, val);
+	if (gmac_stat & MVNETA_GMAC_SPEED_1000)
+		state->speed = SPEED_1000;
+	else if (gmac_stat & MVNETA_GMAC_SPEED_100)
+		state->speed = SPEED_100;
+	else
+		state->speed = SPEED_10;
 
-			pp->duplex = phydev->duplex;
-			pp->speed  = phydev->speed;
-		}
+	state->an_complete = !!(gmac_stat & MVNETA_GMAC_AN_COMPLETE);
+	state->link = !!(gmac_stat & MVNETA_GMAC_LINK_UP);
+	state->duplex = !!(gmac_stat & MVNETA_GMAC_FULL_DUPLEX);
+
+	return 1;
+}
+
+static void mvneta_mac_an_restart(struct net_device *ndev, unsigned int mode)
+{
+	struct mvneta_port *pp = netdev_priv(ndev);
+
+	if (mode == MLO_AN_8023Z) {
+		u32 gmac_an = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
+
+		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG,
+			    gmac_an | MVNETA_GMAC_INBAND_RESTART_AN);
+		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG,
+			    gmac_an & ~MVNETA_GMAC_INBAND_RESTART_AN);
 	}
+}
 
-	if (phydev->link != pp->link) {
-		if (!phydev->link) {
-			pp->duplex = -1;
-			pp->speed = 0;
-		}
+static void mvneta_mac_config(struct net_device *ndev, unsigned int mode,
+	const struct phylink_link_state *state)
+{
+	struct mvneta_port *pp = netdev_priv(ndev);
+	u32 new_ctrl0, gmac_ctrl0 = mvreg_read(pp, MVNETA_GMAC_CTRL_0);
+	u32 new_ctrl2, gmac_ctrl2 = mvreg_read(pp, MVNETA_GMAC_CTRL_2);
+	u32 new_clk, gmac_clk = mvreg_read(pp, MVNETA_GMAC_CLOCK_DIVIDER);
+	u32 new_an, gmac_an = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
+
+	new_ctrl0 = gmac_ctrl0 & ~MVNETA_GMAC0_PORT_1000BASE_X;
+	new_ctrl2 = gmac_ctrl2 & ~MVNETA_GMAC2_INBAND_AN_ENABLE;
+	new_clk = gmac_clk & ~MVNETA_GMAC_1MS_CLOCK_ENABLE;
+	new_an = gmac_an & ~(MVNETA_GMAC_INBAND_AN_ENABLE |
+			     MVNETA_GMAC_INBAND_RESTART_AN |
+			     MVNETA_GMAC_CONFIG_MII_SPEED |
+			     MVNETA_GMAC_CONFIG_GMII_SPEED |
+			     MVNETA_GMAC_AN_SPEED_EN |
+			     MVNETA_GMAC_ADVERT_SYM_FLOW_CTRL |
+			     MVNETA_GMAC_CONFIG_FLOW_CTRL |
+			     MVNETA_GMAC_AN_FLOW_CTRL_EN |
+			     MVNETA_GMAC_CONFIG_FULL_DUPLEX |
+			     MVNETA_GMAC_AN_DUPLEX_EN);
+
+	if (phylink_test(state->advertising, Pause))
+		new_an |= MVNETA_GMAC_ADVERT_SYM_FLOW_CTRL;
+
+	switch (mode) {
+	case MLO_AN_SGMII:
+		/* SGMII mode receives the state from the PHY */
+		new_ctrl2 |= MVNETA_GMAC2_INBAND_AN_ENABLE;
+		new_clk |= MVNETA_GMAC_1MS_CLOCK_ENABLE;
+		new_an = (new_an & ~(MVNETA_GMAC_FORCE_LINK_DOWN |
+				     MVNETA_GMAC_FORCE_LINK_PASS)) |
+			 MVNETA_GMAC_INBAND_AN_ENABLE |
+			 MVNETA_GMAC_AN_SPEED_EN |
+			 MVNETA_GMAC_AN_DUPLEX_EN;
+		break;
 
-		pp->link = phydev->link;
-		status_change = 1;
+	case MLO_AN_8023Z:
+		/* 802.3z negotiation - only 1000base-X */
+		new_ctrl0 |= MVNETA_GMAC0_PORT_1000BASE_X;
+		new_clk |= MVNETA_GMAC_1MS_CLOCK_ENABLE;
+		new_an = (new_an & ~(MVNETA_GMAC_FORCE_LINK_DOWN |
+				     MVNETA_GMAC_FORCE_LINK_PASS)) |
+			 MVNETA_GMAC_INBAND_AN_ENABLE |
+			 MVNETA_GMAC_CONFIG_GMII_SPEED |
+			 /* The MAC only supports FD mode */
+			 MVNETA_GMAC_CONFIG_FULL_DUPLEX;
+
+		if (state->an_enabled)
+			new_an |= MVNETA_GMAC_AN_FLOW_CTRL_EN;
+		break;
+
+	default:
+		/* Phy or fixed speed */
+		if (state->duplex)
+			new_an |= MVNETA_GMAC_CONFIG_FULL_DUPLEX;
+
+		if (state->speed == SPEED_1000)
+			new_an |= MVNETA_GMAC_CONFIG_GMII_SPEED;
+		else if (state->speed == SPEED_100)
+			new_an |= MVNETA_GMAC_CONFIG_MII_SPEED;
+		break;
 	}
 
-	if (status_change) {
-		if (phydev->link) {
-			if (!pp->use_inband_status) {
-				u32 val = mvreg_read(pp,
-						  MVNETA_GMAC_AUTONEG_CONFIG);
-				val &= ~MVNETA_GMAC_FORCE_LINK_DOWN;
-				val |= MVNETA_GMAC_FORCE_LINK_PASS;
-				mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG,
-					    val);
-			}
-			mvneta_port_up(pp);
-		} else {
-			if (!pp->use_inband_status) {
-				u32 val = mvreg_read(pp,
-						  MVNETA_GMAC_AUTONEG_CONFIG);
-				val &= ~MVNETA_GMAC_FORCE_LINK_PASS;
-				val |= MVNETA_GMAC_FORCE_LINK_DOWN;
-				mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG,
-					    val);
-			}
-			mvneta_port_down(pp);
-		}
-		phy_print_status(phydev);
+	/* Armada 370 documentation says we can only change the port mode
+	 * and in-band enable when the link is down, so force it down
+	 * while making these changes. We also do this for GMAC_CTRL2 */
+	if ((new_ctrl0 ^ gmac_ctrl0) & MVNETA_GMAC0_PORT_1000BASE_X ||
+	    (new_ctrl2 ^ gmac_ctrl2) & MVNETA_GMAC2_INBAND_AN_ENABLE ||
+	    (new_an  ^ gmac_an) & MVNETA_GMAC_INBAND_AN_ENABLE) {
+		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG,
+			    (gmac_an & ~MVNETA_GMAC_FORCE_LINK_PASS) |
+			    MVNETA_GMAC_FORCE_LINK_DOWN);
+	}
+
+	if (new_ctrl0 != gmac_ctrl0)
+		mvreg_write(pp, MVNETA_GMAC_CTRL_0, new_ctrl0);
+	if (new_ctrl2 != gmac_ctrl2)
+		mvreg_write(pp, MVNETA_GMAC_CTRL_2, new_ctrl2);
+	if (new_clk != gmac_clk)
+		mvreg_write(pp, MVNETA_GMAC_CLOCK_DIVIDER, new_clk);
+	if (new_an != gmac_an)
+		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG, new_an);
+}
+
+static void mvneta_mac_link_down(struct net_device *ndev, unsigned int mode)
+{
+	struct mvneta_port *pp = netdev_priv(ndev);
+	u32 val;
+
+	mvneta_port_down(pp);
+
+	if (mode == MLO_AN_PHY || mode == MLO_AN_FIXED) {
+		val = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
+		val &= ~MVNETA_GMAC_FORCE_LINK_PASS;
+		val |= MVNETA_GMAC_FORCE_LINK_DOWN;
+		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG, val);
 	}
 }
 
-static int mvneta_mdio_probe(struct mvneta_port *pp)
+static void mvneta_mac_link_up(struct net_device *ndev, unsigned int mode)
 {
-	struct phy_device *phy_dev;
+	struct mvneta_port *pp = netdev_priv(ndev);
+	u32 val;
 
-	phy_dev = of_phy_connect(pp->dev, pp->phy_node, mvneta_adjust_link, 0,
-				 pp->phy_interface);
-	if (!phy_dev) {
-		netdev_err(pp->dev, "could not find the PHY\n");
-		return -ENODEV;
+	if (mode == MLO_AN_PHY || mode == MLO_AN_FIXED) {
+		val = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
+		val &= ~MVNETA_GMAC_FORCE_LINK_DOWN;
+		val |= MVNETA_GMAC_FORCE_LINK_PASS;
+		mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG, val);
 	}
 
-	phy_dev->supported &= PHY_GBIT_FEATURES;
-	phy_dev->advertising = phy_dev->supported;
+	mvneta_port_up(pp);
+}
 
-	pp->link    = 0;
-	pp->duplex  = 0;
-	pp->speed   = 0;
+static const struct phylink_mac_ops mvneta_phylink_ops = {
+	.validate_support = mvneta_validate_support,
+	.mac_link_state = mvneta_mac_link_state,
+	.mac_an_restart = mvneta_mac_an_restart,
+	.mac_config = mvneta_mac_config,
+	.mac_link_down = mvneta_mac_link_down,
+	.mac_link_up = mvneta_mac_link_up,
+};
 
-	return 0;
+static int mvneta_mdio_probe(struct mvneta_port *pp)
+{
+	int err = phylink_of_phy_connect(pp->phylink, pp->dn);
+	if (err)
+		netdev_err(pp->dev, "could not attach PHY\n");
+
+	return err;
 }
 
 static void mvneta_mdio_remove(struct mvneta_port *pp)
 {
-	struct net_device *ndev = pp->dev;
-
-	phy_disconnect(ndev->phydev);
+	phylink_disconnect_phy(pp->phylink);
 }
 
 /* Electing a CPU must be done in an atomic way: it should be done
@@ -3537,10 +3589,9 @@ static int mvneta_stop(struct net_device
 
 static int mvneta_ioctl(struct net_device *dev, struct ifreq *ifr, int cmd)
 {
-	if (!dev->phydev)
-		return -ENOTSUPP;
+	struct mvneta_port *pp = netdev_priv(dev);
 
-	return phy_mii_ioctl(dev->phydev, ifr, cmd);
+	return phylink_mii_ioctl(pp->phylink, ifr, cmd);
 }
 
 /* Ethtool methods */
@@ -3551,44 +3602,18 @@ mvneta_ethtool_set_link_ksettings(struct
 				  const struct ethtool_link_ksettings *cmd)
 {
 	struct mvneta_port *pp = netdev_priv(ndev);
-	struct phy_device *phydev = ndev->phydev;
-
-	if (!phydev)
-		return -ENODEV;
 
-	if ((cmd->base.autoneg == AUTONEG_ENABLE) != pp->use_inband_status) {
-		u32 val;
-
-		mvneta_set_autoneg(pp, cmd->base.autoneg == AUTONEG_ENABLE);
-
-		if (cmd->base.autoneg == AUTONEG_DISABLE) {
-			val = mvreg_read(pp, MVNETA_GMAC_AUTONEG_CONFIG);
-			val &= ~(MVNETA_GMAC_CONFIG_MII_SPEED |
-				 MVNETA_GMAC_CONFIG_GMII_SPEED |
-				 MVNETA_GMAC_CONFIG_FULL_DUPLEX);
-
-			if (phydev->duplex)
-				val |= MVNETA_GMAC_CONFIG_FULL_DUPLEX;
-
-			if (phydev->speed == SPEED_1000)
-				val |= MVNETA_GMAC_CONFIG_GMII_SPEED;
-			else if (phydev->speed == SPEED_100)
-				val |= MVNETA_GMAC_CONFIG_MII_SPEED;
-
-			mvreg_write(pp, MVNETA_GMAC_AUTONEG_CONFIG, val);
-		}
+	return phylink_ethtool_ksettings_set(pp->phylink, cmd);
+}
 
-		pp->use_inband_status = (cmd->base.autoneg == AUTONEG_ENABLE);
-		netdev_info(pp->dev, "autoneg status set to %i\n",
-			    pp->use_inband_status);
-
-		if (netif_running(ndev)) {
-			mvneta_port_down(pp);
-			mvneta_port_up(pp);
-		}
-	}
+/* Get link ksettings for ethtools */
+static int
+mvneta_ethtool_get_link_ksettings(struct net_device *ndev,
+				  struct ethtool_link_ksettings *cmd)
+{
+	struct mvneta_port *pp = netdev_priv(ndev);
 
-	return phy_ethtool_ksettings_set(ndev->phydev, cmd);
+	return phylink_ethtool_ksettings_get(pp->phylink, cmd);
 }
 
 /* Set interrupt coalescing for ethtools */
@@ -3696,26 +3721,28 @@ static void mvneta_ethtool_update_stats(
 {
 	const struct mvneta_statistic *s;
 	void __iomem *base = pp->base;
-	u32 high, low, val;
-	u64 val64;
+	u32 high, low;
+	u64 val;
 	int i;
 
 	for (i = 0, s = mvneta_statistics;
 	     s < mvneta_statistics + ARRAY_SIZE(mvneta_statistics);
 	     s++, i++) {
+		val = 0;
+
 		switch (s->type) {
 		case T_REG_32:
 			val = readl_relaxed(base + s->offset);
-			pp->ethtool_stats[i] += val;
 			break;
 		case T_REG_64:
 			/* Docs say to read low 32-bit then high */
 			low = readl_relaxed(base + s->offset);
 			high = readl_relaxed(base + s->offset + 4);
-			val64 = (u64)high << 32 | low;
-			pp->ethtool_stats[i] += val64;
+			val = (u64)high << 32 | low;
 			break;
 		}
+
+		pp->ethtool_stats[i] += val;
 	}
 }
 
@@ -3875,7 +3902,7 @@ const struct ethtool_ops mvneta_eth_tool
 	.get_rxnfc	= mvneta_ethtool_get_rxnfc,
 	.get_rxfh	= mvneta_ethtool_get_rxfh,
 	.set_rxfh	= mvneta_ethtool_set_rxfh,
-	.get_link_ksettings = phy_ethtool_get_link_ksettings,
+	.get_link_ksettings = mvneta_ethtool_get_link_ksettings,
 	.set_link_ksettings = mvneta_ethtool_set_link_ksettings,
 };
 
@@ -4002,14 +4029,13 @@ static int mvneta_probe(struct platform_
 	const struct mbus_dram_target_info *dram_target_info;
 	struct resource *res;
 	struct device_node *dn = pdev->dev.of_node;
-	struct device_node *phy_node;
 	struct device_node *bm_node;
 	struct mvneta_port *pp;
 	struct net_device *dev;
+	struct phylink *phylink;
 	const char *dt_mac_addr;
 	char hw_mac_addr[ETH_ALEN];
 	const char *mac_from;
-	const char *managed;
 	int tx_csum_limit;
 	int phy_mode;
 	int err;
@@ -4025,31 +4051,11 @@ static int mvneta_probe(struct platform_
 		goto err_free_netdev;
 	}
 
-	phy_node = of_parse_phandle(dn, "phy", 0);
-	if (!phy_node) {
-		if (!of_phy_is_fixed_link(dn)) {
-			dev_err(&pdev->dev, "no PHY specified\n");
-			err = -ENODEV;
-			goto err_free_irq;
-		}
-
-		err = of_phy_register_fixed_link(dn);
-		if (err < 0) {
-			dev_err(&pdev->dev, "cannot register fixed PHY\n");
-			goto err_free_irq;
-		}
-
-		/* In the case of a fixed PHY, the DT node associated
-		 * to the PHY is the Ethernet MAC DT node.
-		 */
-		phy_node = of_node_get(dn);
-	}
-
 	phy_mode = of_get_phy_mode(dn);
 	if (phy_mode < 0) {
 		dev_err(&pdev->dev, "incorrect phy-mode\n");
 		err = -EINVAL;
-		goto err_put_phy_node;
+		goto err_free_irq;
 	}
 
 	dev->tx_queue_len = MVNETA_MAX_TXD;
@@ -4060,12 +4066,7 @@ static int mvneta_probe(struct platform_
 
 	pp = netdev_priv(dev);
 	spin_lock_init(&pp->lock);
-	pp->phy_node = phy_node;
-	pp->phy_interface = phy_mode;
-
-	err = of_property_read_string(dn, "managed", &managed);
-	pp->use_inband_status = (err == 0 &&
-				 strcmp(managed, "in-band-status") == 0);
+	pp->dn = dn;
 
 	pp->rxq_def = rxq_def;
 
@@ -4076,7 +4077,7 @@ static int mvneta_probe(struct platform_
 		pp->clk = devm_clk_get(&pdev->dev, NULL);
 	if (IS_ERR(pp->clk)) {
 		err = PTR_ERR(pp->clk);
-		goto err_put_phy_node;
+		goto err_free_irq;
 	}
 
 	clk_prepare_enable(pp->clk);
@@ -4184,6 +4185,14 @@ static int mvneta_probe(struct platform_
 	dev->priv_flags |= IFF_LIVE_ADDR_CHANGE;
 	dev->gso_max_segs = MVNETA_MAX_TSO_SEGS;
 
+	phylink = phylink_create(dev, dn, phy_mode, &mvneta_phylink_ops);
+	if (IS_ERR(phylink)) {
+		err = PTR_ERR(phylink);
+		goto err_free_stats;
+	}
+
+	pp->phylink = phylink;
+
 	err = register_netdev(dev);
 	if (err < 0) {
 		dev_err(&pdev->dev, "failed to register\n");
@@ -4195,14 +4204,6 @@ static int mvneta_probe(struct platform_
 
 	platform_set_drvdata(pdev, pp->dev);
 
-	if (pp->use_inband_status) {
-		struct phy_device *phy = of_phy_find_device(dn);
-
-		mvneta_fixed_link_update(pp, phy);
-
-		put_device(&phy->mdio.dev);
-	}
-
 	return 0;
 
 err_netdev:
@@ -4213,16 +4214,14 @@ err_netdev:
 				       1 << pp->id);
 	}
 err_free_stats:
+	if (pp->phylink)
+		phylink_destroy(pp->phylink);
 	free_percpu(pp->stats);
 err_free_ports:
 	free_percpu(pp->ports);
 err_clk:
 	clk_disable_unprepare(pp->clk_bus);
 	clk_disable_unprepare(pp->clk);
-err_put_phy_node:
-	of_node_put(phy_node);
-	if (of_phy_is_fixed_link(dn))
-		of_phy_deregister_fixed_link(dn);
 err_free_irq:
 	irq_dispose_mapping(dev->irq);
 err_free_netdev:
@@ -4234,7 +4233,6 @@ err_free_netdev:
 static int mvneta_remove(struct platform_device *pdev)
 {
 	struct net_device  *dev = platform_get_drvdata(pdev);
-	struct device_node *dn = pdev->dev.of_node;
 	struct mvneta_port *pp = netdev_priv(dev);
 
 	unregister_netdev(dev);
@@ -4242,10 +4240,8 @@ static int mvneta_remove(struct platform
 	clk_disable_unprepare(pp->clk);
 	free_percpu(pp->ports);
 	free_percpu(pp->stats);
-	if (of_phy_is_fixed_link(dn))
-		of_phy_deregister_fixed_link(dn);
 	irq_dispose_mapping(dev->irq);
-	of_node_put(pp->phy_node);
+	phylink_destroy(pp->phylink);
 	free_netdev(dev);
 
 	if (pp->bm_priv) {
