From 4ac9222778478a00c7fc9d347b7ed1e0e595120d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 4 Jan 2018 08:05:34 +0100
Subject: [PATCH] mtd: ofpart: add of_match_table with "fixed-partitions"
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This allows using this parser with any flash driver that takes care of
setting of_node (using mtd_set_of_node helper) correctly. Up to now
support for "fixed-partitions" DT compatibility string was working only
with flash drivers that were specifying "ofpart" (manually or by letting
mtd use the default set of parsers).

This matches existing bindings documentation.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Reviewed-by: Brian Norris <computersforpeace@gmail.com>
Tested-by: Brian Norris <computersforpeace@gmail.com>
Signed-off-by: Boris Brezillon <boris.brezillon@free-electrons.com>
---
 drivers/mtd/ofpart.c | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/drivers/mtd/ofpart.c
+++ b/drivers/mtd/ofpart.c
@@ -140,9 +140,16 @@ ofpart_none:
 	return ret;
 }
 
+static const struct of_device_id parse_ofpart_match_table[] = {
+	{ .compatible = "fixed-partitions" },
+	{},
+};
+MODULE_DEVICE_TABLE(of, parse_ofpart_match_table);
+
 static struct mtd_part_parser ofpart_parser = {
 	.parse_fn = parse_ofpart_partitions,
 	.name = "ofpart",
+	.of_match_table = parse_ofpart_match_table,
 };
 
 static int parse_ofoldpart_partitions(struct mtd_info *master,
