From bf25fbdc7dfb256f267725336e29e232aadd5123 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Fri, 21 Jul 2017 08:43:58 +0200
Subject: [PATCH 36/57] net-next: mediatek: fix typos inside the header file

Trivial patch fixing 2 typos.

Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.h | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -525,8 +525,8 @@ struct mtk_rx_ring {
  * @pctl:		The register map pointing at the range used to setup
  *			GMAC port drive/slew values
  * @dma_refcnt:		track how many netdevs are using the DMA engine
- * @tx_ring:		Pointer to the memore holding info about the TX ring
- * @rx_ring:		Pointer to the memore holding info about the RX ring
+ * @tx_ring:		Pointer to the memory holding info about the TX ring
+ * @rx_ring:		Pointer to the memory holding info about the RX ring
  * @tx_napi:		The TX NAPI struct
  * @rx_napi:		The RX NAPI struct
  * @scratch_ring:	Newer SoCs need memory for a second HW managed TX ring
