From ec3e465ecf3f7dd26f2e22170e4c5f4b9979df5d Mon Sep 17 00:00:00 2001
From: Matthew McClintock <mmcclint@codeaurora.org>
Date: Mon, 21 Mar 2016 15:55:21 -0500
Subject: [PATCH 26/69] dts: ipq4019: Add support for IPQ4019 DK04 board

This is pretty similiar to a DK01 but has a bit more IO. Some notable
differences are listed below however they are not in the device tree yet
as we continue adding more support

- second serial port
- PCIe
- NAND
- SD/EMMC

Signed-off-by: Matthew McClintock <mmcclint@codeaurora.org>
---
 arch/arm/boot/dts/Makefile                      |   1 +
 arch/arm/boot/dts/qcom-ipq4019-ap.dk01.1.dtsi   |  12 +-
 arch/arm/boot/dts/qcom-ipq4019-ap.dk04.1-c1.dts |  21 +++
 arch/arm/boot/dts/qcom-ipq4019-ap.dk04.1.dtsi   | 163 ++++++++++++++++++++++++
 4 files changed, 189 insertions(+), 8 deletions(-)
 create mode 100644 arch/arm/boot/dts/qcom-ipq4019-ap.dk04.1-c1.dts
 create mode 100644 arch/arm/boot/dts/qcom-ipq4019-ap.dk04.1.dtsi

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -617,6 +617,7 @@ dtb-$(CONFIG_ARCH_QCOM) += \
 	qcom-apq8084-ifc6540.dtb \
 	qcom-apq8084-mtp.dtb \
 	qcom-ipq4019-ap.dk01.1-c1.dtb \
+	qcom-ipq4019-ap.dk04.1-c1.dtb \
 	qcom-ipq8064-ap148.dtb \
 	qcom-msm8660-surf.dtb \
 	qcom-msm8960-cdp.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/qcom-ipq4019-ap.dk04.1-c1.dts
@@ -0,0 +1,22 @@
+/* Copyright (c) 2015, The Linux Foundation. All rights reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
+ * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
+ * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
+ * OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ */
+
+#include "qcom-ipq4019-ap.dk04.1.dtsi"
+
+/ {
+	model = "Qualcomm Technologies, Inc. IPQ40xx/AP-DK04.1-C1";
+	compatible = "qcom,ap-dk04.1-c1", "qcom,ipq4019";
+};
--- /dev/null
+++ b/arch/arm/boot/dts/qcom-ipq4019-ap.dk04.1.dtsi
@@ -0,0 +1,163 @@
+/* Copyright (c) 2015, The Linux Foundation. All rights reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
+ * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
+ * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
+ * OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ */
+
+#include "qcom-ipq4019.dtsi"
+
+/ {
+	model = "Qualcomm Technologies, Inc. IPQ4019/AP-DK04.1";
+	compatible = "qcom,ipq4019";
+
+	clocks {
+                xo: xo {
+                        compatible = "fixed-clock";
+                        clock-frequency = <48000000>;
+                        #clock-cells = <0>;
+                };
+	};
+
+	soc {
+		timer {
+			compatible = "arm,armv7-timer";
+			interrupts = <1 2 0xf08>,
+				     <1 3 0xf08>,
+				     <1 4 0xf08>,
+				     <1 1 0xf08>;
+			clock-frequency = <48000000>;
+		};
+
+		pinctrl@0x01000000 {
+			serial_0_pins: serial_pinmux {
+				mux {
+					pins = "gpio16", "gpio17";
+					function = "blsp_uart0";
+					bias-disable;
+				};
+			};
+
+                       serial_1_pins: serial1_pinmux {
+				mux {
+					pins = "gpio8", "gpio9";
+					function = "blsp_uart1";
+					bias-disable;
+				};
+			};
+
+			spi_0_pins: spi_0_pinmux {
+				pinmux {
+					function = "blsp_spi0";
+					pins = "gpio13", "gpio14", "gpio15";
+				};
+				pinmux_cs {
+					function = "gpio";
+					pins = "gpio12";
+				};
+				pinconf {
+					pins = "gpio13", "gpio14", "gpio15";
+					drive-strength = <12>;
+					bias-disable;
+				};
+				pinconf_cs {
+					pins = "gpio12";
+					drive-strength = <2>;
+					bias-disable;
+					output-high;
+				};
+			};
+
+			i2c_0_pins: i2c_0_pinmux {
+				pinmux {
+					function = "blsp_i2c0";
+					pins = "gpio10", "gpio11";
+				};
+				pinconf {
+					pins = "gpio10", "gpio11";
+					drive-strength = <16>;
+					bias-disable;
+				};
+			};
+		};
+
+		blsp_dma: dma@7884000 {
+			status = "ok";
+		};
+
+		spi_0: spi@78b5000 {
+			pinctrl-0 = <&spi_0_pins>;
+			pinctrl-names = "default";
+			status = "ok";
+			cs-gpios = <&tlmm 12 0>;
+
+			mx25l25635e@0 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				reg = <0>;
+				compatible = "mx25l25635e";
+				spi-max-frequency = <24000000>;
+			};
+		};
+
+		i2c_0: i2c@78b7000 { /* BLSP1 QUP2 */
+			pinctrl-0 = <&i2c_0_pins>;
+			pinctrl-names = "default";
+
+			status = "ok";
+		};
+
+		serial@78af000 {
+			pinctrl-0 = <&serial_0_pins>;
+			pinctrl-names = "default";
+			status = "ok";
+		};
+
+		serial@78b0000 {
+			pinctrl-0 = <&serial_1_pins>;
+			pinctrl-names = "default";
+			status = "ok";
+		};
+
+		usb3_ss_phy: ssphy@9a000 {
+			status = "ok";
+		};
+
+		usb3_hs_phy: hsphy@a6000 {
+			status = "ok";
+		};
+
+		usb3: usb3@8af8800 {
+			status = "ok";
+		};
+
+		usb2_hs_phy: hsphy@a8000 {
+			status = "ok";
+		};
+
+		usb2: usb2@60f8800 {
+			status = "ok";
+		};
+
+		cryptobam: dma@8e04000 {
+			status = "ok";
+		};
+
+		crypto@8e3a000 {
+			status = "ok";
+		};
+
+		watchdog@b017000 {
+			status = "ok";
+		};
+	};
+};
