From a4077ce5871304f8a78f80b74b18b6052a410f1a Mon Sep 17 00:00:00 2001
From: "Andrey Jr. Melnikov" <temnota.am@gmail.com>
Date: Thu, 8 Dec 2016 19:57:08 +0300
Subject: [PATCH] mtd: nand: Add Winbond manufacturer id

Add WINBOND manufacturer id.

Signed-off-by: Andrey Jr. Melnikov <temnota.am@gmail.com>
Signed-off-by: Boris Brezillon <boris.brezillon@free-electrons.com>
---
 drivers/mtd/nand/nand_ids.c | 1 +
 include/linux/mtd/nand.h    | 1 +
 2 files changed, 2 insertions(+)

--- a/drivers/mtd/nand/nand_ids.c
+++ b/drivers/mtd/nand/nand_ids.c
@@ -181,6 +181,7 @@ struct nand_manufacturers nand_manuf_ids
 	{NAND_MFR_SANDISK, "SanDisk"},
 	{NAND_MFR_INTEL, "Intel"},
 	{NAND_MFR_ATO, "ATO"},
+	{NAND_MFR_WINBOND, "Winbond"},
 	{0x0, "Unknown"}
 };
 
--- a/include/linux/mtd/nand.h
+++ b/include/linux/mtd/nand.h
@@ -736,6 +736,7 @@ struct nand_chip {
 #define NAND_MFR_SANDISK	0x45
 #define NAND_MFR_INTEL		0x89
 #define NAND_MFR_ATO		0x9b
+#define NAND_MFR_WINBOND	0xef
 
 /* The maximum expected count of bytes in the NAND ID sequence */
 #define NAND_MAX_ID_LEN 8
