From a501a14e38cc4d8e9c91bb508cdca7032d53f717 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Fri, 30 Sep 2016 10:05:32 +0200
Subject: clk: sunxi-ng: Rename the internal structures

Rename the structures meant to be embedded in other structures to make it
consistent with the mux structure name

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
Acked-by: Chen-Yu Tsai <wens@csie.org>
---
 drivers/clk/sunxi-ng/ccu_div.h  |  6 +++---
 drivers/clk/sunxi-ng/ccu_frac.c | 12 ++++++------
 drivers/clk/sunxi-ng/ccu_frac.h | 14 +++++++-------
 drivers/clk/sunxi-ng/ccu_mp.h   |  4 ++--
 drivers/clk/sunxi-ng/ccu_mult.h |  4 ++--
 drivers/clk/sunxi-ng/ccu_nk.h   |  4 ++--
 drivers/clk/sunxi-ng/ccu_nkm.h  |  6 +++---
 drivers/clk/sunxi-ng/ccu_nkmp.h |  8 ++++----
 drivers/clk/sunxi-ng/ccu_nm.h   |  6 +++---
 9 files changed, 32 insertions(+), 32 deletions(-)

--- a/drivers/clk/sunxi-ng/ccu_div.h
+++ b/drivers/clk/sunxi-ng/ccu_div.h
@@ -20,7 +20,7 @@
 #include "ccu_mux.h"
 
 /**
- * struct _ccu_div - Internal divider description
+ * struct ccu_div_internal - Internal divider description
  * @shift: Bit offset of the divider in its register
  * @width: Width of the divider field in its register
  * @max: Maximum value allowed for that divider. This is the
@@ -36,7 +36,7 @@
  * It is basically a wrapper around the clk_divider functions
  * arguments.
  */
-struct _ccu_div {
+struct ccu_div_internal {
 	u8			shift;
 	u8			width;
 
@@ -78,7 +78,7 @@ struct _ccu_div {
 struct ccu_div {
 	u32			enable;
 
-	struct _ccu_div		div;
+	struct ccu_div_internal		div;
 	struct ccu_mux_internal	mux;
 	struct ccu_common	common;
 };
--- a/drivers/clk/sunxi-ng/ccu_frac.c
+++ b/drivers/clk/sunxi-ng/ccu_frac.c
@@ -14,7 +14,7 @@
 #include "ccu_frac.h"
 
 bool ccu_frac_helper_is_enabled(struct ccu_common *common,
-				struct _ccu_frac *cf)
+				struct ccu_frac_internal *cf)
 {
 	if (!(common->features & CCU_FEATURE_FRACTIONAL))
 		return false;
@@ -23,7 +23,7 @@ bool ccu_frac_helper_is_enabled(struct c
 }
 
 void ccu_frac_helper_enable(struct ccu_common *common,
-			    struct _ccu_frac *cf)
+			    struct ccu_frac_internal *cf)
 {
 	unsigned long flags;
 	u32 reg;
@@ -38,7 +38,7 @@ void ccu_frac_helper_enable(struct ccu_c
 }
 
 void ccu_frac_helper_disable(struct ccu_common *common,
-			     struct _ccu_frac *cf)
+			     struct ccu_frac_internal *cf)
 {
 	unsigned long flags;
 	u32 reg;
@@ -53,7 +53,7 @@ void ccu_frac_helper_disable(struct ccu_
 }
 
 bool ccu_frac_helper_has_rate(struct ccu_common *common,
-			      struct _ccu_frac *cf,
+			      struct ccu_frac_internal *cf,
 			      unsigned long rate)
 {
 	if (!(common->features & CCU_FEATURE_FRACTIONAL))
@@ -63,7 +63,7 @@ bool ccu_frac_helper_has_rate(struct ccu
 }
 
 unsigned long ccu_frac_helper_read_rate(struct ccu_common *common,
-					struct _ccu_frac *cf)
+					struct ccu_frac_internal *cf)
 {
 	u32 reg;
 
@@ -84,7 +84,7 @@ unsigned long ccu_frac_helper_read_rate(
 }
 
 int ccu_frac_helper_set_rate(struct ccu_common *common,
-			     struct _ccu_frac *cf,
+			     struct ccu_frac_internal *cf,
 			     unsigned long rate)
 {
 	unsigned long flags;
--- a/drivers/clk/sunxi-ng/ccu_frac.h
+++ b/drivers/clk/sunxi-ng/ccu_frac.h
@@ -18,7 +18,7 @@
 
 #include "ccu_common.h"
 
-struct _ccu_frac {
+struct ccu_frac_internal {
 	u32		enable;
 	u32		select;
 
@@ -33,21 +33,21 @@ struct _ccu_frac {
 	}
 
 bool ccu_frac_helper_is_enabled(struct ccu_common *common,
-				struct _ccu_frac *cf);
+				struct ccu_frac_internal *cf);
 void ccu_frac_helper_enable(struct ccu_common *common,
-			    struct _ccu_frac *cf);
+			    struct ccu_frac_internal *cf);
 void ccu_frac_helper_disable(struct ccu_common *common,
-			     struct _ccu_frac *cf);
+			     struct ccu_frac_internal *cf);
 
 bool ccu_frac_helper_has_rate(struct ccu_common *common,
-			      struct _ccu_frac *cf,
+			      struct ccu_frac_internal *cf,
 			      unsigned long rate);
 
 unsigned long ccu_frac_helper_read_rate(struct ccu_common *common,
-					struct _ccu_frac *cf);
+					struct ccu_frac_internal *cf);
 
 int ccu_frac_helper_set_rate(struct ccu_common *common,
-			     struct _ccu_frac *cf,
+			     struct ccu_frac_internal *cf,
 			     unsigned long rate);
 
 #endif /* _CCU_FRAC_H_ */
--- a/drivers/clk/sunxi-ng/ccu_mp.h
+++ b/drivers/clk/sunxi-ng/ccu_mp.h
@@ -29,8 +29,8 @@
 struct ccu_mp {
 	u32			enable;
 
-	struct _ccu_div		m;
-	struct _ccu_div		p;
+	struct ccu_div_internal		m;
+	struct ccu_div_internal		p;
 	struct ccu_mux_internal	mux;
 	struct ccu_common	common;
 };
--- a/drivers/clk/sunxi-ng/ccu_mult.h
+++ b/drivers/clk/sunxi-ng/ccu_mult.h
@@ -4,7 +4,7 @@
 #include "ccu_common.h"
 #include "ccu_mux.h"
 
-struct _ccu_mult {
+struct ccu_mult_internal {
 	u8	shift;
 	u8	width;
 };
@@ -18,7 +18,7 @@ struct _ccu_mult {
 struct ccu_mult {
 	u32			enable;
 
-	struct _ccu_mult	mult;
+	struct ccu_mult_internal	mult;
 	struct ccu_mux_internal	mux;
 	struct ccu_common	common;
 };
--- a/drivers/clk/sunxi-ng/ccu_nk.h
+++ b/drivers/clk/sunxi-ng/ccu_nk.h
@@ -30,8 +30,8 @@ struct ccu_nk {
 	u32			enable;
 	u32			lock;
 
-	struct _ccu_mult	n;
-	struct _ccu_mult	k;
+	struct ccu_mult_internal	n;
+	struct ccu_mult_internal	k;
 
 	unsigned int		fixed_post_div;
 
--- a/drivers/clk/sunxi-ng/ccu_nkm.h
+++ b/drivers/clk/sunxi-ng/ccu_nkm.h
@@ -29,9 +29,9 @@ struct ccu_nkm {
 	u32			enable;
 	u32			lock;
 
-	struct _ccu_mult	n;
-	struct _ccu_mult	k;
-	struct _ccu_div		m;
+	struct ccu_mult_internal	n;
+	struct ccu_mult_internal	k;
+	struct ccu_div_internal		m;
 	struct ccu_mux_internal	mux;
 
 	struct ccu_common	common;
--- a/drivers/clk/sunxi-ng/ccu_nkmp.h
+++ b/drivers/clk/sunxi-ng/ccu_nkmp.h
@@ -29,10 +29,10 @@ struct ccu_nkmp {
 	u32			enable;
 	u32			lock;
 
-	struct _ccu_mult	n;
-	struct _ccu_mult	k;
-	struct _ccu_div		m;
-	struct _ccu_div		p;
+	struct ccu_mult_internal	n;
+	struct ccu_mult_internal	k;
+	struct ccu_div_internal		m;
+	struct ccu_div_internal		p;
 
 	struct ccu_common	common;
 };
--- a/drivers/clk/sunxi-ng/ccu_nm.h
+++ b/drivers/clk/sunxi-ng/ccu_nm.h
@@ -30,9 +30,9 @@ struct ccu_nm {
 	u32			enable;
 	u32			lock;
 
-	struct _ccu_mult	n;
-	struct _ccu_div		m;
-	struct _ccu_frac	frac;
+	struct ccu_mult_internal	n;
+	struct ccu_div_internal		m;
+	struct ccu_frac_internal	frac;
 
 	struct ccu_common	common;
 };
