--- a/drivers/pinctrl/Kconfig
+++ b/drivers/pinctrl/Kconfig
@@ -228,6 +228,15 @@ config PINCTRL_COH901
 	  COH 901 335 and COH 901 571/3. They contain 3, 5 or 7
 	  ports of 8 GPIO pins each.
 
+config PINCTRL_OXNAS
+	bool "OXNAS pinctrl driver"
+	depends on OF
+	depends on ARCH_OXNAS
+	select PINMUX
+	select PINCONF
+	help
+	  Say Y here to enable the oxnas pinctrl driver
+
 config PINCTRL_PALMAS
 	bool "Pinctrl driver for the PALMAS Series MFD devices"
 	depends on OF && MFD_PALMAS
--- a/drivers/pinctrl/Makefile
+++ b/drivers/pinctrl/Makefile
@@ -17,6 +17,7 @@ obj-$(CONFIG_PINCTRL_AMD)	+= pinctrl-amd
 obj-$(CONFIG_PINCTRL_DIGICOLOR)	+= pinctrl-digicolor.o
 obj-$(CONFIG_PINCTRL_FALCON)	+= pinctrl-falcon.o
 obj-$(CONFIG_PINCTRL_MESON)	+= meson/
+obj-$(CONFIG_PINCTRL_OXNAS)	+= pinctrl-oxnas.o
 obj-$(CONFIG_PINCTRL_PALMAS)	+= pinctrl-palmas.o
 obj-$(CONFIG_PINCTRL_PISTACHIO)	+= pinctrl-pistachio.o
 obj-$(CONFIG_PINCTRL_ROCKCHIP)	+= pinctrl-rockchip.o
