From: Russell King <rmk+kernel@arm.linux.org.uk>
Date: Fri, 16 Oct 2015 12:18:41 +0100
Subject: [PATCH] phy: export phy_start_machine() for phylink

phylink will need phy_start_machine exported, so lets export it as a
GPL symbol.  Documentation/networking/phy.txt indicates that this
should be a PHY API function.

Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Russell King <rmk+kernel@arm.linux.org.uk>
---

--- a/drivers/net/phy/phy.c
+++ b/drivers/net/phy/phy.c
@@ -612,6 +612,7 @@ void phy_start_machine(struct phy_device
 {
 	queue_delayed_work(system_power_efficient_wq, &phydev->state_queue, HZ);
 }
+EXPORT_SYMBOL_GPL(phy_start_machine);
 
 /**
  * phy_trigger_machine - trigger the state machine to run
