/*
 * Device Tree file for the Edimax BR-6478AC V2
 * based on Linksys E1700
 *
 * Copyright (C) 2016 Rohan Murch <rohan.murch@gmail.com>
 * Copyright (C) 2016 Hans Ulli Kroll <ulli.kroll@googlemail.com>
 * Copyright (C) 2017 James McKenzie <openwrt@madingley.org>
 *
 * This file is licensed under the terms of the GNU General Public
 * License version 2.  This program is licensed "as is" without any
 * warranty of any kind, whether express or implied.
 */

/dts-v1/;

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "edimax,br-6478ac-v2", "ralink,mt7620a-soc";
	model = "Edimax BR-6478AC v2";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset_wps {
			label = "reset_wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "br-6478ac-v2:white:power";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};
		internet {
			label = "br-6478ac-v2:blue:internet";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};
		wlan {
			label = "br-6478ac-v2:blue:wlan";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};
		usb {
			label = "br-6478ac-v2:blue:usb";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};
	};


	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;
		usb-power {
			gpio-export,name="usb-power";
			gpio-export,output=<1>;
			gpios = <&gpio2 5 GPIO_ACTIVE_HIGH>;
		};
	};
};


&gpio2 {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0 0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "cimage";
				reg = <0x50000 0x20000>;
				read-only;
			};

			partition@70000 {
				label = "firmware";
				reg = <0x00070000 0x00790000>;
			};
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "uartf", "nd_sd";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x4>;
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii1_pins &rgmii2_pins &mdio_pins>;
	mediatek,portmap = "wllll";

	port@5 {
		status = "okay";
		mediatek,fixed-link = <1000 1 1 1>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			reg = <0>;
			phy-mode = "rgmii";
		};

		phy1: ethernet-phy@1 {
			reg = <1>;
			phy-mode = "rgmii";
		};

		phy2: ethernet-phy@2 {
			reg = <2>;
			phy-mode = "rgmii";
		};

		phy3: ethernet-phy@3 {
			reg = <3>;
			phy-mode = "rgmii";
		};

		phy4: ethernet-phy@4 {
			reg = <4>;
			phy-mode = "rgmii";
		};

		phy1f: ethernet-phy@1f {
			reg = <0x1f>;
			phy-mode = "rgmii";
		};
	};
};

&gsw {
	mediatek,port4 = "gmac";
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		mediatek,2ghz = <0>;
	};
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};
