--- a/drivers/net/ethernet/dec/tulip/Kconfig
+++ b/drivers/net/ethernet/dec/tulip/Kconfig
@@ -60,6 +60,14 @@ config TULIP_PCI
 	  To compile this driver as a module, choose M here. The module will
 	  be called tulip.
 
+config TULIP_PLATFORM
+	tristate "DECchip Tulip (dc2114x) Platform support"
+	depends on HAS_IOMEM
+	select TULIP
+	select CRC32
+	---help---
+	   This driver is for the platform variant.
+
 config TULIP_MWI
 	bool "New bus configuration (EXPERIMENTAL)"
 	depends on TULIP_PCI && EXPERIMENTAL
--- a/drivers/net/ethernet/dec/tulip/tulip_core.c
+++ b/drivers/net/ethernet/dec/tulip/tulip_core.c
@@ -27,6 +27,8 @@
 #include <linux/init.h>
 #include <linux/interrupt.h>
 #include <linux/etherdevice.h>
+#include <linux/platform_device.h>
+#include <linux/platform_data/tulip.h>
 #include <linux/delay.h>
 #include <linux/mii.h>
 #include <linux/crc32.h>
@@ -204,6 +206,9 @@ struct tulip_chip_table tulip_tbl[] = {
   { "Conexant LANfinity", 256, 0x0001ebef,
 	HAS_MII | HAS_ACPI, tulip_timer, tulip_media_task },
 
+  { "Infineon ADM8668", 256, 0x0001a451,
+	MC_HASH_ONLY | COMET_MAC_ADDR, tulip_timer, tulip_media_task, },
+
 };
 
 #ifdef CONFIG_TULIP_PCI
@@ -395,6 +400,7 @@ static void tulip_up(struct net_device *
 	i = 0;
 	if (tp->mtable == NULL)
 		goto media_picked;
+
 	if (dev->if_port) {
 		int looking_for = tulip_media_cap[dev->if_port] & MediaIsMII ? 11 :
 			(dev->if_port == 12 ? 0 : dev->if_port);
@@ -488,6 +494,10 @@ media_picked:
 		iowrite32(ioread32(ioaddr + 0x88) | 1, ioaddr + 0x88);
 		dev->if_port = tp->mii_cnt ? 11 : 0;
 		tp->csr6 = 0x00040000;
+	} else if (tp->chip_id == ADM8668) {
+		/* Enable automatic Tx underrun recovery. */
+		iowrite32(ioread32(ioaddr + 0x88) | 1, ioaddr + 0x88);
+		tp->csr6 = 0x00040000;
 	} else if (tp->chip_id == AX88140) {
 		tp->csr6 = tp->mii_cnt ? 0x00040100 : 0x00000100;
 	} else
@@ -657,6 +667,10 @@ static void tulip_init_ring(struct net_d
 		mapping = pci_map_single(tp->pdev, skb->data,
 					 PKT_BUF_SZ, PCI_DMA_FROMDEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+		mapping = dma_map_single(&tp->pldev->dev, skb->data,
+					PKT_BUF_SZ, DMA_FROM_DEVICE);
+#endif
 		tp->rx_buffers[i].mapping = mapping;
 		skb->dev = dev;			/* Mark as being used by this device. */
 		tp->rx_ring[i].status = cpu_to_le32(DescOwned);	/* Owned by Tulip chip */
@@ -694,6 +708,11 @@ tulip_start_xmit(struct sk_buff *skb, st
 	mapping = pci_map_single(tp->pdev, skb->data,
 				 skb->len, PCI_DMA_TODEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+	mapping = dma_map_single(&tp->pldev->dev, skb->data,
+				 skb->len,
+				 DMA_TO_DEVICE);
+#endif
 	tp->tx_buffers[entry].mapping = mapping;
 	tp->tx_ring[entry].buffer1 = cpu_to_le32(mapping);
 
@@ -757,6 +776,11 @@ static void tulip_clean_tx_ring(struct t
 				tp->tx_buffers[entry].skb->len,
 				PCI_DMA_TODEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+		dma_unmap_single(&tp->pldev->dev, tp->tx_buffers[entry].mapping,
+				tp->tx_buffers[entry].skb->len,
+				DMA_TO_DEVICE);
+#endif
 
 		/* Free the original skb. */
 		dev_kfree_skb_irq(tp->tx_buffers[entry].skb);
@@ -834,6 +858,10 @@ static void tulip_free_ring (struct net_
 			pci_unmap_single(tp->pdev, mapping, PKT_BUF_SZ,
 					 PCI_DMA_FROMDEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+			dma_unmap_single(&tp->pldev->dev, mapping, PKT_BUF_SZ,
+					DMA_FROM_DEVICE);
+#endif
 			dev_kfree_skb (skb);
 		}
 	}
@@ -846,6 +874,10 @@ static void tulip_free_ring (struct net_
 			pci_unmap_single(tp->pdev, tp->tx_buffers[i].mapping,
 					 skb->len, PCI_DMA_TODEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+			dma_unmap_single(&tp->pldev->dev, tp->tx_buffers[i].mapping,
+					 skb->len, DMA_TO_DEVICE);
+#endif
 			dev_kfree_skb (skb);
 		}
 		tp->tx_buffers[i].skb = NULL;
@@ -900,6 +932,9 @@ static void tulip_get_drvinfo(struct net
 #ifdef CONFIG_TULIP_PCI
 	strlcpy(info->bus_info, pci_name(np->pdev), sizeof(info->bus_info));
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+	strlcpy(info->bus_info, "platform", sizeof(info->bus_info));
+#endif
 }
 
 
@@ -915,6 +950,9 @@ static int tulip_ethtool_set_wol(struct
 #ifdef CONFIG_TULIP_PCI
 	device_set_wakeup_enable(&tp->pdev->dev, tp->wolinfo.wolopts);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+	device_set_wakeup_enable(&tp->pldev->dev, tp->wolinfo.wolopts);
+#endif
 	return 0;
 }
 
@@ -1193,9 +1231,9 @@ static void set_rx_mode(struct net_devic
 
 			}
 
+#ifdef CONFIG_TULIP_PCI
 			tp->tx_buffers[entry].skb = NULL;
 			tp->tx_buffers[entry].mapping =
-#ifdef CONFIG_TULIP_PCI
 				pci_map_single(tp->pdev, tp->setup_frame,
 					       sizeof(tp->setup_frame),
 					       PCI_DMA_TODEVICE);
@@ -1219,6 +1257,9 @@ static void set_rx_mode(struct net_devic
 		spin_unlock_irqrestore(&tp->lock, flags);
 	}
 
+	if (tp->chip_id == ADM8668)
+		csr6 |= (1 << 9);	/* force 100Mbps full duplex */
+
 	iowrite32(csr6, ioaddr + CSR6);
 }
 
@@ -1991,6 +2032,124 @@ static void __devexit tulip_remove_one (
 }
 #endif /* CONFIG_TULIP_PCI */
 
+#ifdef CONFIG_TULIP_PLATFORM
+static int __devinit tulip_probe(struct platform_device *pdev)
+{
+	struct tulip_private *tp;
+	struct tulip_platform_data *pdata;
+	struct net_device *dev;
+	struct resource *res;
+	void __iomem *ioaddr;
+	int irq;
+
+	if (pdev->id < 0 || pdev->id >= MAX_UNITS)
+		return -EINVAL;
+
+	if (!(res = platform_get_resource(pdev, IORESOURCE_IRQ, 0)))
+		return -ENODEV;
+	irq = res->start;
+	if (!(res = platform_get_resource(pdev, IORESOURCE_MEM, 0)))
+		return -ENODEV;
+	if (!(ioaddr = ioremap(res->start, res->end - res->start)))
+		return -ENODEV;
+
+	pdata = pdev->dev.platform_data;
+	if (!pdata)
+		return -ENODEV;
+
+	if (!(dev = alloc_etherdev(sizeof (*tp))))
+		return -ENOMEM;
+
+	/* setup net dev */
+	dev->base_addr = (unsigned long)res->start;
+	dev->irq = irq;
+	SET_NETDEV_DEV(dev, &pdev->dev);
+
+	/* tulip private struct */
+	tp = netdev_priv(dev);
+	tp->dev = dev;
+	tp->base_addr = ioaddr;
+	tp->csr0 = 0;
+	tp->pldev = pdev;
+	tp->rx_ring = dma_alloc_coherent(&pdev->dev,
+				sizeof(struct tulip_rx_desc) * RX_RING_SIZE +
+				sizeof(struct tulip_tx_desc) * TX_RING_SIZE,
+				&tp->rx_ring_dma, GFP_KERNEL);
+	if (!tp->rx_ring)
+		return -ENODEV;
+	tp->tx_ring = (struct tulip_tx_desc *)(tp->rx_ring + RX_RING_SIZE);
+	tp->tx_ring_dma = tp->rx_ring_dma + sizeof(struct tulip_rx_desc) * RX_RING_SIZE;
+
+	tp->chip_id = pdata->chip_id;
+	tp->flags = tulip_tbl[tp->chip_id].flags;
+
+	spin_lock_init(&tp->lock);
+	spin_lock_init(&tp->mii_lock);
+
+	init_timer(&tp->timer);
+	tp->timer.data = (unsigned long)dev;
+	tp->timer.function = tulip_tbl[tp->chip_id].media_timer;
+
+	INIT_WORK(&tp->media_work, tulip_tbl[tp->chip_id].media_task);
+
+	/* Stop the chip's Tx and Rx processes. */
+	tulip_stop_rxtx(tp);
+
+	/* Clear the missed-packet counter. */
+	ioread32(ioaddr + CSR8);
+
+	if (!is_valid_ether_addr(pdata->mac)) {
+		dev_info(&pdev->dev, "generating random ethernet MAC\n");
+		random_ether_addr(dev->dev_addr);
+	} else
+		memcpy(dev->dev_addr, pdata->mac, ETH_ALEN);
+
+	/* The Tulip-specific entries in the device structure. */
+	dev->netdev_ops = &tulip_netdev_ops;
+	dev->watchdog_timeo = TX_TIMEOUT;
+	netif_napi_add(dev, &tp->napi, tulip_poll, 16);
+	SET_ETHTOOL_OPS(dev, &ops);
+
+	if (register_netdev(dev))
+		goto err_out_free_ring;
+
+	dev_info(&dev->dev,
+		 "tulip_platform (%s) at MMIO %#lx %pM, IRQ %d\n",
+		 tulip_tbl[tp->chip_id].chip_name,
+		 (unsigned long)dev->base_addr, dev->dev_addr, irq);
+
+	platform_set_drvdata(pdev, dev);
+	return 0;
+
+err_out_free_ring:
+	dma_free_coherent(&pdev->dev,
+		     sizeof (struct tulip_rx_desc) * RX_RING_SIZE +
+		     sizeof (struct tulip_tx_desc) * TX_RING_SIZE,
+		     tp->rx_ring, tp->rx_ring_dma);
+	return -ENODEV;
+}
+
+static int __devexit tulip_remove(struct platform_device *pdev)
+{
+	struct net_device *dev = platform_get_drvdata (pdev);
+	struct tulip_private *tp;
+
+	if (!dev)
+		return -ENODEV;
+
+	tp = netdev_priv(dev);
+	unregister_netdev(dev);
+	dma_free_coherent(&pdev->dev,
+			     sizeof (struct tulip_rx_desc) * RX_RING_SIZE +
+			     sizeof (struct tulip_tx_desc) * TX_RING_SIZE,
+			     tp->rx_ring, tp->rx_ring_dma);
+	iounmap(tp->base_addr);
+	free_netdev(dev);
+	platform_set_drvdata(pdev, NULL);
+	return 0;
+}
+#endif
+
 #ifdef CONFIG_NET_POLL_CONTROLLER
 /*
  * Polling 'interrupt' - used by things like netconsole to send skbs
@@ -2021,6 +2180,17 @@ static struct pci_driver tulip_pci_drive
 };
 #endif
 
+#ifdef CONFIG_TULIP_PLATFORM
+static struct platform_driver tulip_platform_driver = {
+	.probe = tulip_probe,
+	.remove = __devexit_p(tulip_remove),
+	.driver = {
+		.owner = THIS_MODULE,
+		.name = DRV_NAME,
+	},
+};
+#endif
+
 
 static int __init tulip_init (void)
 {
@@ -2037,6 +2207,9 @@ static int __init tulip_init (void)
 #ifdef CONFIG_TULIP_PCI
 	ret = pci_register_driver(&tulip_pci_driver);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+	ret = platform_driver_register(&tulip_platform_driver);
+#endif
 	return ret;
 }
 
@@ -2046,6 +2219,9 @@ static void __exit tulip_cleanup (void)
 #ifdef CONFIG_TULIP_PCI
 	pci_unregister_driver (&tulip_pci_driver);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+	platform_driver_unregister (&tulip_platform_driver);
+#endif
 }
 
 
--- a/drivers/net/ethernet/dec/tulip/tulip.h
+++ b/drivers/net/ethernet/dec/tulip/tulip.h
@@ -21,6 +21,8 @@
 #include <linux/timer.h>
 #include <linux/delay.h>
 #include <linux/pci.h>
+#include <linux/platform_device.h>
+#include <linux/platform_data/tulip.h>
 #include <asm/io.h>
 #include <asm/irq.h>
 #include <asm/unaligned.h>
@@ -69,28 +71,6 @@ enum tbl_flag {
 };
 
 
-/* chip types.  careful!  order is VERY IMPORTANT here, as these
- * are used throughout the driver as indices into arrays */
-/* Note 21142 == 21143. */
-enum chips {
-	DC21040 = 0,
-	DC21041 = 1,
-	DC21140 = 2,
-	DC21142 = 3, DC21143 = 3,
-	LC82C168,
-	MX98713,
-	MX98715,
-	MX98725,
-	AX88140,
-	PNIC2,
-	COMET,
-	COMPEX9881,
-	I21145,
-	DM910X,
-	CONEXANT,
-};
-
-
 enum MediaIs {
 	MediaIsFD = 1,
 	MediaAlwaysFD = 2,
@@ -446,7 +426,12 @@ struct tulip_private {
 	struct mediatable *mtable;
 	int cur_index;		/* Current media index. */
 	int saved_if_port;
+#ifdef CONFIG_TULIP_PCI
 	struct pci_dev *pdev;
+#endif
+#ifdef CONFIG_TULIP_PLATFORM
+	struct platform_device *pldev;
+#endif
 	int ttimer;
 	int susp_rx;
 	unsigned long nir;
--- a/drivers/net/ethernet/dec/tulip/interrupt.c
+++ b/drivers/net/ethernet/dec/tulip/interrupt.c
@@ -76,6 +76,10 @@ int tulip_refill_rx(struct net_device *d
 			mapping = pci_map_single(tp->pdev, skb->data, PKT_BUF_SZ,
 						 PCI_DMA_FROMDEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+			mapping = dma_map_single(&tp->pldev->dev, skb->data, PKT_BUF_SZ,
+						 DMA_FROM_DEVICE);
+#endif
 			tp->rx_buffers[entry].mapping = mapping;
 
 			skb->dev = dev;			/* Mark as being used by this device. */
@@ -198,8 +202,7 @@ int tulip_poll(struct napi_struct *napi,
 						dev->stats.rx_fifo_errors++;
                                }
                        } else {
-                               struct sk_buff *skb;
-
+				struct sk_buff *skb;
                                /* Check if the packet is long enough to accept without copying
                                   to a minimally-sized skbuff. */
                                if (pkt_len < tulip_rx_copybreak &&
@@ -242,6 +245,10 @@ int tulip_poll(struct napi_struct *napi,
                                        pci_unmap_single(tp->pdev, tp->rx_buffers[entry].mapping,
                                                         PKT_BUF_SZ, PCI_DMA_FROMDEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+				       dma_unmap_single(&tp->pldev->dev, tp->rx_buffers[entry].mapping,
+						       PKT_BUF_SZ, DMA_FROM_DEVICE);
+#endif
 
                                        tp->rx_buffers[entry].skb = NULL;
                                        tp->rx_buffers[entry].mapping = 0;
@@ -635,6 +642,11 @@ irqreturn_t tulip_interrupt(int irq, voi
 						 tp->tx_buffers[entry].skb->len,
 						 PCI_DMA_TODEVICE);
 #endif
+#ifdef CONFIG_TULIP_PLATFORM
+				dma_unmap_single(&tp->pldev->dev, tp->tx_buffers[entry].mapping,
+						 tp->tx_buffers[entry].skb->len,
+						 DMA_TO_DEVICE);
+#endif
 
 				/* Free the original skb. */
 				dev_kfree_skb_irq(tp->tx_buffers[entry].skb);
--- /dev/null
+++ b/include/linux/platform_data/tulip.h
@@ -0,0 +1,31 @@
+#ifndef _LINUX_TULIP_PDATA_H
+#define _LINUX_TULIP_PDATA_H
+
+/* chip types.  careful!  order is VERY IMPORTANT here, as these
+ * are used throughout the driver as indices into arrays */
+/* Note 21142 == 21143. */
+enum chips {
+	DC21040 = 0,
+	DC21041 = 1,
+	DC21140 = 2,
+	DC21142 = 3, DC21143 = 3,
+	LC82C168,
+	MX98713,
+	MX98715,
+	MX98725,
+	AX88140,
+	PNIC2,
+	COMET,
+	COMPEX9881,
+	I21145,
+	DM910X,
+	CONEXANT,
+	ADM8668,
+};
+
+struct tulip_platform_data {
+	u8		mac[6];
+	enum chips	chip_id;
+};
+
+#endif
