--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -17,6 +17,7 @@
 #include <linux/spi/spi.h>
 #include <linux/spi/spi_gpio.h>
 #include <linux/spi/74x164.h>
+#include <linux/rtl8367.h>
 #include <asm/addrspace.h>
 #include <bcm63xx_board.h>
 #include <bcm63xx_cpu.h>
@@ -56,6 +57,8 @@
 #define NB4_SPI_GPIO_MOSI	7
 #define NB4_SPI_GPIO_CLK	6
 #define NB4_74HC64_GPIO(X)	(NB4_74X164_GPIO_BASE + (X))
+#define NB6_GPIO_RTL8367_SDA	18
+#define NB6_GPIO_RTL8367_SCK	20
 
 #define CT6373_PID_OFFSET		0xff80
 #define CT6373_74X164_GPIO_BASE	64
@@ -2665,6 +2668,103 @@ static struct board_info __initdata boar
 };
 #endif
 
+#ifdef CONFIG_BCM63XX_CPU_6362
+static struct rtl8367_extif_config nb6_rtl8367_extif0_cfg = {
+	.mode = RTL8367_EXTIF_MODE_RGMII,
+	.txdelay = 1,
+	.rxdelay = 5,
+	.ability = {
+		.force_mode = 1,
+		.txpause = 1,
+		.rxpause = 1,
+		.link = 1,
+		.duplex = 1,
+		.speed = RTL8367_PORT_SPEED_1000,
+	},
+};
+
+static struct rtl8367_platform_data nb6_rtl8367_data = {
+	.gpio_sda	= NB6_GPIO_RTL8367_SDA,
+	.gpio_sck	= NB6_GPIO_RTL8367_SCK,
+	.extif0_cfg	= &nb6_rtl8367_extif0_cfg,
+};
+
+static struct platform_device nb6_rtl8367_device = {
+	.name		= RTL8367_DRIVER_NAME,
+	.id		= -1,
+	.dev = {
+		.platform_data	= &nb6_rtl8367_data,
+	}
+};
+
+static struct platform_device * __initdata nb6_devices[] = {
+	&nb6_rtl8367_device,
+};
+
+static struct board_info __initdata board_nb6 = {
+	.name				= "NB6",
+	.expected_cpu_id		= 0x6362,
+
+	.has_uart0			= 1,
+
+	.has_ohci0			= 1,
+	.has_ehci0			= 1,
+
+	.has_enetsw			= 1,
+
+	.enetsw = {
+		.used_ports = {
+			[4] = {
+				.used	= 1,
+				.phy_id	= 0xff,
+				.bypass_link = 1,
+				.force_speed = 1000,
+				.force_duplex_full = 1,
+				.name	= "RGMII",
+			},
+		},
+	},
+
+	.buttons = {
+		{
+			.desc		= "reset",
+			.gpio		= 24,
+			.type		= EV_KEY,
+			.code		= KEY_RESTART,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+			.active_low	= 1,
+		},
+		{
+			.desc		= "wps",
+			.gpio		= 25,
+			.type		= EV_KEY,
+			.code		= KEY_WPS_BUTTON,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+			.active_low	= 1,
+		},
+		{
+			.desc		= "wlan",
+			.gpio		= 12,
+			.type		= EV_KEY,
+			.code		= KEY_WLAN,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+			.active_low	= 1,
+		},
+		{
+			.desc		= "service",
+			.gpio		= 10,
+			.type		= EV_KEY,
+			.code		= BTN_0,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+			.active_low	= 1,
+		},
+	},
+
+	.devs = nb6_devices,
+	.num_devs = ARRAY_SIZE(nb6_devices),
+};
+#endif
+
 /*
  * known 6368 boards
  */
@@ -2864,6 +2964,10 @@ static const struct board_info __initcon
 	&board_DVAG3810BN,
 #endif
 
+#ifdef CONFIG_BCM63XX_CPU_6362
+	&board_nb6,
+#endif
+
 #ifdef CONFIG_BCM63XX_CPU_6368
 	&board_96368mvwg,
 	&board_96368mvngr,
@@ -2931,6 +3035,11 @@ static void __init boardid_fixup(u8 *boo
 		}
 	}
 
+	if (BCMCPU_IS_6362() && (!strncmp(board_name, "NB6-", sizeof("NB6-") - 1))) {
+		board_name[sizeof("NB6") - 1] = '\0';
+		return ;
+	}
+
 	/* check if bcm_tag is at 64k offset */
 	if (strncmp(board_name, tag->board_id, BOARDID_LEN) != 0) {
 		/* else try 128k */
