Now that we have DT bindings to specify which devices should not
be reset and idled during init, make hwmod extract the information
(and store them in internal flags) from Device tree.

Signed-off-by: Rajendra Nayak <rnayak@ti.com>

---
arch/arm/mach-omap2/omap_hwmod.c |   23 ++++++++++++++++-------
 1 file changed, 16 insertions(+), 7 deletions(-)

--- a/arch/arm/mach-omap2/omap_hwmod.c
+++ b/arch/arm/mach-omap2/omap_hwmod.c
@@ -2363,11 +2363,11 @@ static struct device_node *of_dev_hwmod_
  * are part of the device's address space can be ioremapped properly.
  * No return value.
  */
-static void __init _init_mpu_rt_base(struct omap_hwmod *oh, void *data)
+static void __init _init_mpu_rt_base(struct omap_hwmod *oh, void *data,
+				     struct device_node *np)
 {
 	struct omap_hwmod_addr_space *mem;
 	void __iomem *va_start = NULL;
-	struct device_node *np;
 
 	if (!oh)
 		return;
@@ -2383,12 +2383,10 @@ static void __init _init_mpu_rt_base(str
 			 oh->name);
 
 		/* Extract the IO space from device tree blob */
-		if (!of_have_populated_dt())
+		if (!np)
 			return;
 
-		np = of_dev_hwmod_lookup(of_find_node_by_name(NULL, "ocp"), oh);
-		if (np)
-			va_start = of_iomap(np, oh->mpu_rt_idx);
+		va_start = of_iomap(np, oh->mpu_rt_idx);
 	} else {
 		va_start = ioremap(mem->pa_start, mem->pa_end - mem->pa_start);
 	}
@@ -2420,12 +2418,16 @@ static void __init _init_mpu_rt_base(str
 static int __init _init(struct omap_hwmod *oh, void *data)
 {
 	int r;
+	struct device_node *np = NULL;
 
 	if (oh->_state != _HWMOD_STATE_REGISTERED)
 		return 0;
 
+	if (of_have_populated_dt())
+		np = of_dev_hwmod_lookup(of_find_node_by_name(NULL, "ocp"), oh);
+
 	if (oh->class->sysc)
-		_init_mpu_rt_base(oh, NULL);
+		_init_mpu_rt_base(oh, NULL, np);
 
 	r = _init_clocks(oh, NULL);
 	if (r < 0) {
@@ -2433,6 +2435,13 @@ static int __init _init(struct omap_hwmo
 		return -EINVAL;
 	}
 
+	if (np) {
+		if (of_find_property(np, "ti,no-reset-on-init", NULL))
+			oh->flags |= HWMOD_INIT_NO_RESET;
+		if (of_find_property(np, "ti,no-idle-on-init", NULL))
+			oh->flags |= HWMOD_INIT_NO_IDLE;
+	}
+
 	oh->_state = _HWMOD_STATE_INITIALIZED;
 
 	return 0;
