From 6bf236bb67dfabd0434df47ff1247b1310d4ccf5 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Tue, 24 Sep 2013 11:09:55 +0300
Subject: [PATCH] ARM: sunxi: Select ARCH_HAS_RESET_CONTROLLER

The A31 has a reset controller, and we have to select this option to
have access to the reset controller framework.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/mach-sunxi/Kconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm/mach-sunxi/Kconfig b/arch/arm/mach-sunxi/Kconfig
index bce0d42..547004c 100644
--- a/arch/arm/mach-sunxi/Kconfig
+++ b/arch/arm/mach-sunxi/Kconfig
@@ -1,5 +1,6 @@
 config ARCH_SUNXI
 	bool "Allwinner A1X SOCs" if ARCH_MULTI_V7
+	select ARCH_HAS_RESET_CONTROLLER
 	select ARCH_REQUIRE_GPIOLIB
 	select ARM_GIC
 	select CLKSRC_MMIO
-- 
1.8.4

