From 1a1769d6268c93b042f635b31b43024fea7feb30 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Thu, 25 Apr 2013 00:31:29 +0200
Subject: [PATCH 08/14] MIPS: BCM63XX: populate irq_{stat,mask}_addr for
 second pin

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/irq.c |   43 ++++++++++++++++++++++++++++++++++++++++++-
 1 file changed, 42 insertions(+), 1 deletion(-)

--- a/arch/mips/bcm63xx/irq.c
+++ b/arch/mips/bcm63xx/irq.c
@@ -30,6 +30,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_3368
 #define irq_stat_reg0		PERF_IRQSTAT_3368_REG
 #define irq_mask_reg0		PERF_IRQMASK_3368_REG
+#define irq_stat_reg1		0
+#define irq_mask_reg1		0
 #define irq_bits		32
 #define is_ext_irq_cascaded	0
 #define ext_irq_start		0
@@ -41,6 +43,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_6328
 #define irq_stat_reg0		PERF_IRQSTAT_6328_REG(0)
 #define irq_mask_reg0		PERF_IRQMASK_6328_REG(0)
+#define irq_stat_reg1		PERF_IRQSTAT_6328_REG(1)
+#define irq_mask_reg1		PERF_IRQMASK_6328_REG(1)
 #define irq_bits		64
 #define is_ext_irq_cascaded	1
 #define ext_irq_start		(BCM_6328_EXT_IRQ0 - IRQ_INTERNAL_BASE)
@@ -52,6 +56,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_6338
 #define irq_stat_reg0		PERF_IRQSTAT_6338_REG
 #define irq_mask_reg0		PERF_IRQMASK_6338_REG
+#define irq_stat_reg1		0
+#define irq_mask_reg1		0
 #define irq_bits		32
 #define is_ext_irq_cascaded	0
 #define ext_irq_start		0
@@ -63,6 +69,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_6345
 #define irq_stat_reg0		PERF_IRQSTAT_6345_REG
 #define irq_mask_reg0		PERF_IRQMASK_6345_REG
+#define irq_stat_reg1		0
+#define irq_mask_reg1		0
 #define irq_bits		32
 #define is_ext_irq_cascaded	0
 #define ext_irq_start		0
@@ -74,6 +82,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_6348
 #define irq_stat_reg0		PERF_IRQSTAT_6348_REG
 #define irq_mask_reg0		PERF_IRQMASK_6348_REG
+#define irq_stat_reg1		0
+#define irq_mask_reg1		0
 #define irq_bits		32
 #define is_ext_irq_cascaded	0
 #define ext_irq_start		0
@@ -85,6 +95,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_6358
 #define irq_stat_reg0		PERF_IRQSTAT_6358_REG(0)
 #define irq_mask_reg0		PERF_IRQMASK_6358_REG(0)
+#define irq_stat_reg1		PERF_IRQSTAT_6358_REG(1)
+#define irq_mask_reg1		PERF_IRQMASK_6358_REG(1)
 #define irq_bits		32
 #define is_ext_irq_cascaded	1
 #define ext_irq_start		(BCM_6358_EXT_IRQ0 - IRQ_INTERNAL_BASE)
@@ -96,6 +108,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_6362
 #define irq_stat_reg0		PERF_IRQSTAT_6362_REG(0)
 #define irq_mask_reg0		PERF_IRQMASK_6362_REG(0)
+#define irq_stat_reg1		PERF_IRQSTAT_6362_REG(1)
+#define irq_mask_reg1		PERF_IRQMASK_6362_REG(1)
 #define irq_bits		64
 #define is_ext_irq_cascaded	1
 #define ext_irq_start		(BCM_6362_EXT_IRQ0 - IRQ_INTERNAL_BASE)
@@ -107,6 +121,8 @@ static void __internal_irq_unmask_64(uns
 #ifdef CONFIG_BCM63XX_CPU_6368
 #define irq_stat_reg0		PERF_IRQSTAT_6368_REG(0)
 #define irq_mask_reg0		PERF_IRQMASK_6368_REG(0)
+#define irq_stat_reg1		PERF_IRQSTAT_6368_REG(1)
+#define irq_mask_reg1		PERF_IRQMASK_6368_REG(1)
 #define irq_bits		64
 #define is_ext_irq_cascaded	1
 #define ext_irq_start		(BCM_6368_EXT_IRQ0 - IRQ_INTERNAL_BASE)
@@ -128,13 +144,20 @@ static void __internal_irq_unmask_64(uns
 
 #define irq_stat_addr0	(bcm63xx_regset_address(RSET_PERF) + irq_stat_reg0)
 #define irq_mask_addr0	(bcm63xx_regset_address(RSET_PERF) + irq_mask_reg0)
+#if (irq_stat_reg1 > 0) && (irq_mask_reg1 > 0)
+#define irq_stat_addr1	(bcm63xx_regset_address(RSET_PERF) + irq_stat_reg1)
+#define irq_mask_addr1	(bcm63xx_regset_address(RSET_PERF) + irq_mask_reg1)
+#else
+#define irq_stat_addr1	0
+#define irq_mask_addr1	0
+#endif
 
 static inline void bcm63xx_init_irq(void)
 {
 }
 #else /* ! BCMCPU_RUNTIME_DETECT */
 
-static u32 irq_stat_addr0, irq_mask_addr0;
+static u32 irq_stat_addr0, irq_mask_addr0, irq_stat_addr1, irq_mask_addr1;
 static void (*dispatch_internal)(void);
 static int is_ext_irq_cascaded;
 static unsigned int ext_irq_count;
@@ -149,11 +172,15 @@ static void bcm63xx_init_irq(void)
 
 	irq_stat_addr0 = bcm63xx_regset_address(RSET_PERF);
 	irq_mask_addr0 = bcm63xx_regset_address(RSET_PERF);
+	irq_stat_addr1 = bcm63xx_regset_address(RSET_PERF);
+	irq_mask_addr1 = bcm63xx_regset_address(RSET_PERF);
 
 	switch (bcm63xx_get_cpu_id()) {
 	case BCM3368_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_3368_REG;
 		irq_mask_addr0 += PERF_IRQMASK_3368_REG;
+		irq_stat_addr1 = 0;
+		irq_stat_addr1 = 0;
 		irq_bits = 32;
 		ext_irq_count = 4;
 		ext_irq_cfg_reg1 = PERF_EXTIRQ_CFG_REG_3368;
@@ -161,6 +188,8 @@ static void bcm63xx_init_irq(void)
 	case BCM6328_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_6328_REG(0);
 		irq_mask_addr0 += PERF_IRQMASK_6328_REG(0);
+		irq_stat_addr1 += PERF_IRQSTAT_6328_REG(1);
+		irq_stat_addr1 += PERF_IRQMASK_6328_REG(1);
 		irq_bits = 64;
 		ext_irq_count = 4;
 		is_ext_irq_cascaded = 1;
@@ -171,6 +200,8 @@ static void bcm63xx_init_irq(void)
 	case BCM6338_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_6338_REG;
 		irq_mask_addr0 += PERF_IRQMASK_6338_REG;
+		irq_stat_addr1 = 0;
+		irq_mask_addr1 = 0;
 		irq_bits = 32;
 		ext_irq_count = 4;
 		ext_irq_cfg_reg1 = PERF_EXTIRQ_CFG_REG_6338;
@@ -178,6 +209,8 @@ static void bcm63xx_init_irq(void)
 	case BCM6345_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_6345_REG;
 		irq_mask_addr0 += PERF_IRQMASK_6345_REG;
+		irq_stat_addr1 = 0;
+		irq_mask_addr1 = 0;
 		irq_bits = 32;
 		ext_irq_count = 4;
 		ext_irq_cfg_reg1 = PERF_EXTIRQ_CFG_REG_6345;
@@ -185,6 +218,8 @@ static void bcm63xx_init_irq(void)
 	case BCM6348_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_6348_REG;
 		irq_mask_addr0 += PERF_IRQMASK_6348_REG;
+		irq_stat_addr1 = 0;
+		irq_mask_addr1 = 0;
 		irq_bits = 32;
 		ext_irq_count = 4;
 		ext_irq_cfg_reg1 = PERF_EXTIRQ_CFG_REG_6348;
@@ -192,6 +227,8 @@ static void bcm63xx_init_irq(void)
 	case BCM6358_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_6358_REG(0);
 		irq_mask_addr0 += PERF_IRQMASK_6358_REG(0);
+		irq_stat_addr1 += PERF_IRQSTAT_6358_REG(1);
+		irq_mask_addr1 += PERF_IRQMASK_6358_REG(1);
 		irq_bits = 32;
 		ext_irq_count = 4;
 		is_ext_irq_cascaded = 1;
@@ -202,6 +239,8 @@ static void bcm63xx_init_irq(void)
 	case BCM6362_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_6362_REG(0);
 		irq_mask_addr0 += PERF_IRQMASK_6362_REG(0);
+		irq_stat_addr1 += PERF_IRQSTAT_6362_REG(1);
+		irq_mask_addr1 += PERF_IRQMASK_6362_REG(1);
 		irq_bits = 64;
 		ext_irq_count = 4;
 		is_ext_irq_cascaded = 1;
@@ -212,6 +251,8 @@ static void bcm63xx_init_irq(void)
 	case BCM6368_CPU_ID:
 		irq_stat_addr0 += PERF_IRQSTAT_6368_REG(0);
 		irq_mask_addr0 += PERF_IRQMASK_6368_REG(0);
+		irq_stat_addr1 += PERF_IRQSTAT_6368_REG(1);
+		irq_mask_addr1 += PERF_IRQMASK_6368_REG(1);
 		irq_bits = 64;
 		ext_irq_count = 6;
 		is_ext_irq_cascaded = 1;
