#!/bin/sh
# Copyright (C) 2013 OpenWrt.org

[ -e /etc/config/network ] && exit 0

touch /etc/config/network

. /lib/functions/uci-defaults.sh
. /lib/mxs.sh

ucidef_set_interface_loopback

board=$(mxs_board_name)

case "$board" in
*)
	ucidef_set_interface_lan 'eth0'
	;;
esac

uci commit network

exit 0
