config interface loopback
	option ifname	lo
	option proto	static
	option ipaddr	127.0.0.1
	option netmask	255.0.0.0

config interface lan
	option ifname	eth0.1
	option type	bridge
	option proto	static
	option ipaddr	192.168.1.1
	option netmask	255.255.255.0
	option ip6assign 60

config interface wan
	option ifname	eth1
	option proto	dhcp

config interface wan6
	option ifname	@wan
	option proto	dhcpv6

config globals globals
	option ula_prefix auto

config switch
	option name	rtl8366s
	option reset	1
	option enable_vlan 1
	# Blinkrate: 0=43ms; 1=84ms; 2=120ms; 3=170ms; 4=340ms; 5=670ms
	option blinkrate	2

config switch_vlan
	option device	rtl8366s
	option vlan 	1
	option ports	"0 1 2 3 5t"

config switch_port
	# Port 1 controls the GREEN configuration of LEDs for
	# the switch and the section does not correspond to a real
	# switch port.
	#
	# 0=LED off; 1=Collision/FDX; 2=Link/activity; 3=1000 Mb/s;
	# 4=100 Mb/s; 5=10 Mb/s; 6=1000 Mb/s+activity; 7=100 Mb/s+activity;
	# 8=10 Mb/s+activity; 9=10/100 Mb/s+activity; 10: Fiber;
	# 11: Fault; 12: Link/activity(tx); 13: Link/activity(rx);
	# 14: Link (master); 15: separate register

	option device		rtl8366s
	option port		1
	option led		6

config switch_port
	# Port 2 controls the ORANGE configuration of LEDs for
	# the switch and the section does not correspond to a real
	# switch port.
	#
	# See the key above for switch port 1 for the meaning of the
	# 'led' setting below.
	
	option device		rtl8366s
	option port		2
	option led		9

config switch_port
	# Port 5 controls the configuration of the WAN LED and the
	# section does not correspond to a real switch port.
	#
	# To toggle the use of green or orange LEDs for the WAN port,
	# see the LED setting for wndr3700:green:wan in /etc/config/system.
	#
	# See the key above for switch port 1 for the meaning of the
	# 'led' setting below.

	option device		rtl8366s
	option port		5
	option led		2
