From ba9cb86c174603252ee5b5f2b277dab46a99cf02 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sat, 5 Oct 2013 14:53:48 +0200
Subject: [PATCH] ARM: sunxi: Register the A31 reset IP in init_time

The A31 has a reset IP that maintains a few other IPs in reset by
default. Among these IPs are the UARTs, and most notably the timers. We
thus need to register the reset driver before initializing the timers so
that the reset timer can use the reset framework.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/mach-sunxi/sunxi.c | 10 +++++++++-
 1 file changed, 9 insertions(+), 1 deletion(-)

diff --git a/arch/arm/mach-sunxi/sunxi.c b/arch/arm/mach-sunxi/sunxi.c
index f184f6c..2e79736 100644
--- a/arch/arm/mach-sunxi/sunxi.c
+++ b/arch/arm/mach-sunxi/sunxi.c
@@ -142,9 +142,17 @@ static void __init sunxi_dt_init(void)
 	NULL,
 };
 
+extern void __init sun6i_reset_init(void);
+static void __init sun6i_timer_init(void)
+{
+	sunxi_init_clocks();
+	sun6i_reset_init();
+	clocksource_of_init();
+}
+
 DT_MACHINE_START(SUN6I_DT, "Allwinner sun6i (A31) Family")
 	.init_machine	= sunxi_dt_init,
-	.init_time	= sunxi_timer_init,
+	.init_time	= sun6i_timer_init,
 	.dt_compat	= sun6i_board_dt_compat,
 	.restart	= sun6i_restart,
 MACHINE_END
-- 
1.8.4

