From 3473e6acea4bd01ba2b334628970390207f9f4fd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Emilio=20L=C3=B3pez?= <emilio@elopez.com.ar>
Date: Tue, 21 May 2013 21:25:05 -0300
Subject: [PATCH] clk: sunxi: mod0 support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This commit implements support for the "module 0" type of clocks, as
used by MMC, IR, NAND, SATA and other components.

Signed-off-by: Emilio López <emilio@elopez.com.ar>
---
 Documentation/devicetree/bindings/clock/sunxi.txt |  1 +
 drivers/clk/sunxi/clk-sunxi.c                     | 57 +++++++++++++++++++++++
 2 files changed, 58 insertions(+)

diff --git a/Documentation/devicetree/bindings/clock/sunxi.txt b/Documentation/devicetree/bindings/clock/sunxi.txt
index 773f3ae..ff3f61c 100644
--- a/Documentation/devicetree/bindings/clock/sunxi.txt
+++ b/Documentation/devicetree/bindings/clock/sunxi.txt
@@ -35,6 +35,7 @@ Required properties:
 	"allwinner,sun7i-a20-apb1-gates-clk" - for the APB1 gates on A20
 	"allwinner,sun6i-a31-apb2-div-clk" - for the APB2 gates on A31
 	"allwinner,sun6i-a31-apb2-gates-clk" - for the APB2 gates on A31
+	"allwinner,sun4i-mod0-clk" - for the module 0 family of clocks
 
 Required properties for all clocks:
 - reg : shall be the control register address for the clock.
diff --git a/drivers/clk/sunxi/clk-sunxi.c b/drivers/clk/sunxi/clk-sunxi.c
index 6947ba9..96c01b2 100644
--- a/drivers/clk/sunxi/clk-sunxi.c
+++ b/drivers/clk/sunxi/clk-sunxi.c
@@ -287,6 +287,47 @@ static void sun4i_get_apb1_factors(u32 *freq, u32 parent_rate,
 
 
 /**
+ * sun4i_get_mod0_factors() - calculates m, n factors for MOD0-style clocks
+ * MMC rate is calculated as follows
+ * rate = (parent_rate >> p) / (m + 1);
+ */
+
+static void sun4i_get_mod0_factors(u32 *freq, u32 parent_rate,
+				   u8 *n, u8 *k, u8 *m, u8 *p)
+{
+	u8 div, calcm, calcp;
+
+	/* These clocks can only divide, so we will never be able to achieve
+	 * frequencies higher than the parent frequency */
+	if (*freq > parent_rate)
+		*freq = parent_rate;
+
+	div = parent_rate / *freq;
+
+	if (div < 16)
+		calcp = 0;
+	else if (div / 2 < 16)
+		calcp = 1;
+	else if (div / 4 < 16)
+		calcp = 2;
+	else
+		calcp = 3;
+
+	calcm = DIV_ROUND_UP(div, 1 << calcp);
+
+	*freq = (parent_rate >> calcp) / calcm;
+
+	/* we were called to round the frequency, we can now return */
+	if (n == NULL)
+		return;
+
+	*m = calcm - 1;
+	*p = calcp;
+}
+
+
+
+/**
  * sunxi_factors_clk_setup() - Setup function for factor clocks
  */
 
@@ -333,6 +374,14 @@ struct factors_data {
 	.pwidth = 2,
 };
 
+/* user manual says "n" but it's really "p" */
+static struct clk_factors_config sun4i_mod0_config = {
+	.mshift = 0,
+	.mwidth = 4,
+	.pshift = 16,
+	.pwidth = 2,
+};
+
 static const struct factors_data sun4i_pll1_data __initconst = {
 	.enable = 31,
 	.table = &sun4i_pll1_config,
@@ -356,6 +405,13 @@ struct factors_data {
 	.getter = sun4i_get_apb1_factors,
 };
 
+static const struct factors_data sun4i_mod0_data __initconst = {
+	.enable = 31,
+	.mux = 24,
+	.table = &sun4i_mod0_config,
+	.getter = sun4i_get_mod0_factors,
+};
+
 static struct clk * __init sunxi_factors_clk_setup(struct device_node *node,
 						const struct factors_data *data)
 {
@@ -779,6 +835,7 @@ static void __init sunxi_divs_clk_setup(struct device_node *node,
 	{.compatible = "allwinner,sun4i-pll1-clk", .data = &sun4i_pll1_data,},
 	{.compatible = "allwinner,sun6i-a31-pll1-clk", .data = &sun6i_a31_pll1_data,},
 	{.compatible = "allwinner,sun4i-apb1-clk", .data = &sun4i_apb1_data,},
+	{.compatible = "allwinner,sun4i-mod0-clk", .data = &sun4i_mod0_data,},
 	{}
 };
 
-- 
1.8.4

