From e7243b7673a20ac28cfdc78c8862587ea8173a39 Mon Sep 17 00:00:00 2001
From: Markus Pargmann <mpa@pengutronix.de>
Date: Mon, 14 Oct 2013 12:49:21 +0000
Subject: ARM: dts: am33xx, change usb ctrl module label

Control module is not usb specific.
Changes the label to usb_ctrl_mod.

Signed-off-by: Markus Pargmann <mpa@pengutronix.de>
Signed-off-by: Benoit Cousson <bcousson@baylibre.com>
---
--- a/arch/arm/boot/dts/am33xx.dtsi
+++ b/arch/arm/boot/dts/am33xx.dtsi
@@ -406,7 +406,7 @@
 			ti,hwmods = "usb_otg_hs";
 			status = "disabled";
 
-			ctrl_mod: control@44e10000 {
+			usb_ctrl_mod: control@44e10000 {
 				compatible = "ti,am335x-usb-ctrl-module";
 				reg = <0x44e10620 0x10
 					0x44e10648 0x4>;
@@ -419,7 +419,7 @@
 				reg = <0x47401300 0x100>;
 				reg-names = "phy";
 				status = "disabled";
-				ti,ctrl_mod = <&ctrl_mod>;
+				ti,ctrl_mod = <&usb_ctrl_mod>;
 			};
 
 			usb0: usb@47401000 {
@@ -467,7 +467,7 @@
 				reg = <0x47401b00 0x100>;
 				reg-names = "phy";
 				status = "disabled";
-				ti,ctrl_mod = <&ctrl_mod>;
+				ti,ctrl_mod = <&usb_ctrl_mod>;
 			};
 
 			usb1: usb@47401800 {
