From b6b668f780d62d41bc14bc7baba1692e17cabf84 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Fri, 26 Apr 2013 11:21:16 +0200
Subject: [PATCH 10/14] MIPS: BCM63XX: add cpu argument to dispatch internal

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/irq.c |   21 +++++++++++----------
 1 file changed, 11 insertions(+), 10 deletions(-)

--- a/arch/mips/bcm63xx/irq.c
+++ b/arch/mips/bcm63xx/irq.c
@@ -19,8 +19,8 @@
 #include <bcm63xx_io.h>
 #include <bcm63xx_irq.h>
 
-static void __dispatch_internal_32(void) __maybe_unused;
-static void __dispatch_internal_64(void) __maybe_unused;
+static void __dispatch_internal_32(int cpu) __maybe_unused;
+static void __dispatch_internal_64(int cpu) __maybe_unused;
 static void __internal_irq_mask_32(unsigned int irq) __maybe_unused;
 static void __internal_irq_mask_64(unsigned int irq) __maybe_unused;
 static void __internal_irq_unmask_32(unsigned int irq) __maybe_unused;
@@ -158,7 +158,7 @@ static inline void bcm63xx_init_irq(void
 #else /* ! BCMCPU_RUNTIME_DETECT */
 
 static u32 irq_stat_addr0, irq_mask_addr0, irq_stat_addr1, irq_mask_addr1;
-static void (*dispatch_internal)(void);
+static void (*dispatch_internal)(int cpu);
 static int is_ext_irq_cascaded;
 static unsigned int ext_irq_count;
 static unsigned int ext_irq_start, ext_irq_end;
@@ -315,14 +315,15 @@ static inline void handle_internal(int i
  */
 
 #define BUILD_IPIC_INTERNAL(width)					\
-void __dispatch_internal_##width(void)					\
+void __dispatch_internal_##width(int cpu)				\
 {									\
 	u32 pending[width / 32];					\
 	unsigned int src, tgt;						\
 	bool irqs_pending = false;					\
-	static int i;							\
-	u32 irq_stat_addr = get_irq_stat_addr(0);			\
-	u32 irq_mask_addr = get_irq_mask_addr(0);			\
+	static int i[NR_CPUS];						\
+	u32 irq_stat_addr = get_irq_stat_addr(cpu);			\
+	u32 irq_mask_addr = get_irq_mask_addr(cpu);			\
+	int *next = &i[cpu];						\
 									\
 	/* read registers in reverse order */				\
 	for (src = 0, tgt = (width / 32); src < (width / 32); src++) {	\
@@ -340,9 +341,9 @@ void __dispatch_internal_##width(void)
 		return;							\
 									\
 	while (1) {							\
-		int to_call = i;					\
+		int to_call = *next;					\
 									\
-		i = (i + 1) & (width - 1);				\
+		*next = (*next + 1) & (width - 1);			\
 		if (pending[to_call / 32] & (1 << (to_call & 0x1f))) {	\
 			handle_internal(to_call);			\
 			break;						\
@@ -394,7 +395,7 @@ asmlinkage void plat_irq_dispatch(void)
 		if (cause & CAUSEF_IP1)
 			do_IRQ(1);
 		if (cause & CAUSEF_IP2)
-			dispatch_internal();
+			dispatch_internal(0);
 		if (!is_ext_irq_cascaded) {
 			if (cause & CAUSEF_IP3)
 				do_IRQ(IRQ_EXT_0);
