--- a/drivers/bcma/host_pci.c
+++ b/drivers/bcma/host_pci.c
@@ -188,8 +188,11 @@ static int bcma_host_pci_probe(struct pc
 		pci_write_config_dword(dev, 0x40, val & 0xffff00ff);
 
 	/* SSB needed additional powering up, do we have any AMBA PCI cards? */
-	if (!pci_is_pcie(dev))
-		bcma_err(bus, "PCI card detected, report problems.\n");
+	if (!pci_is_pcie(dev)) {
+		bcma_err(bus, "PCI card detected, they are not supported.\n");
+		err = -ENXIO;
+		goto err_pci_release_regions;
+	}
 
 	/* Map MMIO */
 	err = -ENOMEM;
@@ -269,6 +272,7 @@ static SIMPLE_DEV_PM_OPS(bcma_pm_ops, bc
 
 static DEFINE_PCI_DEVICE_TABLE(bcma_pci_bridge_tbl) = {
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x0576) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4313) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 43224) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4331) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4353) },
