From 2beb91164802b1cbfda369564d3371b3ff649eec Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Sun, 13 Oct 2013 16:05:49 +0200
Subject: [PATCH 6/6] MIPS: BCM47XX: fix detection of some boards

This adds some more boards

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
--- a/arch/mips/bcm47xx/board.c
+++ b/arch/mips/bcm47xx/board.c
@@ -56,6 +56,10 @@ struct bcm47xx_board_type_list1 bcm47xx_
 /* hardware_version */
 static const
 struct bcm47xx_board_type_list1 bcm47xx_board_list_hardware_version[] __initconst = {
+	{{BCM47XX_BOARD_ASUS_RTN10U, "Asus RT-N10U"}, "RTN10U"},
+	{{BCM47XX_BOARD_ASUS_RTN12, "Asus RT-N12"}, "RT-N12"},
+	{{BCM47XX_BOARD_ASUS_RTN12D1, "Asus RT-N12D1"}, "RTN12D1"},
+	{{BCM47XX_BOARD_ASUS_RTN12B1, "Asus RT-N12B1"}, "RTN12B1"},
 	{{BCM47XX_BOARD_ASUS_RTN16, "Asus RT-N16"}, "RT-N16-"},
 	{{BCM47XX_BOARD_ASUS_WL320GE, "Asus WL320GE"}, "WL320G-"},
 	{{BCM47XX_BOARD_ASUS_WL330GE, "Asus WL330GE"}, "WL330GE-"},
@@ -174,6 +178,8 @@ struct bcm47xx_board_type_list3 bcm47xx_
 	{{BCM47XX_BOARD_HUAWEI_E970, "Huawei E970"}, "0x048e", "0x5347", "0x11"},
 	{{BCM47XX_BOARD_PHICOMM_M1, "Phicomm M1"}, "0x0590", "80", "0x1104"},
 	{{BCM47XX_BOARD_ZTE_H218N, "ZTE H218N"}, "0x053d", "1234", "0x1305"},
+	{{BCM47XX_BOARD_NETGEAR_WNR3500L, "Netgear WNR3500L"}, "0x04CF", "3500", "02"},
+	{{BCM47XX_BOARD_LINKSYS_WRT54GSV1, "Linksys WRT54GS V1"}, "0x0101", "42", "0x10"},
 	{ {0}, 0},
 };
 
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
@@ -66,6 +66,7 @@ enum bcm47xx_board {
 	BCM47XX_BOARD_LINKSYS_WRT310NV1,
 	BCM47XX_BOARD_LINKSYS_WRT310NV2,
 	BCM47XX_BOARD_LINKSYS_WRT54G3GV2,
+	BCM47XX_BOARD_LINKSYS_WRT54GSV1,
 	BCM47XX_BOARD_LINKSYS_WRT610NV1,
 	BCM47XX_BOARD_LINKSYS_WRT610NV2,
 	BCM47XX_BOARD_LINKSYS_WRTSL54GS,
