From 0bebda684857f76548ea48c8886785198701d8d3 Mon Sep 17 00:00:00 2001
From: Markus Pargmann <mpa@pengutronix.de>
Date: Thu, 17 Oct 2013 07:18:38 +0000
Subject: ARM: OMAP2+: irq, AM33XX add missing register check

am33xx has a INTC_PENDING_IRQ3 register that is not checked for pending
interrupts. This patch adds AM33XX to the ifdef of SOCs that have to
check this register.

Cc: stable@vger.kernel.org
Signed-off-by: Markus Pargmann <mpa@pengutronix.de>
Signed-off-by: Tony Lindgren <tony@atomide.com>
---
--- a/arch/arm/mach-omap2/irq.c
+++ b/arch/arm/mach-omap2/irq.c
@@ -233,7 +233,7 @@ static inline void omap_intc_handle_irq(
 			goto out;
 
 		irqnr = readl_relaxed(base_addr + 0xd8);
-#ifdef CONFIG_SOC_TI81XX
+#if IS_ENABLED(CONFIG_SOC_TI81XX) || IS_ENABLED(CONFIG_SOC_AM33XX)
 		if (irqnr)
 			goto out;
 		irqnr = readl_relaxed(base_addr + 0xf8);
