AES interrupts were previously not used, but after recent changes to omap-aes
driver, its being used. We correct the interrupt number to have working PIO
mode.

Signed-off-by: Joel Fernandes <joelf@ti.com>

---
arch/arm/boot/dts/am33xx.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/am33xx.dtsi
+++ b/arch/arm/boot/dts/am33xx.dtsi
@@ -721,7 +721,7 @@
 			compatible = "ti,omap4-aes";
 			ti,hwmods = "aes";
 			reg = <0x53500000 0xa0>;
-			interrupts = <102>;
+			interrupts = <103>;
 			dmas = <&edma 6>,
 			       <&edma 5>;
 			dma-names = "tx", "rx";
